ERRATIC TEMP. READING OR E.C.C CONTROLS ARE TOO HOT/COLD. Buick Reatta 1991

For 1990-2009 cars

# ERRATIC TEMP. READING OR E.C.C CONTROLS ARE TOO HOT/COLD

SOME 1991 ELDORADOS BUILT BEFORE VIN BREAKPOINT 602439, SEVILLES BUILT BEFORE VIN BREAKPOINT 802449, AND RIVIERAS BUILT BEFORE VIN BREAKPOINT 402341 MAY EXPERIENCE ONE OR MORE OF THE FOLLOWING CONDITIONS:

O INTERMITTENT CODE B110 O ERRATIC OUTSIDE TEMPERATURE SENSOR READINGS O ELECTRONIC CLIMATE CONTROL TOO WARM OR TOO COLD AT TIMES

THESE CONDITIONS MAY BE CAUSED BY A BAD CONNECTION AT THE OUTSIDE AIR TEMPERATURE (OAT) SENSOR UNDER HOOD. SOME VEHICLES WERE BUILT WITH MALE TERMINALS ON BOTH SIDES OF THE OAT SENSOR (MALE TERMINALS ON THE SENSOR AND MALE TERMINALS ON THE HARNESS). TO REPAIR THIS CONDITION REPLACE THE TWO MALE TERMINALS ON THE HARNESS WITH FEMALE TERMINALS, P/N 12010182 (INCLUDED IN THE TERMINAL REPAIR KIT J-38125).

FOR WARRANTY PURPOSES USE LABOR OPERATION N6280 AT .5 HOUR.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1990 CADILLAC MOTOR CAR DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.