CONVERTIBLE TOP, DIFFICULT TO LATCH IN THE REAR. Buick Reatta 1990

For 1990-2009 cars

# CONVERTIBLE TOP, DIFFICULT TO LATCH IN THE REAR

#### SUBJECT: CONVERTIBLE TOP DIFFICULT TO LATCH IN REAR (PULL BACK HEADLINER IN SAIL PANEL)

#### VEHICLES AFFECTED: 1990 REATTA 'E'

Some 1990 Reatta convertibles may experience a condition of the convertible top being difficult to latch in the rear. To repair this condition use the following service procedure:

1. Pull back headliner in sail panel area of top to expose the #4 bow adjustment screws. Refer to Figure 1.

2. Loosen the four adjustment screws and lower #4 bow to bottom of slots to relieve excessive top tension.

#### NOTE: Slots may be elongated as much as twice their original length to provide additional adjustment.

3. Adjust #4 bow upward until top wrinkles and sags are minimized.

4. Tighten the four adjustment screws.

5. Re-centre #5 bow latch pins using J-38842 centering tool. Place tool in tonneau bezel, loosen #5 bow pin locking nuts, and lower #5 bow until pins engage tool. Tighten pin locking nuts.

Use the most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.