For 1990-2009 cars

## Console Rear Trim Plate Replacement Buick

### Removal Procedure

1. Remove the console assembly. Refer to Console Replacement .
2. Place the console on a clean protected surface.
3. Remove the rear air outlet deflector. Refer to Air Outlet Replacement .
4. Remove the fasteners (1) from the console accessory housing.
5. Pull rearward in order to remove the housing (1).

### Installation Procedure

1. Align the console accessory housing (1) to the console assembly.
2. Install the lower console accessory housing fasteners (1).
3. Install the rear air outlet deflector. Refer to Air Outlet Replacement .
4. Install the console assembly. Refer to Console Replacement .

## Console Rear Trim Plate Replacement Oldsmobile

### Removal Procedure

1. Remove the storage bin. Refer to Front Floor Console Compartment Replacement .
2. Disconnect the console air control linkage (1, 2).
3. Remove the rear plate housing fasteners (1).
4. Remove the rear plate housing from the console.

### Installation Procedure

1. Align the rear plate housing to the console.
2. Install the fasteners (1) to the rear plate housing.
3. Connect the console air control linkage (1, 2).
4. Install the storage bin. Refer to Front Floor Console Compartment Replacement .