For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Move the left front door lock/window switch to the LOCK position.
2. Move the left front door lock/window switch to the UNLOCK position.
3. Move the right front door lock/window switch to the LOCK position.
4. Move the right front door lock/window switch to the UNLOCK position.

• | All of the doors lock and stay locked when a lock switch is pressed.

• | All of the doors unlock and stay unlocked when an unlock switch is pressed.

• | Power Door Locks Inoperative

• | Power Door Locks Inoperative - One Motor

• | Power Door Locks Inoperative - One Motor

• | Power Door Locks Inoperative, RKE Operates

• | Power Door Locks - Lock Inoperative Unlock Operates

• | Power Door Locks - Unlock Inoperative Lock Operates

• | Power Door Locks Switch Lock Function Inoperative - One

• | Power Door Locks Switch Lock Function Inoperative - One

• | Power Door Locks Switch Unlock Function Inoperative - One

• | Power Door Locks Switch Unlock Function Inoperative - One

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.