For 1990-2009 cars

### Removal Procedure

Caution: When you are carrying an undeployed inflator module:

• | Do not carry the inflator module by the wires or connector on the inflator module

• | Make sure the bag opening points away from you

When you are storing an undeployed inflator module, make sure the bag opening points away from the surface on which the inflator module rests. When you are storing a steering column, do not rest the column with the bag opening facing down and the column vertical. Provide free space for the air bag to expand in case of an accidental deployment. Otherwise, personal injury may result.

1. Turn the ignition switch to OFF position.
2. Remove the Instrument Panel (IP) Cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Guages and Console.
3. Remove the lamp.

### Installation Procedure

1. Install new lamp.
2. Install the Instrument Panel (IP) Cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Guages and Console.