For 1990-2009 cars

### Removal Procedure

1. Remove the injector sight shield if necessary. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical.

Important: Remember the cable routing for the replacement procedure.

2. Disconnect the cruise control cable (1) from the following components:

• | The TBI cam

• | The throttle body bracket

3. Remove the cruise control cable (2) from the cruise control module (1).

### Installation Procedure

1. Install the cruise control cable (2) to the cruise control module (1).
2. Connect the cruise control cable (1) to the following components:

• | The TBI cam

• | The throttle body bracket

3. Adjust the cable. Refer to Cruise Control Cable Adjustment .
4. Install the injector sight shield if necessary. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical.