For 1990-2009 cars

1. Install the spring guide (1) into the tilt spring (2). Lubricate the assembly with synthetic grease.

Caution
The tilt spring and the spring guide are under pressure and could become a projectile. During the disassembly and assembly procedures, secure the tilt spring. Exercise caution when removing or installing the tilt spring and the spring guide, as bodily injury may result.

Install the tilt spring (1).

2.1. | Install the tilt spring (1) to the post on the steering column support assembly (2).

2.2. | Secure the tilt spring (1).

2. Install the upper cover and the lower cover. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .