For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC. 6 NEW BEARING CLEARANCE

#### SUBJECT: SMU/SEC 6 ENGINE MECHANICAL-CRANKSHAFT MAIN BEARING, CONNECTING ROD (NEW BEARING CLEARANCE)

#### VEHICLES AFFECTED: 1985-1991 ALL CARS W/3.0, 3300, 3.8, 3800

The following revised bearing clearances should be used when servicing main bearings and connecting rod bearings on the engines listed above. Note that the clearances are the same for main and rod bearings.

#### CRANKSHAFT MAIN BEARINGS

Bearing to Journal Clearance 0.020 - 0.055 mm. (.0008 - .0022 in.)

#### CONNECTING ROD BEARINGS

Bearing to Journal Clearance 0.020 - 0.055 mm. (.0008 - .0022 in.)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.