For 1990-2009 cars

### Removal Procedure

1. Remove the case side cover. Refer to Control Valve Body Cover Replacement .
2. Disconnect the transaxle wirng harness.
3. Remove the torque converter clutch solenoid (315).

### Installation Procedure

1. Install the torque converter clutch solenoid (315).
2. Connect the transaxle wirng harness.
3. Install the case side cover. Refer to Control Valve Body Cover Replacement .