For 1990-2009 cars

### Removal Procedure

1. Remove the right sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.
2. Remove the HVAC programmer bracket. Refer to Programmer Replacement in HVAC System-Automatic.
3. Disconnect the electrical connector.
4. Remove the PASS-Key ® II theft deterrent module (2) from the bracket (1).

### Installation Procedure

1. Slide the Pass-Key ® II theft deterrent module (2) onto the bracket (1).
2. Connect the electrical connector.
3. Install the HVAC programmer bracket. Refer to Programmer Replacement in HVAC System-Automatic.
4. Install the right sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.