For 1990-2009 cars

### Removal Procedure

1. Remove the air inlet ducts.
2. Drain the coolant from the recovery reservoir. Refer to Cooling System Draining and Filling .
3. Disconnect the reservoir to radiator hose and clamps.
4. Remove the fasteners retaining the reservoir.
5. Remove the reservoir.

### Installation Procedure

1. Install the recovery reservoir in the vehicle.
2. Install the fasteners.
3. Connect the hoses and the clamps.
4. Refill the reservoir with coolant. Refer to Cooling System Draining and Filling
5. Install the air inlet duct.