For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Disconnect the electrical connector.
3. Remove the 2 push-in retainers (1) that secure the RFA module (3) to the bottom of the package shelf.
4. Remove the RFA module.

### Installation Procedure

1. Align the RFA module to the rear shelf.
2. Install the retainers for the RFA module (3) onto the package shelf.
3. Connect the electrical connector.
4. Close the rear compartment lid.
5. Program the transmitters. Refer to Transmitter Programming .
6. Program options for RFA module. Refer to Remote Control Door Lock Reprogramming .