For 1990-2009 cars

## Front Fender Insulator Replacement Oldsmobile

### Removal Procedure

1. Remove the wheelhouse assembly. Refer to Wheelhouse Panel Replacement .
2. Remove the push-in retainer (2) from the sound insulator (3).
3. Remove the fender sound insulator (3).

### Installation Procedure

1. Install the fender sound insulator (3).
2. Install the push-in retainer (2).
3. Install the wheelhouse assembly. Refer to Wheelhouse Panel Replacement .

## Front Fender Insulator Replacement Buick

### Removal Procedure

1. Remove the wheelhouse assembly. Refer to Wheelhouse Panel Replacement .
2. Remove the push-in retainer (2) from the sound insulator (3).
3. Remove the fender sound insulator (3).

### Installation Procedure

1. Install the fender sound insulator (3).
2. Install the push-in retainer (2).
3. Install the wheelhouse assembly. Refer to Wheelhouse Panel Replacement .