For 1990-2009 cars

## Drive Belt Idler Pulley Replacement VIN 1

### Removal Procedure

• | J 28467-360 Engine Support Fixture

• | J 28467-94B Engine Support Fixture Adapter

• | J 28467-330 Engine Support Fixture Adapter

• | J 28467-350 Engine Support Fixture Adapter

1. Raise the vehicle. Suitably support the vehicle. Refer to Section 0A.
2. Remove the front lower splash shield.
3. Drain the coolant. Refer to Draining and Filling the Coolant System in Engine Cooling.
4. Close the radiator drain cock. Install the front splash shield.
5. Lower the vehicle.
6. Install the J 28467-360 to the engine.
7. Remove the supercharger belt. Refer to Drive Belt Replacement .
8. Remove the ignition module.
9. Remove the supercharger belt tensioner. Refer to Drive Belt Tensioner Replacement .
10. Remove the accessory drive belt. Refer to Drive Belt Replacement .
11. Remove the torque axis engine mount. Refer to Engine Mount Replacement .
12. Remove the power steering pump. Set the pump aside. Refer to Section 3B.
13. Remove the engine mount bracket. Refer to Engine Mount Bracket Replacement .
14. Remove the idler pulley/bracket bolts.
15. Remove the idler pulley/bracket.

### Installation Procedure

1. Install the idler pulley/bracket.
2. Install the idler pulley/bracket bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the engine mount bracket. Refer to Engine Mount Bracket Replacement .
4. Install the power steering pump. Refer to Section 3B.
5. Install the torque axis engine mount. Refer to Engine Mount Replacement .
6. Install the accessory drive belt. Refer to Drive Belt Replacement .
7. Install the supercharger belt tensioner. Refer to Drive Belt Tensioner Replacement .
8. Install the ignition module.
9. Install the supercharger belt. Refer to Drive Belt Replacement .
10. Remove the engine support fixture.
11. Refill the coolant. Refer to Draining and Filling the Coolant System in Engine Cooling.