For 1990-2009 cars

# FLYWHEEL-CONVERTER BOLTS REVISED TORQ SPECIFICATIONS

#### Models Affected: All 1984 and Later With Automatic Transmissions

Flywheel to torque converter bolt torque has been changed from 40-54 Nm 35-40 lb/ft to 55-70 Nm 41-52 lb/ft. Also re-torque the first bolt after all three (3) have been torqued.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.