For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Disconnect the wiper motor connector C1.
2. Set the ignition switch to RUN.
3. Set the wiper switch to LO.
4. Connect a test light from connector C1, terminal F to ground.
5. Momentarily activate the washer switch while observing the test light.

Is the test light on when the washer switch is released?

--

Go to Step 3

Go to Step 4

3 | Replace the wiper/washer switch. Refer to Multifunction Turn Signal Lever Replacement - On Vehicle . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
4 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --