For 1990-2009 cars

# 4T40E , 4T45E , 4T65E Surge Slip Condition Under Load in 2nd, 3rd , and or 4th - kw 3.1 automatic body chuggle fourth hesitation hot LG8 miss second shift third valve

Subject: | 4T40E, 4T45E, 4T65E Surge Slip Condition Under Load in 2nd 3rd and or 4th

Models: | .

When servicing the vehicle with the VIN you entered, the following diagnosis might be helpful if the vehicle exhibits the described symptoms.

### Condition/Concern:

The 4T40E/4T45E/4T65E automatic transmission may experience a slip surge condition in second, third and or fourth gears while under load, such as driving up a long hill or mountain. The conditions either separate or working in combination seem to cause the 'Engine Load %' to drop to a value which the PCM commands a lower line pressure (increase in PCS amperage).

'Normal' degradation of MAF over time aggravated by induction of foreign material (fine dust, oil from non-OEM air induction systems; secondly, build up of carbon deposits in combustion chamber/intake valves over time; thirdly, outside ambient temperatures above 95 degrees F(35 degrees C) seem to aggravate the condition.

### Recommendation/Instructions:

1. The MAF should be swapped from a known good unit or replaced and the vehicle evaluated
2. Clean the top half of engine to remove carbon deposits. Use GM PN 12378546, 3 Step Induction Cleaner Kit, available through GMSPO.The 3 Step Induction Cleaner Kit should be used with tool E-957-001-C available from Auto Tech Industries at 1-800-522-8882 who is the approved supplier of the installation tool. The E-957-001-C kit costs about $595 but has all the adapters to work on TBI and multiport systems and EGR cleaning.

.

Please follow this diagnosis process thoroughly and complete each step. If the condition exhibited is resolved without completing every step, the remaining steps do not need to be performed. If these steps do not resolve the condition, please contact GM TAC for further diagnostic assistance. This diagnostic approach was developed for the vehicle with the VIN you entered and should not be automatically be used for other vehicles with similar symptoms.

### Models:

(99 - 03 General Motors Passenger Cars)

.