For 1990-2009 cars

Use the following procedure in order to prepare the top strut mounting holes:

1. Remove the top struts from the washers.
2. Lift the front of the vehicle by the body in order to separate the strut from the inner wheel house.
3. Drill two 13/32 inch holes at the front and the rear of the oval strut mounting hole on the left and right strut towers.
4. File the excess metal in order to make slotted holes.
5. Paint the exposed metal using rust preventative paint or primer.
6. Lower the front of the vehicle.
7. Install the strut attaching nuts.

Do not tighten the nuts at this time.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

8. Move the top of the strut forward or rearward in order to adjust the caster. A 1 mm (0.040 in) position change at the tower is about equal to a 0.1 degree change in the caster. Refer to Wheel Alignment Specifications .

Tighten
Tighten the strut attaching nuts to 47 N·m (35 lb ft).