For 1990-2009 cars

## Door Body Side Molding Replacement Oldsmobile

### Removal Procedure

1. Using a flat bladed tool, gently pry the front door moldings (1) in order to release the clips (4).
2. Using a flat bladed tool, gently pry the rear door moldings (1) in order to release the clips (3).
3. Remove the door molding(s) (1).

### Installation Procedure

1. Install the rear door molding(s) (1) over the locating pin (2).
2. Install the front door molding(s) (1) over the locating pin (2).
3. Press the molding(s) (1) in order to engage the clips (4).

## Door Body Side Molding Replacement Buick

### Removal Procedure

1. Using a flat bladed tool, gently pry the door molding (1) in order to release the clips (3).
2. Remove the door molding (1).

### Installation Procedure

1. Install the door molding (1) over the locating clip (3).
2. Press the molding (1) in order to engage the clips (2).