For 1990-2009 cars

#### Tools Required

J 39601 Camber Adjustment Tool

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.

Important: Do not allow bolts to turn this will ruin the serratted shoulder.

3. Tap the upper and lower bolt and nut from the strut and knuckle.
4. Seperate the strut from the knuckle.

Important: It is necessary to grind the lower bolt hole on the strut to achieve proper camber setting.

If camber specification is not achieved by this procedure check for bent or worn parts.
5. Using a round file or a die grinder file the inner metal plate to the outside plates diameter.
6. File excess metal to make the slotted holes.
7. Paint the exposed metal with rust preventive paint or primer.
8. Replace the strut to the knuckle.
9. Install both the upper and lower bolts.
10. Do not tighten at this time. (leave loose).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

11. Using the J 39601 , set the camber. Refer to Wheel Alignment Specifications .

Tighten
Tighten the upper strut to knuckle nut to 225 N·m (166 lb ft).

12. Remove the J 39601 .
13. Tighten the lower strut to knuckle nut to 225 N·m (166 lb ft).
14. Replace the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tire and Wheels.
15. Lower the vehicle.
16. Perform a wheel alignment. Refer to Wheel Alignment Specifications in Wheel Alignment.