For 1990-2009 cars

# RIVIERA BODYSIDE MOLDING THICKNESS INCREASED-NEW PARTS

#### VEHICLES AFFECTED: 1989 E CARS

The body side mouldings used on E cars were originally manufactured in stainless steel in a thickness of .46-.50 mm. To improve the ability to resist denting, a new moulding is being released for service. The new moulding has a gauge thickness of .54-.60 mm. Part numbers for these mouldings are listed below:

Front Fender Right/Left 20729258/-9 Door Right/Left 12500994/-3 Rear Quarter Right/Left 12394244/-5

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.