For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the negative battery cable.
3. Remove the Rear seat lower portion. Refer to Body Seats And Carpet.
4. Remove the fuel pump relay from the fuel pump relay electrical connector.

### Installation Procedure

1. Installation the fuel pump relay.
2. Installation the rear seat lower portion. Refer to General Body Service
3. Turn the ignition OFF.
4. Installation the negative battery cable.