For 1990-2009 cars

#### Tools Required

• | J 22124-B Pressure Gage

• | J 22124-91 Pressure Gage Adapter

1. Attach the J 22124-91 to the air dryer.
2. Attach the J 22124-B to the J 22124-91 with the toggle valve (5) on the opposite side of the air compressor. Close the toggle valve.
3. Apply air pressure at the schrader valve (4). Pressurize until the J 22124-B reads 690 kPa (100 psi).
4. Check the following areas using soap bubbles:

• | Solenoid valve (1) -- Replace the air compressor head if leaking.

• | Air dryer to compressor head o-ring (2) -- Replace the air dryer if leaking.

• | Air dryer cover (3) -- Replace the air dryer if leaking.

• | Air compressor head gasket (6) -- Replace the air compressor head if leaking.

• | Air compressor head cover gasket (7) -- Tighten the cover bolts to 5.6 N·m (50 lb in) if the head cover gasket is leaking. If the leak persists, replace the air compressor head.