For 1990-2009 cars

# HARD START/POOR PERFORMANCE INTERMITTENT ELEC. FUEL PUMP

#### MODELS AFFECTED: All EFI Engines

Intermittent operation of an electric fuel pump may be due to an improperly crimped wire terminal connection at the fuel pump. An improper crimp at the terminal may have damaged the wire, causing an intermittent connection.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.