For 1990-2009 cars

# INFO ON AN INTERMITTENT NO START

THIS IS A MONTHLY SERVICE NEWSLETTER ARTICLE. THIS BULLETIN IS NOT INTENDED FOR PUBLICATION.

#### SUBJECT: INFORMATION ON AN INTERMITTENT NO START

#### MODELS: 1995-98 RIVIERA

THE ENGINE INTERMITTENTLY WILL NOT START. CHECK THE POWER FEED CABLE FROM THE BATTERY TO THE FUSE/RELAY CENTER UNDER THE REAR SEAT FOR OVERTORQUED OR LOOSE CONDITION.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.