For 1990-2009 cars

1. Remove the fuel injector sight shield, if equipped with engine option code L67. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical-3.8L.
2. Disengage the adjustment lock (1) on the cruise control cable. The lock is located at the TBI end of the cable.

When the lock is disengaged, the cable moves freely in and out of the adjuster.

3. Hold the TBI at the closed position.
4. Pull the cable conduit in order to reduce the slack in the cable.
5. Engage the adjustment lock.
6. Install the fuel injector sight shield, if equipped with engine option code L67. Refer to Fuel Injector Sight Shield Replacement in Engine Mechanical-3.8L.