For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Interior Lamps System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 |

1. Disconnect the rear compartment lid latch switch connector.
2. Connect a fused jumper between the switch connector terminal A (ORN/BLK) of the rear compartment lid latch and ground.
3. Turn the ignition switch to the ON position.

Does the rear compartment lamp light?

--

Go to Step 3

Go to Step 4

3 | Test CKT 1050 (BLK) for an open. Refer to Testing for Continuity in Wiring Systems. Is CKT 1050 OK? | -- | Go to Step 6 | Go to Step 8
4 | Test CKT 1732 (ORN) for an open or a short to ground between S336 and the rear compartment lamp. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 1732 OK? | -- | Go to Step 5 | Go to Step 8
5 | Test CKT 737 (ORN/BLK) for an open. Refer to Testing for Continuity in Wiring Systems. Is CKT 737 OK? | -- | Go to Step 7 | Go to Step 8
6 | Replace the rear compartment lid latch switch. Is the repair complete? | -- | Go to Interior Lamps System Check | --
7 | Replace the rear compartment lamp. Refer to Rear Compartment Courtesy Lamp Replacement . Is the repair complete? | -- | Go to Interior Lamps System Check | --
8 | Repair the suspect wiring. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check | --