For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint to Knuckle | 10 N·m plus 150 degrees | 7 lb ft plus 15 degrees
Brake Bracket to Strut | 17 N·m | 13 lb ft
Brake Caliper to Knuckle | 51 N·m | 38 lb ft
Control Arm Front Nut | 126 N·m | 93 lb ft
Control Arm Rear Bolt | 158 N·m | 117 lb ft
Drive Axle Nut | 145 N·m | 107 lb ft
Front Wheel Speed Sensor Bracket to Strut | 17 N·m | 13 lb ft
Hub and Bearing to Knuckle | 95 N·m | 70 lb ft
Service Ball Joint to Knuckle | 68 N·m | 50 lb ft
Stabilizer Shaft Bracket Bolt | 40 N·m | 30 lb ft
Stabilizer Shaft Link Nut | 17 N·m | 13 lb ft
Strut Mount Nut | 75 N·m | 55 lb ft
Strut Mount to Body Nuts | 47 N·m | 35 lb ft
Strut to Knuckle Nuts | 185 N·m | 136 lb ft
Tie Rod to Knuuckle (Do not exced 70 N·m (52 lb in) to align cotter pin.) | 47 N·m | 35 lb ft