For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to the OFF position.
2. Place the headlamp switch in the OFF position.

All of the exterior lamps are off.

Park Lamps Always On

2 | Place the headlamp switch in the PARK position. | All of the following lamps turn on:

• | The park lamps

• | The side marker lamps

• | The tail lamps

• | The license lamps

• | Park Lamps Inoperative

• | Park Lamps Inoperative

3 |

1. Place the headlamp switch in the OFF position.
2. Place the hazard switch in the ON position.

The turn lamps flash approximately 80-90 times per minute.

Hazard Lamps Inoperative

4 |

1. Place the hazard switch in the OFF position.
2. Press the brake pedal.

All of the stop lamps are on with the pedal pressed.

Stop Lamps Inoperative

5 |

1. Turn the ignition switch to the RUN position.
2. Place the multi-function lever (turn/hazard switch assembly) in the left turn position.

• | The left turn lamps flash approximately 80-90 times per minute.

• | The left cornering lamp lights.

• | Turn Signal Lamps Inoperative

• | Cornering Lamps Inoperative

• | Cornering Lamp Inoperative - Left Side

6 | Place the multi-function lever (turn/hazard switch assembly) in the right turn position. |

• | The right turn lamps flash approximately 80-90 times per minute.

• | The right cornering lamp lights.

• | Turn Signal Lamps Inoperative

• | Cornering Lamps Inoperative

• | Cornering Lamp Inoperative - Right Side

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.