For 1990-2009 cars

Table 1: | C100 (Buick)
Table 2: | C100 (Oldsmobile)
Table 3: | C101 (Buick)
Table 4: | C101 (Oldsmobile)
Table 5: | C102 (Buick)
Table 6: | C102 (Oldsmobile)
Table 7: | C103
Table 8: | C104
Table 9: | C105
Table 10: | C107
Table 11: | C114
Table 12: | C127 (Oldsmobile)
Table 13: | C200 (Buick)
Table 14: | C200 (Oldsmobile)
Table 15: | C202 (Buick)
Table 16: | C202 (Oldsmobile)
Table 17: | C203 (Buick)
Table 18: | C203 (Oldsmobile)
Table 19: | C205
Table 20: | C206
Table 21: | C207
Table 22: | C208
Table 23: | C209 (Buick)
Table 24: | C209 (Oldsmobile)
Table 25: | C212
Table 26: | C215
Table 27: | C219 (Buick)
Table 28: | C219 (Oldsmobile)
Table 29: | C301 (Buick w/ A43)
Table 30: | C301 (Oldsmobile)
Table 31: | C303 (Buick)
Table 32: | C303 (Oldsmobile)
Table 33: | C305
Table 34: | C307
Table 35: | C308
Table 36: | C400
Table 37: | C401
Table 38: | C404 (Buick)
Table 39: | C405
Table 40: | C406
Table 41: | C407
Table 42: | C420
Table 43: | C501 (Buick)
Table 44: | C501 (Oldsmobile)
Table 45: | C505 (Buick)
Table 46: | C600
Table 47: | C601
Table 48: | C605 (Buick)

#### C100 (Buick)

Connector Part Information |

• | 12160280

• | 20 Way F Micro-Pack 100W Series (GRY)

Connector Part Information

• | 12176566

• | 20 Way M Micro-Pack 100W Series, Lock Assist/Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control | A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control
B | YEL/BLK | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control | B | YEL | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control
C | RED/BLK | 1228 | Pressure Control Solenoid (PC SOL) Valve - High | C | PPL | 1228 | Pressure Control Solenoid (PC SOL) Valve - High
D | LT BLU/WHT | 1229 | Pressure Control Solenoid (PC SOL) Valve - Low | D | LT BLU | 1229 | Pressure Control Solenoid (PC SOL) Valve - Low
E | PNK | 639 | Fused Ignition 1 Feed | E | RED | 839 | Fused Ignition 1 Feed
F-K | - | - | Not Used | F-K | - | - | Not Used
L | YEL/BLK | 1227 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal | L | BRN | 1227 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal
M | BLK | 808 | Sensor Ground | M | GRY | 452 | Sensor Ground
N | PNK | 1224 | Trans Fluid Pressure Switch A Input | N | PNK | 1224 | Trans Fluid Pressure Switch A Input
P | RED | 1226 | Trans Fluid Pressure Switch C Input | P | ORN | 1226 | Trans Fluid Pressure Switch C Input
R | DK BLU | 1225 | Trans Fluid Pressure Switch B Input | R | DK BLU | 1225 | Trans Fluid Pressure Switch B Input
S | RED/BLK | 1230 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - High | S | BLK | 1230 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - High
T | BRN | 418 | Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve Control | T | BRN | 418 | Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM SOL) Valve Control
U | YEL | 657 | TCC Release Switch Input | U | WHT | 1804 | TCC Release Switch Input
V | DK BLU/WHT | 1231 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - Low | V | DK GRN | 1231 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - Low
W | - | - | Not Used | W | - | - | Not Used

#### C100 (Oldsmobile)

Connector Part Information |

• | 12160280

• | 20 Way F Micro-Pack 100W Series (GRY)

Connector Part Information

• | 12160542

• | 20 Way M Micro-Pack 100W Series, Lock Assist/Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control | A | LT GRN | 1222 | 1-2 Shift Solenoid (1-2 SS) Valve Control
B | YEL/BLK | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control | B | YEL | 1223 | 2-3 Shift Solenoid (2-3 SS) Valve Control
C | RED/BLK | 1228 | Pressure Control Solenoid (PC SOL) Valve - High | C | PPL | 1228 | Pressure Control Solenoid (PC SOL) Valve - High
D | LT BLU/WHT | 1229 | Pressure Control Solenoid (PC SOL) Valve - Low | D | LT BLU | 1229 | Pressure Control Solenoid (PC SOL) Valve - Low
E | PNK | 339 | Fused Ignition 1 Feed | E | RED | 839 | Fused Ignition 1 Feed
F-K | - | - | Not Used | F-K | - | - | Not Used
L | BLK | 452 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal - Low | L | BRN | 1227 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal - Low
M | TAN/WHT | 585 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal - High | M | GRY | 452 | Automatic Transaxle Fluid Temperature (TFT) Sensor Signal - High
N | PNK | 1224 | Trans Fluid Pressure Switch A Input | N | PNK | 1224 | Trans Fluid Pressure Switch A Input
P | RED | 1226 | Trans Fluid Pressure Switch C Input | P | ORN | 1226 | Trans Fluid Pressure Switch C Input
R | DK BLU | 1225 | Trans Fluid Pressure Switch B Input | R | DK BLU | 1225 | Trans Fluid Pressure Switch B Input
S | RED/BLK | 1230 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - High | S | BLK | 1230 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - High
T | TAN/BLK | 422 | Torque Converter Pulse Width Modulation Solenoid (TCC PWM SOL) Valve Control | T | TAN | 418 | Torque Converter Pulse Width Modulation Solenoid (TCC PWM SOL) Valve Control
U | PNK | 339 | Fused Ignition 1 Feed | U | WHT | 1135 | Fused Ignition 1 Feed
V | DK BLU/WHT | 1231 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - Low | V | DK GRN | 1231 | Automatic Transaxle Input Shaft Speed (A/T ISS) Sensor - Low
W | - | - | Not Used | W | - | - | Not Used

#### C101 (Buick)

Connector Part Information |

• | 12129207

• | 78 Way F Metri-Pack MXD (BLK)

Connector Part Information

• | 12176888

• | 78 Way M Metri-Pack MXD (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | BLK | 451 | PCM Ground | A1 | BLK/WHT | 451 | PCM Ground
A2-A5 | -- | -- | Not Used | A2-A5 | -- | -- | Not Used
A6 | YEL | 492 | MAF Signal | A6 | YEL | 492 | MAF Signal
A7 | BLK | 630 | Camshaft Signal | A7 | BLK | 630 | Camshaft Signal
B1-B7 | -- | -- | Not Used | B1-B7 | -- | -- | Not Used
C1 | BLK | 1350 | Ground | C1 | BLK | 1350 | Ground
C2 | PNK | 439 | Fused Output (IGN) | C2 | PNK | 439 | Fused Output (IGN)
C3 | PNK | 439 | Fused Output (IGN) | C3 | PNK | 439 | Fused Output (IGN)
C4 | BLK/WHT | 651 | Sensor Return | C4 | BLK/WHT | 651 | Sensor Return
C5 | PNK | 639 | Fused Output (IGN) | C5 | PNK | 639 | Fused Output (IGN)
C6 | ORN | 540 | Fused Output (IGN) | C6 | ORN | 540 | Fused Output (IGN)
C7 | GRY | 605 | 5 Volt Reference | C7 | GRY | 605 | 5 Volt Reference
D1 | LT GRN | 432 | MAP Sensor Signal | D1 | LT GRN | 432 | MAP Sensor Signal
D2 | LT BLU/BLK | 647 | Crankshaft Position Output | D2 | LT BLU/BLK | 647 | Crankshaft Position Output
D3 | BLK | 552 | Sensor Return | D3 | BLK | 552 | Sensor Return
D4 | BLK | 1744 | Fuel Injector #1 | D4 | BLK | 1744 | Fuel Injector #1
D5 | LT GRN/BLK | 1745 | Fuel Injector #2 | D5 | LT GRN/BLK | 1745 | Fuel Injector #2
D6 | PNK/BLK | 1746 | Fuel Injector #3 | D6 | PNK/BLK | 1746 | Fuel Injector #3
D7 | LT BLU/BLK | 844 | Fuel Injector #4 | D7 | LT BLU/BLK | 844 | Fuel Injector #4
E1 | WHT | 423 | EST Control Signal | E1 | WHT | 423 | EST Control Signal
E2 | TAN/BLK | 424 | EST Bypass Signal | E2 | TAN/BLK | 424 | EST Bypass Signal
E3 | DK GRN/WHT | 428 | Canister Purge Solenoid Output | E3 | DK GRN/WHT | 428 | Canister Purge Solenoid Output
E4 | PPL/WHT | 430 | EST Reference Signal | E4 | PPL/WHT | 430 | EST Reference Signal
E5 | TAN/BLK | 231 | Oil Pressure Signal | E5 | TAN/BLK | 231 | Oil Pressure Signal
E6 | GRY | 435 | EGR Solenoid Output | E6 | GRY | 435 | EGR Solenoid Output
E7 | LT BLU/WHT | 1747 | IAC Feed Coil A (High) | E7 | LT BLU/WHT | 1747 | IAC Feed Coil A (High)
F1 | RED | 225 | Alternator Reference Voltage | F1 | RED | 225 | Alternator Reference Voltage
F2 | -- | -- | Not Used | F2 | -- | -- | Not Used
F6 | YEL | 400 | VSS Signal | F6 | YEL | 400 | VSS Signal
F7 | PPL | 401 | VSS Return | F7 | PPL | 401 | VSS Return
G1 | -- | -- | Not Used | G1 | -- | -- | Not Used
G7 | PPL | 6 | Starter Solenoid Feed | G7 | PPL | 6 | Starter Solenoid Feed
H1 | YEL | 410 | CTS Signal | H1 | YEL | 410 | CTS Signal
H2 | PPL | 412 | HO2S Signal | H2 | PPL | 412 | HO2S Signal
H6 | TAN | 413 | HO2S Return | H6 | TAN | 413 | HO2S Return
H7 | DK BLU | 417 | TPS Signal | H7 | DK BLU | 417 | TPS Signal
J1 | LT BLU/BLK | 1748 | IAC Feed Coil A (Low) | J1 | LT BLU/BLK | 1748 | IAC Feed Coil A (Low)
J2 | LT GRN/WHT | 1749 | IAC Feed Coil B (High) | J2 | LT GRN/WHT | 1749 | IAC Feed Coil B (High)
J3 | LT GRN/BLK | 444 | IAC Feed Coil B (Low) | J3 | LT GRN/BLK | 444 | IAC Feed Coil B (Low)
J4 | BLK | 452 | Sensor Return | J4 | BLK | 452 | Sensor Return
J5 | RED/BLK | 453 | EST Signal (Low) | J5 | RED/BLK | 453 | EST Signal (Low)
J6 | GRY | 474 | 5 Volt Reference | J6 | GRY | 474 | 5 Volt Reference
J7 | DK BLU | 496 | Knock Sensor Signal | J7 | DK BLU | 496 | Knock Sensor Signal
K1 | BLK/WHT | 845 | Fuel Injector #5 | K1 | BLK/WHT | 845 | Fuel Injector #5
K2 | YEL/BLK | 846 | Fuel Injector #6 | K2 | YEL/BLK | 846 | Fuel Injector #6
K3 | BRN | 1174 | Oil Level Sensor Return | K3 | BRN | 1174 | Oil Level Sensor Return
K4 | -- | -- | Not Used | K4 | -- | -- | Not Used
K5 | BRN | 1456 | EGR Position Signal | K5 | BRN | 1456 | EGR Position Signal
K6 | RED/BLK | 380 | A/C Pressure Sensor Signal | K6 | RED/BLK | 380 | A/C Pressure Sensor Signal
K7 | LT GRN | 36 | Coolant Temperature Signal | K7 | LT GRN | 36 | Coolant Temperature Signal
L1 | BLK | 808 | Sensor Return | L1 | BLK | 808 | Sensor Return
L2 | GRY | 1724 | Supercharger Boost Solenoid Output | L2 | GRY | 1724 | Supercharger Boost Solenoid Output
L3 | PNK | 1039 | Fused Output (IGN) | L3 | PNK | 1039 | Fused Output (IGN)
L4 | -- | -- | Not Used | L4 | -- | -- | Not Used
L5 | WHT | 121 | Tachometer Signal | L5 | WHT | 121 | Tachometer Signal
L6-L7 | -- | -- | Not Used | L6-L7 | -- | -- | Not Used
M1 | BLK` | 470 | Sensor Return | M1 | BLK | 470 | Sensor Return
M2 | ORN/BLK | 469 | MAP Sensor Return | M2 | ORN/BLK | 469 | MAP Sensor Return
M3 | LT BLU | 1876 | Knock Sensor Signal 2 | M3 | LT BLU | 1876 | Knock Sensor Signal 2
M4 | WHT | 257 | EGR Vent Solenoid Output | M4 | WHT | 257 | EGR Vent Solenoid Output
M5 | GRY | 23 | Alternator Field Duty Cycle Signal | M5 | GRY | 23 | Alternator Field Duty Cycle Signal
M6 | -- | -- | Not Used | M6 | -- | -- | Not Used
M7 | GRY | 1787 | Variable Steering Feed (High Effort) | M7 | GRY | 1787 | Variable Steering Feed (High Effort)
N1 | DK BLU | 338 | Fused Output (IGN) | N1 | DK BLU | 338 | Fused Output (IGN)
N2 | RED | 1642 | Battery | N2 | RED | 1642 | Battery
N3 | RED | 1642 | Fused Output (BAT) | N3 | RED | 1642 | Fused Output Battery
N4 | -- | -- | Not Used | N4 | -- | -- | Not Used
N5 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed | N5 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed
N6 | -- | -- | Not Used | N6 | -- | -- | Not Used
N7 | WHT | 345 | Variable Steering Feed (Low Effort) | N7 | WHT | 345 | Variable Steering Feed (Low Effort)

#### C101 (Oldsmobile)

Connector Part Information |

• | 12129207

• | 78 Way F Metri-Pack MXD (BLK)

Connector Part Information

• | 12176688

• | 78 Way M Metri-Pack MXD (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | LT BLU/WHT | 1747 | IAC Feed Coil A (High) | A1 | LT BLU/WHT | 1747 | IAC Feed Coil A (High)
A2 | PNK | 239 | Fused Output (IGN) | A2 | PNK | 239 | Fused Output (IGN)
A3 | PPL | 1666 | HO2S Signal | A3 | PPL | 1666 | HO2S Signal
A4 | -- | -- | Not Used | A4 | -- | -- | NOt Used
A5 | RED | 1642 | Battery | A5 | RED | 1642 | Battery
A6 | GRY | 435 | EGR Solenoid Output | A6 | GRY | 435 | EGR Solenoid Output
A7 | BLK/WHT | 651 | Ground | A7 | BLK/WHT | 651 | Ground
B1 | BLK | 552 | Sensor Return | B1 | BLK | 552 | Sensor Return
B2 | RED/BLK | 877 | Fuel Injector #7 | B2 | RED/BLK | 877 | Fuel Injector #7
B3 | DK BLU/WHT | 878 | Fuel Injector #8 | B3 | DK BLU/WHT | 878 | Fuel Injector #8
B4 | TAN | 1667 | HO2S Return | B4 | TAN | 1667 | HO2S Return
B5 | LT GRN | 1222 | Shift Solenoid A Output | B5 | LT GRN | 1222 | Shift Solenoid A Output
B6 | YEL/BLK | 1223 | Shift Solenoid B Output | B6 | YEL/BLK | 1223 | Shift Solenoid B Output
B7 | PNK | 1224 | Transmission Pressure Signal A | B7 | PNK | 1224 | Transmission Pressure Signal A
C1 | -- | -- | Not Used | C1 | -- | -- | Not Used
C2 | LT BLU/BLK | 1748 | IAC Feed Coil A (Low) | C2 | LT BLU/BLK | 1748 | IAC Feed Coil A (Low)
C3 | PNK | 339 | Fused Output (IGN) | C3 | PNK | 339 | Fused Output (IGN)
C4 | PNK | 439 | Ignition 1 Output | C4 | PNK | 439 | Ignition 1 Output
C5 | PNK | 1239 | Fused Output (IGN) | C5 | PNK | 1239 | Fused Output (IGN)
C6 | BLK | 1350 | Ground | C6 | BLK | 1350 | Ground
C7 | -- | -- | Not Used | C7 | -- | -- | Not Used
D1 | DK BLU | 604 | A/C High Pressure Output | D1 | DK BLU | 604 | A/C High Pressure Output
D2 | LT BLU/BLK | 647 | Crankshaft Position Output | D2 | LT BLU/BLK | 647 | Crankshaft Position Output
D3 | LT GRN/WHT | 1749 | IAC Feed Coil B (High) | D3 | LT GRN/WHT | 1749 | IAC Feed Coil B (High)
D4 | BLK | 1744 | Fuel Injector #1 | D4 | BLK | 1744 | Fuel Injector #1
D5 | LT GRN/BLK | 1745 | Fuel Injector #2 | D5 | LT GRN/BLK | 1745 | Fuel Injector #2
D6 | PNK/BLK | 1746 | Fuel Injector #3 | D6 | PNK/BLK | 1746 | Fuel Injector #3
D7 | LT BLU/BLK | 844 | Fuel Injector #4 | D7 | LT BLU/BLK | 844 | Fuel Injector #4
E1 | WHT | 423 | EST Control Signal | E1 | WHT | 423 | EST Control Signal
E2 | TAN/BLK | 424 | EST Bypass Signal | E2 | TAN/BLK | 424 | EST Bypass Signal
E3 | DK GRN/WHT | 428 | Canister Purge Solenoid Output | E3 | DK GRN/WHT | 428 | Canister Purge Solenoid Output
E4 | PPL/WHT | 430 | EST Reference Signal | E4 | PPL/WHT | 430 | EST Reference Signal
E5 | LT GRN | 432 | MAP Signal | E5 | LT GRN | 432 | MAP Signal
E6 | YEL | 492 | MAF Sensor Signal | E6 | YEL | 492 | MAF Signal
E7 | GRY | 23 | Alternator Duty Signal | E7 | GRY | 23 | Alternator Duty Signal
F1 | RED | 225 | Alternator Reference Voltage | F1 | RED | 225 | Alternator Reference Voltage
F2 | TAN/BLK | 231 | Oil Pressure Signal | F2 | TAN/BLK | 231 | Oil Pressure Signal
F6 | YEL | 400 | VSS Signal | F6 | YEL | 400 | VSS Signal
F7 | PPL | 401 | VSS Return | F7 | PPL | 401 | VSS Return
G1 | BLK/WHT | 451 | PCM Ground | G1 | BLK/WHT | 451 | PCM Ground
G7 | PPL | 6 | Starter Solenoid Feed | G7 | PPL | 6 | Starter Solenoid Feed
H1 | YEL | 410 | CTS Signal | H1 | YEL | 410 | CTS Signal
H2 | PPL | 412 | HO2S Signal | H2 | PPL | 412 | HO2S Signal
H6 | TAN | 413 | HO2S Return | H6 | TAN | 413 | HO2S Return
H7 | DK BLU | 417 | TPS Signal | H7 | DK BLU | 417 | TPS Signal
J1 | GRY | 474 | 5 Volt Reference | J1 | GRY | 474 | 5 Volt Reference
J2-J3 | -- | -- | Not Used | J2-J3 | -- | -- | Not Used
J4 | PNK | 639 | Fused Output (IGN) | J4 | PNK | 639 | Fused Output (IGN)
J5 | RED/BLK | 453 | EST Signal (Low) | J5 | RED/BLK | 453 | EST Signal (Low)
J6 | LT BLU/BLK | 1688 | 5 Volt Reference | J6 | LT BLU/BLK | 1698 | 5 Volt Reference
J7 | DK BLU | 496 | Knock Sensor Signal | J7 | DK BLU | 496 | Knock Sensor Signal
K1 | BLK/WHT | 845 | Fuel Injector #5 | K1 | BLK/WHT | 845 | Fuel Injector
K2 | YEL/BLK | 846 | Fuel Injector #6 | K2 | YEL/BLK | 846 | Fuel Injector
K3 | BRN | 1174 | Oil Level Sensor Return | K3 | BRN | 1174 | Oil Level Sensor Return
K4 | -- | -- | Not Used | K4 | -- | -- | Not Used
K5 | BRN | 1456 | EGR Position Signal | K5 | BRN | 1456 | EGR Position Signal
K6 | TAN/BLK | 422 | TCC Solenoid Output | K6 | TAN/BLK | 422 | TCC Solenoid Output
K7 | LT GRN/BLK | 444 | IAC Feed Coil B (Low) | K7 | LT GRN/BLK | 444 | IAC Feed Coil B (Low)
L1 | PNK | 739 | Fused Output (IGN) | L1 | PNK | 739 | Fused Output (IGN)
L2 | ORN/BLK | 495 | Power Steering Pressure Sensor Signal | L2 | ORN/BLK | 495 | Power Steering Pressure Sensor Signal
L3 | TAN/WHT | 585 | Trans Temperature Sensor Signal | L3 | TAN/WHT | 585 | Trans Temperature Sensor Signal
L4 | PNK | 439 | Fused Output (IGN) | L4 | PNK | 439 | Fused Output (IGN)
L5 | LT BLU | 725 | Voltage Regulator Output | L5 | LT BLU | 725 | Voltage Regulator Output
L6 | BLK | 630 | Camshaft Position Signal | L6 | BLK | 630 | Camshaft Position Signal
L7 | BLK | 452 | Sensor Return | L7 | BLK | 452 | Sensor Return
M1 | DK BLU | 1225 | Trans Pressure Signal A | M1 | DK BLU | 1225 | Trans Pressure Signal A
M2 | RED | 1226 | Trans Pressure Signal B | M2 | RED | 1226 | Trans Pressure Signal
M3 | RED/BLK | 1228 | Trans Force Motor Feed | M3 | RED/BLK | 1228 | Trans Force Motor Feed
M4 | LT BLU/WHT | 1229 | Trans Force Motor Return | M4 | LT BLU/WHT | 1229 | Trans Force Motor Return
M5 | RED/BLK | 1230 | Trans Speed Signal Input | M5 | RED/BLK | 1230 | Trans Speed Signal Input
M6 | DK BLU/WHT | 1231 | Trans Speed Signal Return | M6 | DK BLU/WHT | 1231 | Trans Speed Signal Return
M7 | GRY | 1787 | Magna Steer Feed (High Effort) | M7 | GRY | 1787 | Magna Steer Feed (High Effort)
N1 | WHT | 121 | Tachometer Signal | N1 | WHT | 121 | Tachometer Signal
N2-N4 | -- | -- | Not Used | N2-N4 | -- | -- | Not Used
N5 | RED | 1642 | Fused Output (BAT) | N5 | RED | 1642 | Fused Output (BAT)
N6 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed | N6 | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed
N7 | WHT | 345 | Magna Steer Feed (Low Effort) | N7 | WHT | 345 | Magna Steer Feed (Low Effort)

#### C102 (Buick)

Connector Part Information |

• | 12065845

• | 30 Way F Metri-Pack Series Junction Systems (BLK)

Connector Part Information

• | 12160959

• | 30 Way M Metri-Pack Series Junction Systems (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | RED | 542 | Fused Output (BAT) | A1 | RED | 542 | Fused Output (BAT)
A2 | PPL | 6 | Starter Solenoid Feed | A2 | PPL | 6 | Starter Solenoid Feed
A3-B1 | -- | -- | Not Used | A3-B1 | -- | -- | Not Used
B2 | DK GRN | 29 | Horn Feed | B2 | DK GRN | 29 | Horn Feed
B3 | TAN | 833 | Wheel Speed Sensor Return, Right Front | B3 | TAN | 833 | Wheel Speed Sensor Return, Right Front
B4 | DK GRN | 872 | Wheel Speed Sensor Signal, Right Front | B4 | DK GRN | 872 | Wheel Speed Sensor Signal, Right Front
C1 | GRY | 397 | Cruise Control ON Switch Output | C1 | GRY | 397 | Cruise Control ON Switch Output
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
D1 | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output | D1 | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output
D2 | LT GRN | 11 | Headlamp Feed (High Beam) | D2 | LT GRN | 11 | Headlamp Feed (High Beam)
D3 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal | D3 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal
D4 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal | D4 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal
E1 | WHT | 345 | Magnetic Steering Variable Assist Motor Feed (Low Effort) | E1 | WHT | 345 | Magnetic Steering Variable Assist Motor Feed (Low Effort)
E4 | PNK | 639 | Fused Output (IGN) | E4 | PNK | 639 | Fused Output (IGN)
F1 | PNK | 639 | Fused Output (IGN) | F1 | PNK | 639 | Fused Output (IGN)
F4 | TAN | 12 | Headlamp Feed (Low Beam) | F4 | TAN | 12 | Headlamp Feed (Low Beam)
G1 | DK GRN | 95 | Windshield Wiper Motor Feed Low Speed | G1 | DK GRN | 95 | Windshield Wiper Motor Feed Low Speed
G2 | RED | 242 | Fused Output (BAT) | G2 | RED | 242 | Fused Output (BAT)
G3 | PPL | 420 | Brake Switch Output Torque Converter Clutch | G3 | PPL | 420 | Brake Switch Output Torque Converter Clutch
G4 | BRN | 341 | Fused Output (IGN) | G4 | BRN | 341 | Fused Output (IGN)
H1 | WHT | 17 | Stoplamp Switch Output | H1 | WHT | 17 | Stoplamp Switch Output
H4 | -- | -- | Not Used | H4 | -- | -- | Not Used
J1 | BLK | 1350 | Ground | J1 | BLK | 1350 | Ground
J2 | GRY | 91 | Windshield Wiper Relay Feed Coil | J2 | GRY | 91 | Windshield Wiper Relay Feed Coil
J3 | PPL | 92 | Windshield Wiper Motor Feed (High Speed) | J3 | PPL | 92 | Windshield Wiper Motor Feed (High Speed)
J4 | PNK | 94 | Windshield Washer Switch Signal | J4 | PNK | 94 | Windshield Washer Switch Signal
K1-K3 | -- | -- | Not Used | K1-K3 | -- | -- | Not Used

#### C102 (Oldsmobile)

Connector Part Information |

• | 12065845

• | 30 Way F Metri-Pack Series Junction Systems (BLK)

Connector Part Information

• | 12160959

• | 30 Way M Metri-Pack Series Junction Systems (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | RED | 542 | Fused Output (BAT) | A1 | RED | 542 | Fused Output (BAT)
A2 | PPL | 6 | Starter Solenoid Feed | A2 | PPL | 6 | Starter Solenoid Feed
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
B1 | PPL | 34 | Fog Lamp Feed | B1 | PPL | 34 | Fog Lamp Feed
B2 | DK GRN | 29 | Horn Feed | B2 | DK GRN | 29 | Horn Feed
B3 | TAN | 833 | Wheel Speed Sensor Return, Right Front | B3 | TAN | 833 | Wheel Speed Sensor Return, Right Front
B4 | DK GRN | 872 | Wheel Speed Sensor Signal, Right Front | B4 | DK GRN | 872 | Wheel Speed Sensor Signal, Right Front
C1 | GRY | 397 | Cruise Control ON Switch Output | C1 | GRY | 397 | Cruise Control ON Switch Output
C4 | BLK | 407 | Sensor Return | C4 | BLK | 407 | Sensor Return
D1 | -- | -- | Not Used | D1 | -- | -- | Not Used
D2 | LT GRN | 11 | Headlamp Feed (High Beam) | D2 | LT GRN | 11 | Headlamp Feed (High Beam)
D3 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal | D3 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal
D4 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal | D4 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal
E1 | WHT | 345 | Magnetic Steering Variable Assist Motor Feed (Low Effort) | E1 | WHT | 345 | Magnetic Steering Variable Assist Motor Feed (Low Effort)
E4 | PNK | 639 | Fused Output (IGN) | E4 | PNK | 639 | Fused Output (IGN)
F1 | -- | -- | Not Used | F1 | -- | -- | Not Used
F4 | TAN | 12 | Headlamp Feed (Low Beam) | F4 | TAN | 12 | Headlamp Feed (Low Beam)
G1 | DK GRN | 95 | Windshield Wiper Motor Feed Low Speed | G1 | DK GRN | 95 | Windshield Wiper Motor Feed Low Speed
G2 | RED | 242 | Fused Output (BAT) | G2 | RED | 242 | Fused Output (BAT)
G3 | PPL | 420 | Brake Switch Output Torque Converter Clutch | G3 | PPL | 420 | Brake Switch Output Torque Converter Clutch
G4 | BRN | 341 | Fused Output (IGN) | G4 | BRN | 341 | Fused Output (IGN)
H1 | WHT | 17 | Stoplamp Switch Output | H1 | WHT | 17 | Stoplamp Switch Output
H4 | PNK | 339 | Fused Output (IGN) | H4 | PNK | 339 | Fused Output (IGN)
J1 | BLK | 1350 | Ground | J1 | BLK | 1350 | Ground
J2 | GRY | 91 | Windshield Wiper Relay Feed Coil | J2 | GRY | 91 | Windshield Wiper Relay Feed Coil
J3 | PPL | 92 | Windshield Wiper Motor Feed (High Speed) | J3 | PPL | 92 | Windshield Wiper Motor Feed (High Speed)
J4 | PNK | 94 | Windshield Washer Switch Signal | J4 | PNK | 94 | Windshield Washer Switch Signal
K1-K3 | -- | -- | Not Used | K1-K3 | -- | -- | Not Used

#### C103

Connector Part Information |

• | 12052638

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | TAN | 833 | Wheel Speed Sensor Return (RH Front) | A | BLK | 833 | Wheel Speed Sensor Return (RH Front)
B | DK GRN | 872 | Wheel Speed Sensor Signal (RH Front) | B | WHT | 872 | Wheel Speed Sensor Signal (RH Front)

#### C104

Connector Part Information |

• | 12052638

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 873 | Wheel Speed Sensor Return (LH Front) | A | BLK | 873 | Wheel Speed Sensor Return (LH Front)
B | LT BLU | 830 | Wheel Speed Sensor Signal (LH Front) | B | WHT | 830 | Wheel Speed Sensor Signal (LH Front)

#### C105

Connector Part Information |

• | 12146044

• | 5 Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12092839

• | 5 Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED | 228 | Windshield Washer Pump Motor Feed | A | RED | 228 | Windshield Washer Motor Pump Feed
B | DK BLU | 227 | Windshield Washer Pump Motor Return | B | DK BLU | 227 | Windshield Washer Pump Motor Return
D | BLK | 1350 | Ground | D | BLK | 1350 | Ground
E | BLK/WHT | 99 | Windshield Washer Fluid Level Sensor | E | BLK/WHT | 99 | Windshield Washer Fluid Level Sensor

#### C107

Connector Part Information |

• | 12047932

• | 8 Way F Metri-Pack 150 Series Sealed (BLK)

Connector Part Information

• | 12047931

• | 8 Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 423 | Electronic Spark Timing Control Signal | A | WHT | 423 | Electronic Spark Timing Control Signal
B | TAN/BLK | 424 | Electronic Spark Timing Bypass Signal | B | TAN/BLK | 424 | Electronic Spark Timing Bypass Signal
C | LT BLU/BLK | 647 | Crankshaft Position Signal | C | LT BLU/BLK | 647 | Crankshaft Position Signal
D | PPL/WHT | 430 | Electronic Spark Timing Signal (High Ref.) | D | PPL/WHT | 430 | Electronic Spark Timing Signal (High Ref.)
E | WHT | 121 | Tachometer Signal | E | WHT | 121 | Tachometer Signal
F | BLK | 630 | Camshaft Position Signal | F | BLK | 630 | Camshaft Position Signal
G | RED/BLK | 453 | Electronic Spark Timing Signal (Low Ref.) | G | RED/BLK | 453 | Electronic Spark Timing Signal (Low Ref.)
H | DK BLU | 338 | Ignition Switch Output | H | PNK | 239 | Fused Output (IGN 1)

#### C114

Connector Part Information |

• | 12059471

• | 7 Way F Metri-Pack Mixed Series, Sealed (BLK)

Connector Part Information

• | 12052200

• | 7 Way M Metri-Pack Mixed Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 434 | Park/Neutral Position Switch Signal | A | ORN/BLK | 434 | Park/Neutral Position Switch Signal
B | PNK | 139 | Fuse Output - IGN1 | B | PNK | 139 | Fuse Output - IGN1
C | LT GRN | 275 | Park/Neutral Position Switch Output - Park | C | LT GRN | 275 | Park/Neutral Position Switch Output - Park
D | BLK/WHT | 451 | Ground | D | BLK/WHT | 451 | Ground
E | YEL/BLK | 625 | Theft System Starter Enable Relay Output - Coil | E | YEL/BLK | 625 | Theft System Starter Enable Relay Output - Coil
F | LT GRN | 24 | Back-Up Lamp Feed | F | LT GRN | 24 | Back-Up Lamp Feed
G | YEL | 575 | Theft System Starter Enable Relay Output | G | YEL | 575 | Theft System Starter Enable Relay Output

#### C127 (Oldsmobile)

Connector Part Information |

• | 12160280

• | 20 Way F Micro-Pack 100 W Series (GRY)

Connector Part Information

• | 12160542

• | 20 Way M Micro-Pack 100 W Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1744 | Fuel Injector #1 Output | A | BLK | 1744 | Fuel Injector #1 Output
B | LT GRN/BLK | 1745 | Fuel Injector #2 Output | B | LT GRN/BLK | 1745 | Fuel Injector #2 Output
C | RED/BLK | 877 | Fuel Injector #7 Output | C | RED/BLK | 877 | Fuel Injector #7 Output
D | PNK/BLK | 1746 | Fuel Injector #3 Output | D | PNK/BLK | 1746 | Fuel Injector #3 Output
E | LT BLU/BLK | 844 | Fuel Injector #4 Output | E | LT BLU/BLK | 844 | Fuel Injector #4 Output
F-L | -- | -- | Not Used | F-L | -- | -- | Not Used
M | BLK | 452 | Sensor Return | M | BLK | 452 | Sensor Return
N | PNK | 739 | Fused Output (IGN) | N | PNK | 739 | Fused Output (IGN)
P | PNK | 1239 | Fused Output (IGN) | P | PNK | 1239 | Fused Output (IGN)
R | LT GRN | 432 | MAP Sensor Signal | R | LT GRN | 432 | MAP Sensor Signal
S | GRY | 474 | 5 Volt Reference | S | GRY | 474 | 5 Volt Reference
T | BLK/WHT | 845 | Fuel Injector #5 Output | T | BLK/WHT | 845 | Fuel Injector #5 Output
U | YEL/BLK | 846 | Fuel Injector #6 Output | U | YEL/BLK | 846 | Fuel Injector #6 Output
V | DK BLU/WHT | 878 | Fuel Injector #8 Output | V | DK BLU/WHT | 878 | Fuel Injector #8 Output

#### C200 (Buick)

Connector Part Information |

• | 12162462

• | 116 Way F Metri-Pack Junction Systems (BLK)

Connector Part Information

• | 12047749

• | 116 Way M Metri-Pack Junction Systems (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1-B12 | -- | -- | Not Used | A1-B12 | -- | -- | Not Used
B13 | LT GRN | 376 | Digital Trip Odometer Reset Switch Signal | B13 | LT GRN | 376 | Digital Trip Odometer Reset Switch Signal
C1-C3 | -- | -- | Not Used | C1-C3 | -- | -- | Not Used
C4 | BRN | 1214 | Strut Position Sensor Feed (5 Volt Reference), Right Rear | C4 | BRN | 1214 | Strut Position Sensor Feed (5 Volt Reference), Right Rear
C5 | LT BLU | 1880 | HVAC Control Assembly Signal Driver | C5 | LT BLU | 1880 | HVAC Control Assembly Signal Driver
C6 | DK GRN | 734 | Inside Temperature Sensor Signal | C6 | DK GRN | 734 | Inside Temperature Sensor Signal
C7 | -- | -- | Not Used | C7 | -- | -- | Not Used
C8 | PPL | 1783 | Twilight sentinel Delay Signal | C8 | PPL | 1783 | Twilight sentinel Delay Signal
C9 | BRN | 41 | Fused Output (IGN) | C9 | BRN | 41 | Fused Output (IGN)
C10 | GRY | 8 | IP Lamp Feed | C10 | GRY | 8 | IP Lamp Feed
C11-D3 | -- | -- | Not Used | C11-D3 | -- | -- | Not Used
D4 | BRN/WHT | 1571 | Traction Control System Switch Signal | D4 | BRN/WHT | 1571 | Traction Control System Switch Signal
D5 | DK GRN | 145 | Power Antenna relay Feed (Coil) | D5 | DK GRN | 145 | Power Antenna relay Feed (Coil)
D6 | GRY/BLK | 308 | Parklamp Switch Signal (Park Lamps ON) | D6 | GRY/BLK | 308 | Parklamp Switch Signal (Park Lamps ON)
D7 | BLK | 1576 | Trunk Release Output | D7 | BLK | 1576 | Trunk Release Output
D8 | DK GRN | 835 | Diagnostic Signal (Entertainment and Comfort) | D8 | DK GRN | 835 | Diagnostic Signal (Entertainment and Comfort)
D9 | LT BLU | 1344 | Trunk Release Relay Output (Coil) | D9 | LT BLU | 1344 | Trunk Release Relay Output (Coil)
D10 | DK GRN | 44 | IP Lamps Dimmer Switch Output | D10 | DK GRN | 44 | IP Lamps Dimmer Switch Output
D11-E1 | -- | -- | Not Used | D11-E1 | -- | -- | Not Used
E2 | PNK | 39 | Fused Output (IGN) | E2 | PNK | 39 | Fused Output (IGN)
E11 | ORN | 440 | Fused Output (BAT) | E11 | ORN | 440 | Fused Output (BAT)
E12-G1 | -- | -- | Not Used | E12-G1 | -- | -- | Not Used
G2 | BLK/WHT | 351 | Ground | G2 | BLK/WHT | 351 | Ground
G11-H2 | -- | -- | Not Used | G11-H2 | -- | -- | Not Used
H3 | BRN | 1349 | Headlamp Switch Return | H3 | BRN | 1349 | Headlamp Switch Return
H4 | WHT | 103 | Headlamp Switch Signal (Headlamps ON) | H4 | WHT | 103 | Headlamp Switch Signal (Headlamps ON)
H5 | BLK | 150 | Ground | H5 | BLK | 150 | Ground
H6 | LT GRN | 1011 | Remote Radio Control Signal | H6 | LT GRN | 1011 | Remote Radio Control Signal
H7 | GRY | 1548 | Solar Sensor Signal (Passenger) | H7 | GRY | 1548 | Solar Sensor Signal (Passenger)
H8 | YEL | 32 | Fused Output (IP Lamps) | H8 | YEL | 32 | Fused Output (IP Lamps)
H9 | WHT | 278 | Photocell Signal | H9 | WHT/BLK | 278 | Photocell Signal
H10 | YEL | 61 | Outside Temperature Sensor Return | H10 | YEL | 61 | Outside Temperature Sensor Return
H11-J1 | -- | -- | Not Used | H11-J1 | -- | -- | Not Used
J2 | ORN | 1640 | Fused Output (BAT) | J2 | ORN | 1640 | Fused Output (BAT)
J3 | YEL | 390 | IP Lamp Feed (Tertiary) | J3 | YEL | 390 | IP Lamp Feed (Tertiary)
J4 | PPL | 1881 | HVAC Control Assembly Signal (Clock, Driver) | J4 | PPL | 1881 | HVAC Control Assembly Signal (Clock, Driver)
J5 | YEL | 43 | Fused Output (Accessory) | J5 | YEL | 43 | Fused Output (Accessory)
J6 | -- | -- | Not Used | J6 | -- | -- | Not Used
J7 | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock (BTSI) Solenoid Feed | J7 | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock (BTSI) Solenoid Feed
J8 | PPL/WHT | 724 | Vacuum Flourescent Dimming Signal | J8 | PPL/WHT | 724 | Vacuum Flourescent Dimming Signal
J9 | LT BLU/BLK | 590 | Solar Sensor Signal Driver | J9 | LT BLU/BLK | 590 | Solar Sensor Signal Driver
J10 | DK BLU | 1393 | Interior Lamp Relay Output (Coil) | J10 | DK BLU | 1393 | Interior Lamp Relay Output (Coil)
J11-L13 | -- | -- | Not Used | J11-L13 | -- | -- | Not Used

#### C200 (Oldsmobile)

Connector Part Information |

• | 12162462

• | 116 Way F Metri-Pack Junction Systems (BLK)

Connector Part Information

• | 12047749

• | 116 Way M Metri-Pack Junction Systems (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1-B4 | -- | -- | Not Used | A1-B4 | -- | -- | Not Used
B5 | WHT | 1512 | Power Mirror Switch Signal, Left Horizontal Motor, Right Direction | B5 | WHT | 1512 | Power Mirror Switch Signal, Left Horizontal Motor, Right Direction
B6 | LT BLU | 1516 | Power Mirror Switch Signal, Left Horizontal Motor, Left Direction | B6 | LT BLU | 1516 | Power Mirror Switch Signal, Left Horizontal Motor, Left Direction
B7 | YEL | 1517 | Power Mirror Switch Signal, Left Vertical Motor, Up Direction | B7 | YEL | 1517 | Power Mirror Switch Signal, Left Vertical Motor, Up Direction
B8 | LT GRN | 1514 | Power Mirror Switch Signal, Left Vertical Motor, Down Direction | B8 | LT GRN | 1514 | Power Mirror Switch Signal, Left Vertical Motor, Down Direction
B9 | RED/WHT | 1513 | Power Mirror Switch Signal, Right Horizontal Motor, Right Direction | B9 | RED/WHT | 1513 | Power Mirror Switch Signal, Right Horizontal Motor, Right Direction
B10 | PPL/WHT | 1515 | Power Mirror Switch Signal, Right Horizontal Motor, Down Direction | B10 | PPL/WHT | 1515 | Power Mirror Switch Signal, Right Horizontal Motor, Down Direction
B11-C4 | -- | -- | Not Used | B11-C4 | -- | -- | Not Used
C5 | ORN | 40 | Fused Output (BAT) | C5 | ORN | 40 | Fused Output (BAT)
C6 | DK GRN | 734 | Inside Temperature Sensor Signal | C6 | DK GRN | 734 | Inside Temperature Sensor Signal
C7 | YEL/BLK | 1784 | Twilight Sentinel Enable Signal | C7 | YEL/BLK | 1784 | Twilight Sentinel Enable Signal
C8 | PPL | 1783 | Twilight sentinel Delay Signal | C8 | PPL | 1783 | Twilight sentinel Delay Signal
C9 | YEL | 317 | Fog Lamp Relay Feed (Coil) | C9 | YEL | 317 | Fog Lamp Relay Feed (Coil)
C10 | GRY | 8 | IP Lamp Feed | C10 | GRY | 8 | IP Lamp Feed
C11-D4 | -- | -- | Not Used | C11-D4 | -- | -- | Not Used
D5 | DK GRN | 145 | Power Antenna relay Feed (Coil) | D5 | DK GRN | 145 | Power Antenna relay Feed (Coil)
D6 | ORN | 840 | Fused Output (BAT) | D6 | ORN | 840 | Fused Output (BAT)
D7 | PNK | 79 | Fuel Door Release Solenoid Feed | D7 | PNK | 79 | Fuel Door Release Solenoid Feed
D8 | DK GRN | 835 | Diagnostic Signal (Entertainment and Comfort) | D8 | DK GRN | 835 | Diagnostic Signal (Entertainment and Comfort)
D9 | BLK/WHT | 56 | Trunk Release Motor Feed | D9 | BLK/WHT | 56 | Trunk Release Motor Feed
D10 | BRN | 1244 | IP Lamp Feed #2 | D10 | BRN | 1244 | IP Lamp Feed #2
D11 | BRN | 1241 | Fused Output (IGN) | D11 | BRN | 1241 | Fused Output (IGN)
D12-E1 | -- | -- | Not Used | D12-E1 | -- | -- | Not Used
E2 | PNK | 39 | Fused Output (IGN) | E2 | PNK | 39 | Fused Output (IGN)
E11-F1 | -- | -- | Not Used | E11-F1 | -- | -- | Not Used
F2 | ORN | 1040 | Fused Output (BAT) | F2 | ORN | 1040 | Fused Output (BAT)
F11-G11 | -- | -- | Not Used | F11-G11 | -- | -- | Not Used
G12 | ORN | 440 | Fused Output (BAT) | G12 | ORN | 440 | Fused Output (BAT)
H1-H4 | -- | -- | Not Used | H1-H4 | -- | -- | Not Used
H5 | BLK | 150 | Ground | H5 | BLK | 150 | Ground
H6 | LT GRN | 1011 | Remote Radio Control Signal | H6 | LT GRN | 1011 | Remote Radio Control Signal
H7 | GRY | 1548 | Solar Sensor Signal (Passenger) | H7 | GRY | 1548 | Solar Sensor Signal (Passenger)
H8 | YEL | 32 | Fused Output (IP Lamps) | H8 | YEL | 32 | Fused Output (IP Lamps)
H9 | WHT | 278 | Photocell Signal | H9 | WHT | 278 | Photocell Signal
H10 | YEL | 61 | Outside Temperature Sensor Return | H10 | YEL | 61 | Outside Temperature Sensor Return
H11-J2 | -- | -- | Not Used | H11-J2 | -- | -- | Not Used
J3 | YEL | 390 | IP Lamp Feed (Tertiary) | J3 | YEL | 390 | IP Lamp Feed (Tertiary)
J4 | -- | -- | Not Used | J4 | -- | -- | Not Used
J5 | YEL | 43 | Fused Output (Accessory) | J5 | YEL | 43 | Fused Output (Accessory)
J6 | DK BLU | 1493 | Transmission Shift Select Indicator Lamp Output Performance | J6 | DK BLU | 1493 | Transmission Shift Select Indicator Lamp Output Performance
J7 | -- | -- | Not Used | J7 | -- | -- | Not Used
J8 | BLK/WHT | 351 | Ground | J8 | BLK/WHT | 351 | Ground
J9 | LT BLU/BLK | 590 | Solar Sensor Signal Driver | J9 | LT BLU/BLK | 590 | Solar Sensor Signal Driver
J10 | DK BLU | 1393 | Interior Lamp Relay Output (Coil) | J10 | DK BLU | 1393 | Interior Lamp Relay Output (Coil)
J11-K5 | -- | -- | Not Used | J11-K5 | -- | -- | Not Used
K6 | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock (BTSI) Solenoid Feed | K6 | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock (BTSI) Solenoid Feed
K7 | PPL | 34 | Fog Lamp Feed | K7 | PPL | 34 | Fog Lamp Feed
K8 | DK GRN | 44 | IP Lamps Dimmer Switch Output | K8 | DK GRN | 44 | IP Lamps Dimmer Switch Output
K9 | BRN/WHT | 1571 | Traction Control Syustem Switch Signal | K9 | BRN/WHT | 1571 | Traction Control Syustem Switch Signal
K10-L13 | -- | -- | Not Used | K10-L13 | -- | -- | Not Used

#### C202 (Buick)

Connector Part Information |

• | 12047842

• | 17 Way F Metri-Pack (BLK)

• | 12047837

• | 18 Way F Metri-Pack (BLK)

• | 12047840

• | 13 Way F Metri-Pack (GRY)

Connector Part Information

• | 12084132

• | 48 Way M Metri-Pack Junction Systems (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | WHT | 17 | Stoplamp Switch Output | A1 | WHT | 17 | Stoplamp Switch Output
A2 | DK GRN | 19 | Stoplamp/Turn Lamp Feed, Right Rear | A2 | DK GRN | 19 | Stoplamp/Turn Lamp Feed, Right Rear
A3 | YEL | 18 | Stoplamp/Turn Lamp Feed, Left Rear | A3 | YEL | 18 | Stoplamp/Turn Lamp Feed, Left Rear
A4 | PPL | 16 | Turn Signal Lamp Flasher Output | A4 | PPL | 16 | Turn Signal Lamp Flasher Output
A5 | BRN | 27 | Hazard Flasher Output | A5 | BRN | 27 | Hazard Flasher Output
A6 | DK BLU/WHT | 15 | Turn Signal Lamp Feed, Right Front | A6 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
A7 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front | A7 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
A8 | RED | 1654 | Fused output (Perimeter Lighting) | A8 | TAN | 1654 | Fused output (Perimeter Lighting)
A9 | BLK/WHT | 58 | Cornering Lamp Feed, Right Side | A9 | BLK | 58 | Cornering Lamp Feed, Right Side
A10 | ORN | 57 | Cornering Lamp Feed, Left Side | A10 | ORN | 57 | Cornering Lamp Feed, Left Side
A11 | BLK | 28 | Horn Relay Output (Coil) | A11 | BLK | 28 | Horn Relay Output (Coil)
A12 | GRY | 397 | Cruise Control ON Switch Output | A12 | GRY | 397 | Cruise Control ON Switch Output
A13 | PNK | 341 | Fused Output (IGN) | A13 | BRN | 341 | Fused Output (IGN)
A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal | A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal
A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal | A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal
A16 | WHT | 1073 | Ignition Key Resistor Feed | A16 | WHT/BLK | 1073 | Ignition Key Resistor Feed
A17 | WHT | 1074 | Ignition Key Resistor Return | A17 | PPL/WHT | 1074 | Ignition Key Resistor Return
B1 | LT GRN | 80 | Key Reminder Switch Signal | B1 | LT GRN | 80 | Key Reminder Switch Signal
B2 | BLK | 150 | Ground | B2 | BLK | 150 | Ground
B3 | TAN/WHT | 33 | Brake Warning Indicator Lamp Output | B3 | -- | -- | Not Used
B4 | LT GRN/BLK | 875 | ABS Indicator Lamp Drive Module Output | B4 | LT GRN/BLK | 875 | ABS Indicator Lamp Drive Module Output
B5 | RED | 1042 | Fused Output (BAT) | B5 | RED | 1042 | Fused Output (BAT)
B6 | PPL/WHT | 338 | Ignition Switch Output (Ignition #1) | B6 | DK BLU | 338 | Ignition Switch Output (Ignition #1)
C1 | PNK/WHT | 1390 | Ignition Switch Output (OFF, RUN, CRANK) | C1 | WHT | 1390 | Ignition Switch Output (OFF, RUN, CRANK)
C2 | -- | -- | Not Used | C2 | -- | -- | Not Used
C3 | YEL | 43 | Fused Output (Accessory) | C3 | YEL | 43 | Fused Output (Accessory)
C4 | GRY | 8 | IP Lamp Feed | C4 | GRY | 8 | IP Lamp Feed
C5 | PNK | 3 | Fused Output (IGN) | C5 | PNK | 3 | Fused Output (IGN)
C6 | ORN | 300 | Fused Output (IGN) | C6 | ORN | 300 | Fused Output (IGN)
D1 | YEL | 5 | Fused Output (IGN) | D1 | YEL | 5 | Fused Output (IGN)
D2 | RED | 1342 | Fused Output (BAT) | D2 | RED | 1342 | Fused Output (BAT)
D3 | LT GRN | 1011 | Remote Radio Control Signal | D3 | LT GRN | 1011 | Remote Radio Control Signal
D4 | BLK | 150 | Ground | D4 | BLK | 150 | Ground
D5 | RED/WHT | 1442 | Fused Output (BAT) | D5 | RED | 1442 | Fused Output (BAT)
D6 | BRN | 4 | Ignition Switch Output (Accessory) | D6 | BRN | 4 | Ignition Switch Output (Accessory)
E1 | YEL | 143 | Fused Output (Accessory) | E1 | YEL | 143 | Fused Output (Accessory)
E2 | GRY | 91 | Windshield Wiper Relay Feed (Coil) | E2 | GRY | 91 | Windshield Wiper Relay Feed (Coil)
E3 | DK GRN | 95 | Windshield Wiper Motor Feed (Low Speed) | E3 | DK GRN | 95 | Windshield Wiper Motor Feed (Low Speed)
E4 | PPL | 92 | Windshield Wiper Motor Feed (High Speed) | E4 | PPL | 92 | Windshield Wiper Motor Feed (High Speed)
E5 | PNK | 94 | Windshield Washer Switch Signal | E5 | PNK | 94 | Windshield Washer Switch Signal
E6 | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock (BTSI) Solenoid Feed | E6 | DK GRN/WHT | 1135 | Brake Transmission Shift Interlock (BTSI) Solenoid Feed
E7 | BLK | 150 | Ground | E7 | BLK/WHT | 150 | Ground
E8-E9 | -- | -- | Not Used | E8-E9 | -- | -- | Not Used
E10 | YEL/BLK | 307 | Headlamp Switdch Output (Flash to Pass) | E10 | YEL/BLK | 307 | Headlamp Switch Output (Flash to Pass)
E11 | BLK/WHT | 351 | Ground | E11 | BLK/WHT | 351 | Ground
E12 | -- | -- | Not Used | E12 | -- | -- | Not Used
E13 | LT GRN | 524 | Headlamp Dimmer Switch Output (High Beam) | E13 | PPL | 524 | Headlamp Dimmer Switch Output (High Beam)

#### C202 (Oldsmobile)

Connector Part Information |

• | 12047842

• | 17 Way F Metri-Pack (BLK)

• | 12047837

• | 18 Way F Metri-Pack (BLK)

• | 12047840

• | 13 Way F Metri-Pack (GRY)

Connector Part Information

• | 12084132

• | 48 Way M Metri-Pack Junction Systems (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | WHT | 17 | Stoplamp Switch Output | A1 | WHT | 17 | Stoplamp Switch Output
A2 | DK GRN | 19 | Stoplamp/Turn Lamp Feed, Right Rear | A2 | DK GRN | 19 | Stoplamp/Turn Lamp Feed, Right Rear
A3 | YEL | 18 | Stoplamp/Turn Lamp Feed, Left Rear | A3 | YEL | 18 | Stoplamp/Turn Lamp Feed, Left Rear
A4 | PPL | 16 | Turn Signal Lamp Flasher Output | A4 | PPL | 16 | Turn Signal Lamp Flasher Output
A5 | BRN | 27 | Hazard Flasher Output | A5 | BRN | 27 | Hazard Flasher Output
A6 | DK BLU/WHT | 15 | Turn Signal Lamp Feed, Right Front | A6 | DK BLU | 15 | Turn Signal Lamp Feed, Right Front
A7 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front | A7 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
A8 | RED | 1654 | Fused output (Perimeter Lighting) | A8 | TAN | 1654 | Fused output (Perimeter Lighting)
A9 | BLK/WHT | 58 | Cornering Lamp Feed, Right Side | A9 | BLK | 58 | Cornering Lamp Feed, Right Side
A10 | ORN | 57 | Cornering Lamp Feed, Left Side | A10 | ORN | 57 | Cornering Lamp Feed, Left Side
A11 | BLK | 28 | Horn Relay Output (Coil) | A11 | BLK | 28 | Horn Relay Output (Coil)
A12 | GRY | 397 | Cruise Control ON Switch Output | A12 | GRY | 397 | Cruise Control ON Switch Output
A13 | PNK | 341 | Fused Output (IGN) | A13 | BRN | 341 | Fused Output (IGN)
A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal | A14 | DK BLU | 84 | Cruise Control SET/COAST Switch Signal
A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal | A15 | GRY/BLK | 87 | Cruise Control RESUME/ACCEL Switch Signal
A16 | WHT | 1073 | Ignition Key Resistor Feed | A16 | WHT/BLK | 1073 | Ignition Key Resistor Feed
A17 | WHT | 1074 | Ignition Key Resistor Return | A17 | PPL/WHT | 1074 | Ignition Key Resistor Return
B1 | LT GRN | 80 | Key Reminder Switch Signal | B1 | LT GRN | 80 | Key Reminder Switch Signal
B2 | BLK | 150 | Ground | B2 | BLK | 150 | Ground
B3 | TAN/WHT | 33 | Brake Warning Indicator Lamp Output | B3 | TAN/WHT | 33 | Brake Warning Indicator Lamp Output
B4 | LT GRN/BLK | 875 | ABS Indicator Lamp Drive Module Output | B4 | LT GRN/BLK | 875 | ABS Indicator Lamp Drive Module Output
B5 | RED | 1042 | Fused Putput (BAT) | B5 | -- | -- | Not Used
B6 | PPL/WHT | 338 | Ignition Switch Output (IGN 1) | B6 | -- | -- | Not Used
C1 | PNK/WHT | 1390 | Ignition Switch Output (Off, Run, Crank) | C1 | -- | -- | Not Used
C2 | -- | -- | Not Used | C2 | -- | -- | Not Used
C3 | YEL | 43 | Fused Output (Accessory) | C3 | YEL | 43 | Fused Output (Accessory)
C4 | GRY | 8 | IP Lamp Feed #2 | C4 | GRY | 8 | IP Lamp Feed #2
C5 | PNK | 3 | Fused Output (IGN) | C5 | PNK | 3 | Fused Output (IGN)
C6 | ORN | 300 | Fused Output (IGN) | C6 | ORN | 300 | Fused Output (IGN)
D1 | YEL | 5 | Fused Output (IGN) | D1 | YEL | 5 | Fused Output (IGN)
D2 | RED | 1342 | Fused Output (BAT) | D2 | RED | 1342 | Fused Output (BAT)
D3 | LT GRN | 1011 | Remote Radio Control Signal | D3 | LT GRN | 1011 | Remote Radio Control Signal
D4 | BLK | 150 | Ground | D4 | BLK | 150 | Ground
D5 | RED | 1442 | Fused Output (BAT) | D5 | RED | 1442 | Fused Output (BAT)
D6 | BRN | 4 | Ignition Switch Output (Accessory) | D6 | BRN | 4 | Ignition Switch Output (Accessory)
E1 | YEL | 143 | Fused Output (Accessory) | E1 | YEL | 143 | Fused Output (Accessory)
E2 | GRY | 91 | Windshield Wiper Relay Feed (Coil) | E2 | GRY | 91 | Windshield Wiper Relay Feed (Coil)
E3 | DK GRN | 95 | Windshield Wiper Motor Feed (Low Speed) | E3 | DK GRN | 95 | Windshield Wiper Motor Feed (Low Speed)
E4 | PPL | 92 | Windshield Wiper Motor Feed (High Speed) | E4 | PPL | 92 | Windshield Wiper Motor Feed (High Speed)
E5 | PNK | 94 | Windshield Washer Switch Signal | E5 | PNK | 94 | Windshield Washer Switch Signal
E6 | BLK/WHT | 351 | Ground | E6 | BLK/WHT | 351 | Ground
E7 | BRN | 1349 | Headlamp Switch Return | E7 | BRN | 1349 | Headlamp Switch Return
E8 | GRY/BLK | 308 | Parklamp Switch Signal (Parklamps ON) | E8 | GRY/BLK | 308 | Parklamp Switch Signal (Parklamps ON)
E9 | YEL | 103 | Headlamp Switch Signal (Headlamps ON) | E9 | WHT | 103 | Headlamp Switch Signal (Headlamps ON)
E10 | RED | 42 | Fused Output (BAT) | E10 | RED | 42 | Fused Output (BAT)
E11 | LT GRN | 11 | Headlamp Feed (High Beam) | E11 | LT GRN | 11 | Headlamp Feed (High Beam)
E12 | TAN | 12 | Headlamp Feed (Low Beam) | E12 | TAN | 12 | Headlamp Feed (Low Beam)
E13 | LT BLU | 1346 | Headlamp Relay Output (N.O. Contact) | E13 | LT BLU | 1346 | Headlamp Relay Output (N.O. Contact)

#### C203 (Buick)

Connector Part Information |

• | 12064998

• | 8 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12066195

• | 8 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | -- | -- | Not Used | B | -- | -- | Not Used
C | GRY | 8 | Instrument Panel Lamp Feed | C | GRY | 8 | Instrument Panel Lamp Feed
D | BLK | 150 | Ground | D | BLK | 150 | Ground
E | DK GRN/WHT | 1135 | Brake/Trans Shift Interlock Solenoid Feed | E | DK GRN/WHT | 1135 | Brake/Trans Shift Interlock Solenoid Feed
F | BRN | 1241 | Fused Output (IGN) | F | BRN | 1241 | Fused Output (IGN)
G | -- | -- | Not Used | G | -- | -- | Not Used
H | -- | -- | Not Used | H | -- | -- | Not Used

#### C203 (Oldsmobile)

Connector Part Information |

• | 12129431

• | 16 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129427

• | 16 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | -- | -- | Not Used | C | -- | -- | Not Used
D | GRY | 8 | IP Lamp Feed | D | GRY | 8 | IP Lamp Feed
E | ORN | 1040 | Fused Output (BAT) | E | ORN | 1040 | Fused Output (BAT)
F | BRN | 1241 | Fused Output (IGN) | F | BRN | 1241 | Fused Output (IGN)
G | PNK | 39 | Fused Output (IGN) | G | PNK | 39 | Fused Output (IGN)
H-N | -- | -- | Not Used | H-N | -- | -- | Not Used
P | BRN/WHT | 1571 | Traction Control System Switch Signal | P | BRN/WHT | 1571 | Traction Control System Switch Signal
R | -- | -- | Not Used | R | -- | -- | Not Used
S | DK BLU | 1493 | Transmission Shift Select Indicator Lamp Output (Performance) | S | DK BLU | 1493 | Transmission Shift Select Indicator Lamp Output (Performance)

#### C205

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12064750

• | 2 Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED | 342 | Fused Output (BAT) | A | RED | 342 | Fused Output (BAT)
B | BLK | 151 | Ground | B | BLK | 151 | Ground

#### C206

Connector Part Information |

• | 12129136

• | 4 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129135

• | 4 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1640 | Fused Output (BAT) | A | ORN | 1640 | Fused Output (BAT)
B | GRY | 8 | Instrument Panel Lamp Feed | B | GRY | 8 | Instrument Panel Lamp Feed
C | BRN | 1241 | Fused Output (IGN) | C | BRN | 1241 | Fused Output (IGN)
D | BLK | 150 | Ground | D | BLK | 150 | Ground

#### C207

Connector Part Information |

• | 12129431

• | 16 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129427

• | 16 Way M Metri-Pack 280 Series (BLKL)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 705 | 5 Volt Reference | A | GRY | 705 | 5 Volt Reference
B | GRY/BLK | 695 | A/C Mode Valve Position Sensor Signal | B | GRY/BLK | 695 | A/C Mode Valve Position Sensor Signal
C | BRN/WHT | 1218 | Mode Valve Motor Feed (Upper) | C | BRN/WHT | 1218 | Mode Valve Motor Feed (Upper)
D | RED | 708 | Mode Valve Position Sensor Signal (Upper) | D | RED | 708 | Mode Valve Position Sensor Signal (Upper)
E | YEL | 1318 | Mode Valve Motor Feed (Lower) | E | YEL | 1318 | Mode Valve Motor Feed (Lower)
F | YEL/BLK | 713 | Mode Valve Position Sensor Signal (Def Htr) | F | YEL/BLK | 713 | Mode Valve Position Sensor Signal (Def Htr)
G | DK GRN | 1614 | Air Inlet Valve Motor Feed | G | DK GRN | 1614 | Air Inlet Valve Motor Feed
H | PPL | 722 | Mode Valve Position Sensor Signal (A/I) | H | PPL | 722 | Mode Valve Position Sensor Signal (A/I)
J | DK BLU | 1199 | Air Temperture Valve Motor Feed | J | DK BLU | 1199 | Air Temperture Valve Motor Feed
K | LT BLU | 733 | Air Temperture Valve Position Sensor Signal | K | LT BLU | 733 | Air Temperture Valve Position Sensor Signal
L | WHT/BLK | 1236 | Air Temperture Valve Motor Feed (Passenger) | L | WHT/BLK | 1236 | Air Temperture Valve Motor Feed (Passenger)
M | DK BLU/WHT | 1646 | Air Temperture Valve Position Sensor Signal (Passenger) | M | DK BLU | 1646 | Air temperture Position Sensor Signal (Passenger)
N | BRN | 541 | Fused Output (IGN) | N | BRN | 541 | Fused Output (IGN)
P | -- | -- | Not Used | P | -- | -- | Not Used
R | PPL | 65 | Blower Motor Feed | R | PPL | 65 | Blower Motor Feed
S | GRY/BLK | 754 | Blower Speed Signal Speed Control | S | GRY/BLK | 754 | Blower Speed Signal Speed Control

#### C208

Connector Part Information |

• | 12064762

• | 6 Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6 Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK BLU | 46 | Speaker Feed (RH Rear) | A | DK BLU | 46 | Speaker Feed (RH Rear)
B | LT BLU | 115 | Speaker Return (RH Rear) | B | LT BLU | 115 | Speaker Return (RH Rear)
C | YEL | 116 | Speaker Return (LH Rear) | C | YEL | 116 | Speaker Return (LH Rear)
D | BRN | 199 | Speaker Feed (LH Rear) | D | BRN | 199 | Speaker Feed (LH Rear)
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used

#### C209 (Buick)

Connector Part Information |

• | 12052832

• | 2 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12052833

• | 2 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 118 | Speaker Return (LH Front) | A | GRY | 118 | Speaker Return (LH Front)
B | TAN | 201 | Speaker Feed (LH Front) | B | TAN | 201 | Speaker Feed (LH Front)

#### C209 (Oldsmobile)

Connector Part Information |

• | 12052832

• | 2 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12052833

• | 2 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK GRN | 117 | Speaker Return (RH Front) | A | DK GRN | 117 | Speaker Return (RH Front)
B | LT GRN | 200 | Speaker Feed (RH Front) | B | LT GRN | 200 | Speaker Feed (RH Front)

#### C212

Connector Part Information |

• | 12064871

• | 10 Way F Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064872

• | 10 Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 599 | Audio Signal - LH Rear - Low Level | A | BRN | 599 | Audio Signal - LH Rear - Low Level
B-C | -- | -- | Not Used | B-C | -- | -- | Not Used
D | DK BLU | 546 | Audio Signal - RH Rear - Low Level | D | DK BLU | 546 | Audio Signal - RH Rear - Low Level
E | -- | -- | Not Used | E | -- | -- | Not Used
F | TAN | 511 | Audio Signal - LH Front - Low Level | F | TAN | 511 | Audio Signal - LH Front - Low Level
G | LT GRN/BLK | 512 | Audio Signal - RH Front - Low Level | G | LT GRN/BLK | 512 | Audio Signal - RH Front - Low Level
H | WHT | 513 | Speaker Return - Low Level | H | WHT | 513 | Speaker Return - Low Level
J | BARE | 1782 | Drain Wire Return | J | BARE | 1782 | Drain Wire Return
K | PNK | 608 | 14 Volt Reference | K | PNK | 608 | 14 Volt Reference

#### C215

Connector Part Information |

• | 12065398

• | 8 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12065396

• | 8 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN/WHT | 367 | Remote Radio Signal Left Audio | A | BRN/WHT | 367 | Remote Radio Signal Left Audio
B | DK GRN/WHT | 368 | Remote Radio Signal Right Audio | B | DK GRN/WHT | 368 | Remote Radio Signal Right Audio
C | BLK/WHT | 372 | Remote Radio Return Audio | C | BLK/WHT | 372 | Remote Radio Return Audio
D | BARE | 514 | Drain Return Wire | D | BARE | 514 | Drain Return Wire
E | -- | -- | Not Used | E | -- | -- | Not Used
F | DK GRN | 835 | Diagnostic Signal (Ent. and Comfort) | F | DK GRN | 835 | Diagnostic Signal (Ent. and Comfort)
G | -- | -- | Not Used | G | -- | -- | Not Used
H | ORN | 440 | Fused Output (BAT) | H | ORN | 440 | Fused Output (BAT)

#### C219 (Buick)

Connector Part Information |

• | 12065398

• | 8 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12065396

• | 8 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 1548 | Solar Sensor Signal (Passenger) | A | GRY | 1548 | Solar Sensor Signal (Passenger)
B | YEL | 61 | Outside Ambient Temperture Sensor Return | B | YEL | 61 | Outside Ambient Temperture Sensor Return
C | BLK/WHT | 351 | Ground | C | BLK/WHT | 351 | Ground
D | WHT | 278 | Photocell Signal | D | WHT/BLK | 278 | Photocell Signal
E | LT BLU/BLK | 590 | Solar Sensor Signal (Driver) | E | LT BLU/BLK | 590 | Solar Sensor Signal (Driver)
F-H | -- | -- | Not Used | F-H | -- | -- | Not Used

#### C219 (Oldsmobile)

Connector Part Information |

• | 12047886

• | 8 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12045688

• | 8 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 1548 | Solar Sensor Signal (Passenger) | A | GRY | 1548 | Solar Sensor Signal (Passenger)
B | YEL | 61 | Outside Ambient Temperture Sensor Return | B | YEL | 61 | Outside Ambient Temperture Sensor Return
C | BLK/WHT | 351 | Ground | C | BLK/WHT | 351 | Ground
D | WHT | 278 | Photocell Signal | D | WHT | 278 | Photocell Signal
E | LT BLU/BLK | 590 | Solar Sensor Signal (Driver) | E | LT BLU/BLK | 590 | Solar Sensor Signal (Driver)
F-H | -- | -- | Not Used | F-H | -- | -- | Not Used

#### C301 (Buick w/ A43)

Connector Part Information |

• | 12092249

• | 23 Way F Metri-Pack 280 Series, ACT (BLK)

Connector Part Information

• | 12092248

• | 23 Way M Metri-Pack 280 Series, ACT (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK GRN | 1518 | Power Seat Switch Signal Front Vertical Lip | A | DK GRN | 1518 | Power Seat Switch Signal Front Vertical Lip
B | YEL | 1519 | Power Seat Swiotch Signal Rear Vertical Lip | B | YEL | 1519 | Power Seat Swiotch Signal Rear Vertical Lip
C | DK BLU | 1520 | Power Seat Switch Signal Front Vertical Down | C | DK BLU | 1520 | Power Seat Switch Signal Front Vertical Down
D | LT BLU | 1521 | Power Seat Switch Signal Rear Vertical Down | D | LT BLU | 1521 | Power Seat Switch Signal Rear Vertical Down
E | TAN | 1522 | Power Seat Switch Signal Horizontal Forward | E | TAN | 1522 | Power Seat Switch Signal Horizontal Forward
F | LT GRN | 1523 | Power Seat Switch Signal Horizontal Rearward | F | LT GRN | 1523 | Power Seat Switch Signal Horizontal Rearward
G | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor, Right Direction | G | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor, Right Direction
H | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor, Left Direction | H | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor, Left Direction
J | YEL | 88 | Power Mirror Motor Feed, Left Vertical Motor, Up Direction | J | YEL | 88 | Power Mirror Motor Feed, Left Vertical Motor, Up Direction
K | LT GRN | 89 | Power Mirror Motor Feed, Left Vertical Motor, Down Direction | K | LT GRN | 89 | Power Mirror Motor Feed, Left Vertical Motor, Down Direction
L | RED WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor, Right Direction | L | RED WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor, Right Direction
M | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor, Down Direction | M | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor, Down Direction
N | ORN | 1340 | Fused Output (BAT) | N | ORN | 1340 | Fused Output (BAT)
P | -- | -- | Not Used | P | -- | -- | Not Used
R | LT GRN | 276 | Power Seat Motor Feed, Driver Recline Forward | R | LT GRN | 276 | Power Seat Motor Feed, Driver Recline Forward
S | LT BLU | 277 | Power Seat Motor Feed, Driver Recline Rearward | S | LT BLU | 277 | Power Seat Motor Feed, Driver Recline Rearward
T | GRY | 788 | Memory Mirror Position Sensor Feed 5 Volt Reference | T | GRY | 788 | Memory Mirror Position Sensor Feed 5 Volt Reference
U | BRN/WHT | 557 | Memory Seat Position Sensor Signal, Front Vertical Motor | U | BRN/WHT | 557 | Memory Seat Position Sensor Signal, Front Vertical Motor
V | DK GRN | 569 | Memory Seat Position Sensor Signal, Horizontal Motor | V | DK GRN | 569 | Memory Seat Position Sensor Signal, Horizontal Motor
W | TAN | 568 | Memory Seat Position Signal, Rear Vertical Motor | W | TAN | 568 | Memory Seat Position Signal, Rear Vertical Motor
X | BLK | 782 | Sensor Return Memory Seat/Mirror | X | BLK | 782 | Sensor Return Memory Seat/Mirror
Y | BLK | 150 | Ground | Y | BLK | 150 | Ground
Z | BLK/WHT | 238 | Seat Belt Switch Signal | Z | BLK/WHT | 238 | Seat Belt Switch Signal

#### C301 (Oldsmobile)

Connector Part Information |

• | 12092249

• | 23 Way F Metri-Pack 280 Series, ACT (BLK)

Connector Part Information

• | 12092248

• | 23 Way M Metri-Pack 280 Series, ACT (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 388 | Lumbar, Left Lower Deflate | A | GRY | 388 | Lumbar, Left Lower Deflate
B | PPL | 385 | Lumbar, Left Lower Inflate | B | PPL | 385 | Lumbar, Left Lower Inflate
C | RED | 387 | Lumbar, Left Upper Inflate | C | RED | 387 | Lumbar, Left Upper Inflate
D | YEL | 386 | Lumbar, Left Upper Deflate | D | YEL | 386 | Lumbar, Left Upper Deflate
E | WHT/BLK | 570 | Memory Seat Position Sensor Signal Driver Recliner Motor | E | -- | -- | Not Used
F | BLK | 150 | Ground | F | BLK | 150 | Ground
G | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor, Right Direction | G | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor, Right Direction
H | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor, Left Direction | H | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor, Left Direction
J | YEL | 88 | Power Mirror Motor Feed, Left Vertical Motor, Up Direction | J | YEL | 88 | Power Mirror Motor Feed, Left Vertical Motor, Up Direction
K | LT GRN | 89 | Power Mirror Motor Feed, Left Vertical Motor, Down Direction | K | LT GRN | 89 | Power Mirror Motor Feed, Left Vertical Motor, Down Direction
L | RED WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor, Right Direction | L | RED WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor, Right Direction
M | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor, Down Direction | M | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor, Down Direction
N | ORN | 1340 | Fused Output (BAT) | N | ORN | 1340 | Fused Output (BAT)
P | RED | 756 | Lumbar, Right Upper Inflate | P | RED | 756 | Lumbar, Right Upper Inflate
R | YEL | 757 | Lumbar, Right Upper Deflate | R | YEL | 757 | Lumbar, Right Upper Deflate
S | GRY | 758 | Lumbar, Right Lower Deflate | S | GRY | 758 | Lumbar, Right Lower Deflate
T | PPL | 759 | Lumbar, Right Lower Inflate | T | PPL | 759 | Lumbar, Right Lower Inflate
U | BRN/WHT | 557 | Memory Seat Position Sensor Signal, Front Vertical Motor | U | BRN/WHT | 557 | Memory Seat Position Sensor Signal, Front Vertical Motor
V | DK GRN | 569 | Memory Seat Position Sensor Signal, Horizontal Motor | V | DK GRN | 569 | Memory Seat Position Sensor Signal, Horizontal Motor
W | TAN | 568 | Memory Seat Position Signal, Rear Vertical Motor | W | TAN | 568 | Memory Seat Position Signal, Rear Vertical Motor
X | BLK | 782 | Sensor Return Memory Seat/Mirror | X | BLK | 782 | Sensor Return Memory Seat/Mirror
Y | GRY | 788 | Memory Mirror Position Sensor Feed (5 Volt Reference) | Y | GRY | 788 | Memory Mirror Position Sensor Feed (5 Volt Reference)
Z | BLK/WHT | 238 | Seat Belt Switch Signal | Z | BLK/WHT | 238 | Seat Belt Switch Signal

#### C303 (Buick)

Connector Part Information |

• | 12064769

• | 10 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1050 | Ground | A | BLK | 1050 | Ground
B | WHT | 156 | Courtesy Lamp Output | B | WHT | 156 | Courtesy Lamp Output
C | ORN | 1732 | 12 Volt Inadvertent Load Control | C | ORN | 1732 | 12 Volt Inadvertent Load Control
D | PNK | 39 | Fused Output (IGN) | D | PNK | 39 | Fused Output (IGN)
E | LT GRN | 24 | Backup Lamp Feed | E | LT GRN | 24 | Backup Lamp Feed
F | PNK | 1691 | Automatic Day/Night Mirror Return, Outside | F | PNK/BLK | 1691 | Automatic Day/Night Mirror Return, Outside
G | GRY | 1690 | Automatic Day/Night Mirror Signal Outside | G | GRY | 1690 | Automatic Day/Night Mirror Signal Outside
H | BLK/WHT | 351 | Ground | H | BLK/WHT | 351 | Ground
J | -- | -- | Not Used | J | DK GRN | 654 | Cellular Telephone Mircophone Return
K | -- | -- | Not Used | K | GRY | 655 | Cellular Telephone Mircophone Signal

#### C303 (Oldsmobile)

Connector Part Information |

• | 12064769

• | 10 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1050 | Ground | A | BLK | 1050 | Ground
B | WHT | 156 | Courtesy Lamp Output | B | WHT | 156 | Courtesy Lamp Output
C | ORN | 1732 | 12 Volt Inadvertent Load Control | C | ORN | 1732 | 12 Volt Inadvertent Load Control
D | PNK | 39 | Fused Output (IGN) | D | PNK | 39 | Fused Output (IGN)
E | LT GRN | 24 | Backup Lamp Feed | E | LT GRN | 24 | Backup Lamp Feed
F-G | -- | -- | Not Used | F-G | -- | -- | Not Used
H | BLK/WHT | 351 | Ground | H | BLK/WHT | 351 | Ground
J | -- | -- | Not Used | J | DK GRN | 654 | Cellular Telephone Mircophone Return
K | -- | -- | Not Used | K | GRY | 655 | Cellular Telephone Mircophone Signal

#### C305

Connector Part Information |

• | 12092249

• | 23 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12092248

• | 23 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A-E | -- | -- | Not Used | A-E | -- | -- | Not Used
F | BLK/WHT | 151 | Ground | F | -- | -- | Not Used
G | YEL | 288 | Power Seat Motor Feed Passenger Rear Vertical Up | G | YEL | 288 | Power Seat Motor Feed Passenger Rear Vertical Up
H | LT BLU | 289 | Power Seat Motor Feed Passenger Rear Vertical Down | H | LT BLU | 289 | Power Seat Motor Feed Passenger Rear Vertical Down
J | LT GRN | 290 | Power Seat Motor Feed Passenger Horizontal Aft | J | LT GRN | 290 | Power Seat Motor Feed Passenger Horizontal Aft
K | TAN | 296 | Power Seat Motor Feed Passenger Horizontal Fore | K | TAN | 296 | Power Seat Motor Feed Passenger Horizontal Fore
L | DK GRN | 297 | Power Seat Motor Feed Passenger Front Vertical Up | L | DK GRN | 297 | Power Seat Motor Feed Passenger Front Vertical Up
M | DK BLU | 298 | Power Seat Motor Feed Passenger Front Vertical Down | M | DK BLU | 298 | Power Seat Motor Feed Passenger Front Vertical Down
N | DK GRN | 76 | Power Seat Motor Feed Passenger Recline Fore | N | DK GRN | 76 | Power Seat Motor Feed Passenger Recline Fore
P | DK BLU | 77 | Power Seat Motor Feed Passenger Recline Aft | P | DK BLU | 77 | Power Seat Motor Feed Passenger Recline Aft
R-Z | -- | -- | Not Used | R-Z | -- | -- | Not Used

#### C307

Connector Part Information |

• | 12129081

• | 2 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129155

• | 2 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1340 | Fused Output (BAT) | A | ORN | 1340 | Fused Output (BAT)
B | BLK | 151 | Ground | B | BLK | 151 | Ground

#### C308

Connector Part Information |

• | 12020397

• | 3 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12020398

• | 3 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 141 | Fused Output (IGN) | A | BRN | 141 | Fused Output (IGN)
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BLK | 1050 | Ground | C | BLK | 1050 | Ground

#### C400

Connector Part Information |

• | 12129431

• | 16 Way F Metri-Pack 280, ACT (BLK)

Connector Part Information

• | 12129427

• | 16 Way M Metri-Pack 280, ACT (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED | 1242 | Fused Output (BAT) | A | RED | 1242 | Fused Output (BAT)
B-H | -- | -- | Not Used | B-H | -- | -- | Not Used
J | GRY | 118 | Speaker Return Left Front | J | GRY | 118 | Speaker Return Left Front
K | TAN | 201 | Speaker Feed Left Front | K | TAN | 201 | Speaker Feed Left Front
L | LT GRN | 200 | Speaker Feed Right Front | L | LT GRN | 200 | Speaker Feed Right Front
M | DK GRN | 117 | Speaker Return Right Front | M | DK GRN | 117 | Speaker Return Right Front
N | LT BLU | 115 | Speaker Return Right Rear | N | LT BLU | 115 | Speaker Return Right Rear
P | YEL | 116 | Speaker Return Left Rear | P | YEL | 116 | Speaker Return Left Rear
R | BRN | 199 | Speaker Feed Left Rear | R | BRN | 199 | Speaker Feed Left Rear
S | DK BLU | 46 | Speaker Feed Right Rear | S | DK BLU | 46 | Speaker Feed Right Rear

#### C401

Connector Part Information |

• | 12052499

• | 5 Way F Metri-Pack 150 Series (MD GRY)

Connector Part Information

• | 12052480

• | 5 Way M Metri-Pack 150 Series (DK GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
B | BRN | 882 | Wheel Speed Sensor Signal RH Rear | B | BLK | 882 | Wheel Speed Sensor Signal RH Rear
C | BLK | 884 | Wheel Speed Sensor Signal LH Rear | C | BLK | 884 | Wheel Speed Sensor Signal LH Rear
E | -- | -- | Not Used | E | -- | -- | Not Used
F | RED | 885 | Wheel Speed Sensor Return LH Rear | F | WHT | 885 | Wheel Speed Sensor Return LH Rear
G | WHT | 883 | Wheel Speed Sensor Return RH Rear | G | WHT | 883 | Wheel Speed Sensor Return RH Rear

#### C404 (Buick)

Connector Part Information |

• | 12064762

• | 6 Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6 Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | PPL | 709 | Park Lamp Feed LH | B | PPL | 709 | Park Lamp Feed LH
C | LT GRN | 24 | Backup Lamp Feed | C | LT GRN | 24 | Backup Lamp Feed
D | BRN/WHT | 309 | Park Lamp Feed RH | D | BRN/WHT | 309 | Park Lamp Feed RH
E | -- | -- | Not Used | E | -- | -- | Not Used
F | BLK | 1250 | Ground | F | BLK | 1250 | Ground

#### C405

Connector Part Information |

• | 12129136

• | 4 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129135

• | 4 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK GRN | 19 | Stop/Turn Lamp Feed RH Rear | A | DK GRN | 19 | Stop/Turn Lamp Feed RH Rear
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BRN/WHT | 309 | Park Lamp Feed RH | C | BRN/WHT | 309 | Park Lamp Feed RH
D | BLK | 1250 | Ground | D | BLK | 1250 | Ground

#### C406

Connector Part Information |

• | 12129136

• | 4 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129135

• | 4 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 18 | Stop/Turn Lamp Feed LH Rear | A | YEL | 18 | Stop/Turn Lamp Feed LH Rear
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BRN/WHT | 309 | Park Lamp Feed LH | C | BRN/WHT | 309 | Park Lamp Feed LH
D | BLK | 1250 | Ground | D | BLK | 1250 | Ground

#### C407

Connector Part Information |

• | 12064762

• | 6 Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6 Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 18 | Stop/Turn Lamp Feed LH Rear | A | YEL | 18 | Stop/Turn Lamp Feed LH Rear
B | DK GRN | 19 | Stop/Turn Lamp Feed RH Rear | B | DK GRN | 19 | Stop/Turn Lamp Feed RH Rear
C | LT GRN | 24 | Backup Lamp Feed | C | LT GRN | 24 | Backup Lamp Feed
D | BRN/WHT | 309 | Park Lamp Feed RH | D | BRN/WHT | 309 | Park Lamp Feed RH
E | PPL | 709 | Park Lamp Feed LH | E | PPL | 709 | Park LAmp Feed LH
F | BLK | 1250 | Ground | F | BLK | 1250 | Ground

#### C420

Connector Part Information |

• | 12059471

• | 7 Way F Metri-Pack Mixed Series, Sealed (BLK)

Connector Part Information

• | 12052200

• | 7 Way M Metri-Pack Mixed Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PPL | 30 | Fuel Gauge Sensor Signal | A | PPL | 30 | Fuel Gauge Sensor Signal
B | GRY | 605 | 5 Volt Reference | B | GRY | 605 | 5 Volt Reference
C | BLK | 808 | Sensor Return | C | BLK | 808 | Sensor Return
D | BLK/WHT | 651 | Fuel Gauge Sensor Ground | D | BLK/WHT | 651 | Fuel Gauge Sensor Ground
E | GRY | 120 | Fuel Pump Motor Feed | E | GRY | 120 | Fuel Pump Motor Feed
F | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | F | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
G | BLK | 1050 | Ground | G | BLK | 1050 | Ground

#### C501 (Buick)

Connector Part Information |

• | 12064769

• | 10 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Feed | A | GRY | 8 | Instrument Panel Lamp Feed
B | TAN | 201 | Speaker Feed Left Front | B | TAN | 201 | Speaker Feed Left Front
C | ORN/BLK | 434 | Transmission Mounted Neutral Safety Switch Signal | C | ORN/BLK | 434 | Transmission Mounted Neutral Safety Switch Signal
D | BLK | 150 | Ground | D | BLK | 150 | Ground
E | GRY | 118 | Speaker Return Left Front | E | GRY | 118 | Speaker Return Left Front
F | BLK | 1576 | Trunk Release Switch Output | F | BLK | 1576 | Trunk Release Switch Output
G | ORN | 740 | Fuse Output - Battery | G | ORN | 740 | Fuse Output - Battery
H | PNK | 79 | Fuel Door Release Solenoid Feed | H | PNK | 79 | Fuel Door Release Solenoid Feed
J | ORN | 1732 | 12 Volt Inadvertent Load Control | J | ORN | 1732 | 12 Volt Inadvertent Load Control
K | WHT | 156 | Courtesy Lamp Output | K | WHT | 156 | Courtesy Lamp Output

#### C501 (Oldsmobile)

Connector Part Information |

• | 12129431

• | 16 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129427

• | 16 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 118 | Speaker Return Left Front | A | GRY | 118 | Speaker Return Left Front
B | ORN | 1732 | 12 Volt Inadvertent Load Control | B | ORN | 1732 | 12 Volt Inadvertent Load Control
C | WHT | 156 | Courtesy Lamp Output | C | WHT | 156 | Courtesy Lamp Output
D | BRN | 141 | Fused Output - IGN | D | BRN | 141 | Fused Output - IGN
E | DK BLU | 1307 | Power Window Master Switch Ouput - Lockout | E | DK BLU | 1307 | Power Window Master Switch Ouput - Lockout
F | DK BLU | 164 | Power Window Motor Feed Left Front Window Up | F | DK BLU | 164 | Power Window Motor Feed Left Front Window Up
G | GRY | 1136 | Power Window Master Switch Output - Left Front Window Down | G | GRY | 1136 | Power Window Master Switch Output - Left Front Window Down
H | LT BLU | 166 | Power Window Master Switch Ouput - Right Front Window Up | H | LT BLU | 166 | Power Window Master Switch Ouput - Right Front Window Up
J | BLK | 150 | Ground | J | BLK | 150 | Ground
K | TAN | 167 | Power Window Master Switch Output - Right Front Window Down | K | TAN | 167 | Power Window Master Switch Output - Right Front Window Down
L | DK GRN | 168 | Power Window Master Switch Output - Left Rear Window Up | L | DK GRN | 168 | Power Window Master Switch Output - Left Rear Window Up
M | PPL | 169 | Power Window Master Switch Output - Left Rear Window Down | M | PPL | 169 | Power Window Master Switch Output - Left Rear Window Down
N | LT GRN | 170 | Power Window Master Switch Output - Right Rear Window Up | N | LT GRN | 170 | Power Window Master Switch Output - Right Rear Window Up
P | PPL | 171 | Power Window Master Switch Output - Right Rear Window Down | P | PPL | 171 | Power Window Master Switch Output - Right Rear Window Down
R | GRY | 8 | Instrument Panel Lamp Feed | R | GRY | 8 | Instrument Panel Lamp Feed
S | TAN | 201 | Speaker Feed Left Front | S | TAN | 201 | Speaker Feed Left Front

#### C505 (Buick)

Connector Part Information |

• | 12129432

• | 16 Way F Metri-Pack 280 Series (GRY)

Connector Part Information

• | 12129428

• | 16 Way M Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A-B | -- | -- | Not Used | A-B | -- | -- | Not Used
C | BLK | 150 | Ground | C | BLK | 150 | Ground
D | TAN | 167 | Power Window Master Switch Output (RH Front Window Down) | D | TAN | 167 | Power Window Master Switch Output (RH Front Window Down)
E | LT BLU | 166 | Power Window Master Switch Output (RH Front Window Up) | E | LT BLU | 166 | Power Window Master Switch Output (RH Front Window Up)
F | GRY | 1136 | Power Window Master Switch Output (LH Front Window Down) | F | GRY | 1136 | Power Window Master Switch Output (LH Front Window Down)
G | DK BLU | 164 | Power Window Motor Feed (LH Front Window Up) | G | DK BLU | 164 | Power Window Motor Feed (LH Front Window Up)
H | BLK/WHT | 151 | Ground | H | BLK/WHT | 151 | Ground
J | RED/BLK | 780 | Power Door Lock Switch Output (Driver Switch Lock) | J | RED/BLK | 790 | Power Door Lock Switch Output (Driver Switch Lock)
K | ORN/BLK | 781 | Power Door Lock Switch Output (Driver Switch Unlock) | K | ORN/BLK | 791 | Power Door Lock Switch Output (Driver Switch Unlock)
L-M | -- | -- | Not Used | L-M | -- | -- | Not Used
N | BRN | 141 | Fused Output (IGN) | N | BRN | 141 | Fused Output (IGN)
P-S | -- | -- | Not Used | P-S | -- | -- | Not Used

#### C600

Connector Part Information |

• | 12064769

• | 10 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Feed | A | GRY | 8 | Instrument Panel Lamp Feed
B | LT GRN | 200 | Speaker Feed Right Front | B | LT GRN | 200 | Speaker Feed Right Front
C | -- | -- | Not Used | C | -- | -- | Not Used
D | BLK/WHT | 151 | Ground | D | BLK/WHT | 151 | Ground
E | DK GRN | 117 | Speaker Return Right Front | E | DK GRN | 117 | Speaker Return Right Front
F-H | -- | -- | Not Used | F-H | -- | -- | Not Used
J | ORN | 1732 | 12 Volt Inadvertent Load Control | J | ORN | 1732 | 12 Volt Inadvertent Load Control
K | WHT | 156 | Courtesy Lamp Output | K | WHT | 156 | Courtesy Lamp Output

#### C601

Connector Part Information |

• | 12129431

• | 16 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12129427

• | 16 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK GRN | 117 | Speaker Return Right Front | A | DK GRN | 117 | Speaker Return Right Front
B | ORN | 1732 | 12 Volt Inadvertent Load Control | B | ORN | 1732 | 12 Volt Inadvertent Load Control
C | WHT | 156 | Courtesy Lamp Output | C | WHT | 156 | Courtesy Lamp Output
D | DK BLU | 1307 | Power Window Master Switch Output - Lockout | D | DK BLU | 1307 | Power Window Master Switch Output - Lockout
E | LT BLU | 166 | Power Window Master Switch Output - Right Front Window Up | E | LT BLU | 166 | Power Window Master Switch Output - Right Front Window Up
F | TAN | 167 | Power Window Master Switch Output - Right Front Window Down | F | TAN | 167 | Power Window Master Switch Output - Right Front Window Down
G | DK BLU | 666 | Power Window Motor Feed Right Front Window Up | G | DK BLU | 666 | Power Window Motor Feed Right Front Window Up
H | GRY | 8 | Instrument Panel Lamp Feed | H | GRY | 8 | Instrument Panel Lamp Feed
J | BRN | 667 | Power Window Motor Feed Right Front Window Down | J | BRN | 667 | Power Window Motor Feed Right Front Window Down
K | BLK/WHT | 151 | Ground | K | BLK/WHT | 151 | Ground
L-N | -- | -- | Not Used | L-N | -- | -- | Not Used
P-R | -- | -- | Not Used | P-R | -- | -- | Not Used
S | LT GRN | 200 | Speaker Feed Right Front | S | LT GRN | 200 | Speaker Feed Right Front

#### C605 (Buick)

Connector Part Information |

• | 12129432

• | 16 Way F Metri-Pack 280 Series (GRY)

Connector Part Information

• | 12129428

• | 16 Way M Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK/WHT | 151 | Ground | A | BLK/WHT | 151 | Ground
B-C | -- | -- | Not Used | B-C | -- | -- | Not Used
D | TAN | 167 | Power Window Master Switch Output (RH Front Window Down) | D | TAN | 167 | Power Window Master Switch Output (RH Front Window Down)
E | BRN | 141 | Fused Output (IGN) | E | BRN | 141 | Fused Output (IGN)
F | LT BLU | 166 | Power Window Master Switch Output (RH Front Window Up) | F | LT BLU | 166 | Power Window Master Switch Output (RH Front Window Up)
G-K | -- | -- | Not Used | G-K | -- | -- | Not Used
L | DK BLU | 666 | Power Window Motor Feed (RH Front Window Up) | L | DK BLU | 666 | Power Window Motor Feed (RH Front Window Up)
M | BRN | 667 | Power Window Motor Feed (RH Front Window Down) | M | BRN | 667 | Power Window Motor Feed (RH Front Window Down)
N-P | -- | -- | Not Used | N-P | -- | -- | Not Used
R | ORN/BLK | 781 | Power Door Lock Switch Output (Driver Switch Unlock) | R | ORN/BLK | 781 | Power Door Lock Switch Output (Driver Switch Unlock)
S | RED/BLK | 780 | Power Door Lock Switch Output (Driver Switch Lock) | S | RED/BLK | 780 | Power Door Lock Switch Output (Driver Switch Lock)