For 1990-2009 cars

# POPPING NOISE FROM FRONT OF VEHICLE

#### SUBJECT: POPPING NOISE FROM FRONT OF VEHICLE WHEN TURNING STEERING WHEEL (INSTALL JOUNCE BUMPER AND BUSHING IN FRONT STRUT)

#### MODELS: 1994-96 BUICK LESABRE, PARK AVENUE 1995-96 BUICK RIVIERA 1994-96 OLDSMOBILE EIGHTY EIGHT, LSS, NINETY EIGHT 1995-96 OLDSMOBILE AURORA 1994-96 PONTIAC BONNEVILLE

#### CONDITION:

SOME OWNERS MAY COMMENT ON A POPPING NOISE FROM THE FRONT OF THE VEHICLE WHEN TURNING THE STEERING WHEEL WITH THE VEHICLE SITTING STILL OR DURING A PARKING MANEUVER.

#### CAUSE:

THIS CONDITION MAY BE DUE TO THE JOUNCE BUMPER CONTACTING/RUBBING ON THE STRUT ROD.

#### CORRECTION:

INSTALL IMPROVED JOUNCE BUMPER AND BUSHING IN FRONT STRUT FOLLOWING THE APPROPRIATE SERVICE PROCEDURE IN SECTION 3C OF THE SERVICE MANUAL.

#### PARTS INFORMATION:

MODEL YEAR VEHICLE P/N ===== ======= ===

1994-96 C/H 25656136 1995-96 G 25656137

PARTS ARE EXPECTED TO BE AVAILABLE JUNE 3, 1996.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED WARRANTY, USE:

LABOR LABOR OPERATION DESCRIPTION TIME ========= =========== =====

E3910/11 SHIELD AND/OR BUMPER, FRONT USE PUBLISHED STRUT - REPLACE (RT/LT) LABOR TIME

E3917 SHIELD AND/OR BUMPER, FRONT USE PUBLISHED STRUT - REPLACE (BOTH) LABOR TIME

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.