For 1990-2009 cars

# RADIAL TIRE/LEAD PULL CORRECTION CHARTS

#### MODELS AFFECTED: ALL FRONT WHEEL DRIVE VEHICLES

The radial tire lead/pull correction charts shown in the 1987 Chassis Service Manual are being superseded by the chart shown on reverse side of this bulletin. This new chart should be used to correct any lead/pull conditions on all front wheel drive vehicles.

This new chart will appear in the final editions of the 1988 Buick Chassis Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.