For 1990-2009 cars

## Sun Load Temperature Sensor Replacement Buick

### Removal Procedure

1. Remove the upper instrument panel (IP) trim pad. Refer to Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.
2. Pry up in order to remove the defroster grille.
3. Twist 1/4 turn in order to remove the sensor (2) from the defroster grill (3).

### Installation Procedure

1. Twist 1/4 turn in order to install the solar sensor (2) to the defroster grill (3).
2. Install the defroster grille into the upper trim pad.
3. Install the upper instrument panel (IP) trim pad. Refer to Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.

## Sun Load Temperature Sensor Replacement Oldsmobile

### Removal Procedure

1. Remove the upper instrument panel (IP) trim pad. Refer to Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.
2. Pry up in order to remove the defroster grille.
3. Twist 1/4 turn in order to remove the sensor (2) from the defroster grill (3).

### Installation Procedure

1. Twist 1/4 turn in order to install the solar sensor (2) to the defroster grill (3).
2. Install the defroster grille into the trim pad.
3. Install the upper instrument panel (IP) trim pad. Refer to Instrument Panel Upper Trim Pad Replacement in Instrument Panel, Gauges and Console.