For 1990-2009 cars

### Removal Procedure

1. Perform the following steps in order to remove the rear compartment courtesy lamp (1) from the rear compartment lid:

1.1. | Compress the tangs.

1.2. | Pull the lamp through the cutout.

2. Disconnect the connector (2).
3. Turn the bulb in a counterclockwise direction in order to remove the bulb from the rear compartment courtesy lamp (1).

### Installation Procedure

1. Turn the bulb in a clockwise direction in order to install the bulb to the lamp (1).
2. Connect the connector (2) to the rear compartment courtesy lamp (1).
3. Position the lamp assembly into the cutout in order to install the rear compartment courtesy lamp (1).
4. Apply pressure in order to secure the lamp.