For 1990-2009 cars

## Transmission Mount Replacement Right Mount

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Support the transmission with a jackstand.
3. Remove the nuts and bolts from the frame-to-mount.
4. Remove the through bolt from the mount.
5. Remove the bolts from the mount-to-transmission.
6. Remove the mount.

### Installation Procedure

1. Install the mount into position.
2. Install the mount-to-transmission bolts.

Tighten
Tighten the mount-to-transmission bolts to 58 N·m (42 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the through bolt and the nut.

Tighten
Tighten the mount through bolt and nut to 102 N·m (75 lb ft).

4. Install the frame-to-mount nuts and bolts.

Tighten
Tighten the frame-to-mount nuts and bolts to 72 N·m (53 lb ft).

5. Remove the jackstand.
6. Lower the vehicle.

## Transmission Mount Replacement Rear Mount

### Removal Procedure

1. Raise the vehicle. Support the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Support the transmission with a jackstand.
3. Remove the nuts from the mount to bracket.
4. Remove the transmission mount bolts.
5. Remove the transmission mount.
6. Remove the bracket bolts.
7. Remove the bracket.

### Installation Procedure

1. Install the mount.
2. Install the mount bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the bracket.
4. Install the bracket bolts.

Tighten
Tighten the bracket bolts to 75 N·m (55 lb ft).

5. Install the nuts.

Tighten
Tighten the nuts to 40 N·m (29 lb ft).

6. Remove the jackstand.
7. Lower the vehicle.