For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Perform the Instrument Cluster System Check before processing. Is the system check complete? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Turn the ignition switch to OFF.
2. Disconnect the instrument cluster connector C1
3. Measure the resistance from connector C1 terminal E9 to ground.

Does the resistance equal the specified value?

Infinite

Go to Step 4

Go to Step 3

3 |

1. Disconnect the trip odometer reset switch connector.
2. Measure the resistance from the instrument cluster connector C1 terminal E9 to ground.

Does the resistance equal the specified value?

Infinite

Go to Step 12

Go to Step 5

4 |

1. Depress the trip odometer reset switch.
2. At the same time, measure the resistance from connector C1 terminal E9 to ground.

Is the resistance less than or equal to the specified value?

5 ohms

Go to Step 7

Go to Step 6

5 | Repair the short to ground in CKT 376 (LT GRN) Is the repair complete? | -- | Go to Instrument Cluster System Check | --
6 |

1. Disconnect the trip odometer.
2. Reset the trip odometer reset switch.
3. Measure the resistance from the reset switch harness connector terminal E to ground.

Is the resistance less than or equal to the specified value?

5 ohms

Go to Step 10

Go to Step 9

7 | Inspect the instrument cluster connector C1 for proper terminal contact. Is the contact OK? | -- | Go to Step 8 | --
8 | Replace the instrument cluster. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
9 | Repair the open in CKT 351 (BLK/WHT) Is the repair complete? | -- | Go to Instrument Cluster System Check | --
10 | Measure the resistance from the trip odometer reset switch harness connector terminal G to connector C1 terminal E9 Is the resistance less than or equal to the specified value? | 5 ohms | Go to Step 12 | Go to Step 11
11 | Repair the open in CKT 376 (LT GRN). Is the repair complete? | -- | Go to Instrument Cluster System Check | --
12 | Replace the trip odometer reset switch. Is the repair complete? | -- | Go to Instrument Cluster System Check | --