For 1990-2009 cars

#### Tools Required

J 36850 Assembly Lubricant

1. Inspect the drive link assembly (507) for damaged, cracked, or binding links.
2. Use J 36850 or equivalent in order to retain the thrust washer (517) onto the drive sprocket (516).
3. Use J 36850 or equivalent in order to retain the thrust washer (508) onto the driven sprocket support.

Important: The drive link assembly must be installed correctly.

4. Assemble the drive and driven sprockets into the drive link assembly (507) according to one of the following criteria:

• | If an old drive link is being reinstalled, put the drive link assembly with the master link (different color) facing up or down, whichever way it was found during disassembly

• | If a new drive link assembly is being installed, put the drive link assembly with the master link facing upward.

5. Install the drive link assembly and the sprockets into the case by hand. A slight rocking motion may be required in order to work the sprockets into place.