For 1990-2009 cars

#### ABS/TCC Switch

Connector Part Information |

• | 12033704

• | 4-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Fused Output - IGN3
B | PPL | 420 | Brake Pedal Switch Output - TCC
C | TAN | 848 | Brake Pedal Switch Output - ABS
D | LT BLU/BLK | 853 | Brake Pedal Switch Return - ABS

#### A/C Clutch

Connector Part Information |

• | 12162017

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 59 | A/C Clutch Solenoid Feed
B | BLK | 1350 | Ground

#### A/C Pressure Sensor

Connector Part Information |

• | 12110192

• | 3-Way F Metri Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 808 | Sensor Return
B | GRY | 474 | 5 Volt Reference Feed
C | RED/BLK | 380 | A/C Refrigerant Pressure Sensor Signal

#### Boost Control Solenoid

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fused Output - IGN1
B | GRY | 1724 | Boost Control Solenoid Output

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 12162272

• | 3-Way F Metri-Pack 150.1 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 633 | Camshaft Position Sensor Signal
B | BLK/WHT | 836 | Crankshaft Position Sensor Return #2
C | WHT/BLK | 644 | Reference Voltage Feed - 10 Volt Ref

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12162724

• | 4-Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU/WHT | 1800 | Crankshaft Position Sensor Signal #2
B | YEL | 573 | Crankshaft Position Sensor Signal
C | BLK/WHT | 836 | Crankshaft Position Sensor Return #2
D | WHT/BLK | 644 | Reference Voltage Feed - 10 Volt Ref

#### Cruise Control Module

Connector Part Information |

• | 12065425

• | 10-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 397 | Cruise Control ON Switch Output
B | DK BLU | 84 | Cruise Control Set/Coast Switch Signal
C | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal
D | PPL | 420 | Brake Pedal Switch Signal - TCC
E | BLK | 1350 | Ground
F | BRN | 341 | Fused Output - IGN3
G | WHT | 17 | Stoplamp Switch Signal
H | DK GRN | 83 | Cruise Control Signal - Disengage
J | LT BLU/BLK | 396 | Cruise Control Signal - Engaged
K | DK GRN/WHT | 817 | Vehicle Speed Signal

#### Data Link Connector (DLC)

Connector Part Information |

• | 12110250

• | 16-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | ORN/BLK | 1061 | Serial Data Line - UART
2 | PPL | 1807 | Serial Data Line - Class 2
3 | - | - | Not Used
4 | BLK | 150 | Ground
5 | BLK/WHT | 451 | Ground
6-7 | - | - | Not Used
8 | BLK | 1455 | Keyless Entry Program Enable Signal
9 | TAN | 800 | Serial Data Line - UART
10 | - | - | Not Used
11 | WHT | 345 | Magnetic Steering Variable Assist Motor Feed - Low Effort
12- 13 | - | - | Not Used
14 | DK GRN | 835 | Serial Data Line - Entertainment and Comfort (E&C)
15 | - | - | Not Used
16 | ORN | 40 | Fused Output - Battery

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12162225

• | 3-Way F Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 470 | Sensor Return
B | YEL | 410 | Coolant Temperature Sensor Signal
C | LT GRN | 36 | Coolant Temperature Signal

#### Engine Oil Level Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1174 | Oil Level Switch Signal
B | BLK | 451 | Ground

#### Evaporative Emissions (EVAP) Canister Purge Valve

Connector Part Information |

• | 12124037

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fused Output - IGN1
B | DK GRN/WHT | 428 | EVAP Purge Valve Output

#### Evaporative Emissions (EVAP) Canister Vent Valve

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series, Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Fused Output - Ignition
B | WHT | 1310 | Canister Vent Valve Solenoid Output

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | 12186057

• | 5-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 435 | EGR Valve Control
B | BLK | 552 | EGR Pintle Position Sensor Ground
C | BRN | 1456 | EGR Pintle Position Signal
D | GRY | 605 | Reference Voltage Feed - 5 Volt Reference A
E | WHT | 257 | EGR Valve Control

#### Fuel Injectors

Connector Part Information |

• | 12129140

• | 2-Way F Metri-Pack 280.1 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1039 | Fuse Output - IGN1
B | BLK | 1744 | Fuel Injector #1 Output
B | LT GRN/BLK | 1745 | Fuel Injector #2 Output
B | PNK/BLK | 1746 | Fuel Injector #3 Output
B | LT BLU/BLK | 844 | Fuel Injector #4 Output
B | BLK/WHT | 845 | Fuel Injector #5 Output
B | YEL/BLK | 846 | Fuel Injector #6 Output

#### Fuel Pump Control Module

1050
Connector Part Information |

• | 12105451

• | 8-Way M Non-Packard (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | - | - | Not Used
4 | BLK | 1050 | Ground
5 | PNK | 1580 | Fuel Pump Motor Return
6 | GRY | 120 | Fuel Pump Motor Feed
7 | BRN | 437 | Fuel Pump PWM Control
8 | LT GRN | 1058 | Fuel Pump Relay Output

#### Fuel Tank In-Line Connector C420

Connector Part Information |

• | 12059471

• | 7-Way F Metri-Pack Mixed Series, Sealed (BLK)

Connector Part Information

• | 12052200

• | 7-Way M Metri-Pack Mixed Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | PPL | 30 | Fuel Gauge Sensor Signal | A | PPL | 30 | Fuel Gauge Sensor Signal
B | GRY | 605 | Reference Voltage Feed - 5 Volt Reference A | B | GRY | 605 | Reference Voltage Feed - 5 Volt Reference A
C | BLK | 808 | Fuel Tank Pressure Sensor Ground | C | BLK | 808 | Fuel Tank Pressure Sensor Ground
D | BLK/WHT | 651 | Fuel Gauge Sensor Ground | D | BLK/WHT | 651 | Fuel Gauge Sensor Ground
E | GRY | 120 | Fuel Pump Motor Feed | E | GRY | 120 | Fuel Pump Motor Feed
F | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | F | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
G | BLK | 1580 | Fuel Pump Motor Return | G | BLK | 1580 | Fuel Pump Motor Return

#### Fuel Tank Pressure Sensor

Connector Part Information |

• | 12059596

• | 3-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 808 | Fuel Tank Pressure Sensor Ground
B | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
C | GRY | 605 | Reference Voltage Feed - 5 Volt Reference A

#### Fuel Tank Unit

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 30 | Fuel Gage Sensor SIgnal
B | GRY | 120 | Fuel Pump Motor Feed
C | BLK | 850 | Ground
D | BLK/WHT | 651 | Ground

#### Heated Oxygen Sensor 1 (HO2S 1)

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | Heated Oxygen Sensor Sensor 1 (HO2S 1) Low
B | PPL | 412 | Heated Oxygen Sensor Sensor 1 (HO2S 1) Signal
C | BLK | 1350 | Ground
D | PNK | 639 | Fused Output - IGN1

#### Heated Oxygen Sensor 2 (HO2S 2)

Connector Part Information |

• | 12160825

• | 4-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | Heated Oxygen Sensor Sensor 2 (HO2S 2) Low
B | PPL/WHT | 1668 | Heated Oxygen Sensor Sensor 2 (HO2S 2) Signal
C | BLK | 1350 | Ground
D | PNK | 639 | Fused Output - IGN1

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 12162187

• | 4-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | IAC Coil B High
B | LT GRN/WHT | 1749 | IAC Coil B Low
C | LT BLU/BLK | 1748 | IAC Coil A High
D | LT BLU/WHT | 1747 | IAC Coil A Low

#### Ignition Control Module

Connector Part Information |

• | 12124379

• | 14-Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 423 | Ignition Control Signal
B | TAN/BLK | 424 | Bypass Signal
C | LT BLU/BLK | 647 | 18x Reference Signal
D | PPL/WHT | 430 | 3x Reference Signal
E | WHT | 121 | Tachometer Signal (Not Used)
F | BLK | 630 | Camshaft Position (CMP) Signal Output
G | YEL | 573 | Crankshaft Position (CKP) 18x Signal
H | LT BLU/WHT | 1800 | CKP Sync Signal
J | BRN/WHT | 633 | CMP Sensor Signal
K | BLK/WHT | 451 | Ground
L | RED/BLK | 453 | Reference Low Signal
M | BLK/WHT | 836 | CMP/CKP Sensor Ground
N | WHT/BLK | 644 | Reference Voltage Feed - 10 Volt Reference
P | PNK | 239 | Fuse Output - IGN1

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162196

• | 2-Way F Metri-Pack 150.2 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/BLK | 645 | IAT Sensor Ground
B | TAN | 472 | IAT Sensor Signal

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12103771

• | 3-Way M Weather Pack (WHT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | MAP Sensor Return
B | LT GRN | 432 | MAP Sensor Signal
C | GRY | 605 | Reference Voltage Feed - 5 Volt Ref

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 492 | MAF Sensor Signal
B | BLK/WHT | 451 | Ground
C | PNK | 439 | Fused Output - IGN1

#### Park/Neutral Position (PNP) Switch Connector C1

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 434 | Park/Neutral Position Switch Signal
B | PNK | 139 | Fuse Output - IGN1
C | LT GRN | 275 | Park/Neutral Position Switch Output - Park
D | BLK/WHT` | 451 | Ground
E | YEL/BLK | 625 | Theft System Starter Enable Relay Output - Coil
F | LT GRN | 24 | Backup-Up Lamp Feed
G | YEL | 575 | Theft System Starter Enable Relay Output

#### Park/Neutral Position (PNP) Switch Connector C2

Connector Part Information |

• | 12191757

• | 4-Way F Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 776 | Transaxle Range Switch Signal - Parity Bit
B | YEL | 772 | Transaxle Range Switch Signal - Bit 2
C | GRY | 773 | Transaxle Range Switch Signal - Bit 3
D | BLK/WHT | 771 | Transaxle Range Switch Signal - Bit 1

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12110294

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 452 | Sensor Return
B | DK BLU | 417 | Throttle Position Sensor Signal
C | GRY | 605 | 5 Volt Reference

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 12162192

• | 2-Way F Metri-Pack 150.2 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | Vehicle Speed Sensor Low
B | YEL | 400 | Vehicle Speed Sensor High