For 1990-2009 cars

# Technical Service Bulletins

- 2008-06-04: No Movement When Transmission is Shifted to Drive or Third - Normal Operation When Shifted to Second, First or Reverse (Replace Forward Sprag Assembly) (08-07-30-027)
- 2007-12-05: 60 Degree V6 Engine Oil Leak at Crankshaft Front Oil Seal (Use New Crankshaft Front Oil Seal Installer Tool EN-48869) (07-06-01-023)
- 2007-10-02: Engine Oil Leak at Crankshaft Rear Main Oil Seal (Install Revised Crankshaft Rear Main Oil Seal Using Revised Rear Main Seal Installer and Remover Tools) (05-06-01-019F)
- 2006-01-27: Service VME - Use Correct Engine Oil Drain Plug - keywords drain engine leak oil pan plug replace (PIP3696)
- 2006-01-18: Info - New Product Feedback Form and Process for Automatic Transmission Core Returns (01-07-30-029A)
- 2004-03-18: No TCC Apply , MIL On , TCC Surge , Possible P0740 , P1870 , or 39 after Installation of Reman ( SRTA ) 4T60 / 4T60E - kw case cover converter slip transmission (PI01880A)
- 2001-04-06: Info - Current CIPS Campaign Number to Previous DIvisional Campaign Number (01-00-89-008)
- 2001-03-02: Info - February, 2001 Bulletin Summary (01-00-89-006)
- 1999-12-23: Info - Dealer Installed Rear Seat Lap/Shoulder Belt Kits (99-09-40-006)
- 1999-07-23: Info - Vehicles Equipped with a Webasto Sunroof System (99-08-67-003)
- 1998-06-03: INFO - NEW TOOL J-42958, REV. CHARTS AND SCHEM. FOR CRUISE (83-90-08)
- 1998-03-13: INFO ON AVAILABILITY OF REPAIRS TO CRT (80-83-07)
- 1998-03-10: INFO. NEW TOOL J-41450-B RELEASED FOR CS GEN DIAG. (83-64-09)
- 1998-01-12: INFO. FRONT. SUPP. INFLAT. RESTRAINTS (SIR) ON-OFF SWITCH (73-90-23)
- 1997-12-11: WARRANTY ADMIN - ACDELCO REMANUFACTURED ENGINES (72-05-07)
- 1997-11-20: CLARIFICATION OF RAIL DUST REM (A5575-A5580) (72-05-11)
- 1997-11-01: WARRANTY ADMIN. - LABOR OPERATION CODE Z1241 (62-05-02A)
- 1997-09-01: INFO. ON ALUMINUM HEATER CORE AND/OR RADIATOR REPL. (73-62-13A)
- 1997-05-29: INFO ON AUTO TRANS OIL COOLER FLUSHING &FLOW CHECK PROC. (77-71-59)
- 1997-05-12: INFORMATION -TWO PART URETHANE ADHESIVE (73-10-54)
- 1997-04-17: INFO. ON A/C TOOL AND EQUIPMENT MAINTENANCE (63-12-08A)
- 1997-02-07: SERVICE ISSUES FOR VEHICLES WITH R12 OR R134A A/C SYSTEMS (73-12-04)
- 1997-01-31: INFO. NEW BODY SEALER TAPE FOR COLLISION REPAIRS (73-10-49)
- 1997-01-13: INFO. ON COMPACT DISC PLAYERS- PROCEDURES (64-96-01)
- 1997-01-01: GUIDELINES FOR RETROFITTING R-12 VEH. TO R-134A (43-12-07E)
- 1996-12-01: SERVICE ADMINISTRATION - WARRANTY CLAIMS PROCESSING (31-05-03C)
- 1996-11-15: INFO. REFERENCE CHART FOR A/C COMPRESSOR SEAL WASHERS (63-12-15)
- 1996-10-15: INFO. ON THE GENERAL MOTORS KEY CODE VOICE RESPONSE SYSTEM (61-01-11)
- 1996-10-01: PROCEDURE TO HANDLE CUSTOMER RADIO CONCERNS (68-96-01A)
- 1996-09-01: ACDELCO SERVICE CENTER LOC. FOR ODOMETER/SPEEDOMETER (66-83-04A)
- 1996-06-05: WARRANTY ADMIN. - GOODWRENCH SERVICE PLUS LIFETIME SERVICE (68-05-03)
- 1996-05-10: INFO. ON SERVICE ISSUES FOR VEHICLES WITH R12 OR R134A (63-12-09)
- 1996-05-07: INFORMATION ON CAMPAIGN SYSTEM COMMONIZATION (62-07-01)
- 1996-05-06: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (63-65-32)
- 1996-05-01: AC DELCO LOCATOR SVCS FOR DELCO ELECTRONICS EXCHANGE (58-83-02B)
- 1996-05-01: WARRANTY ADMINISTRATION TIRE REPLACEMENTS (60-05-01A)
- 1996-04-15: INFO. ON HEADLAMP LENS DISTORTION (63-81-11)
- 1996-02-02: INFORMATION ON UPDATED BATTERY REPLACEMENT CATALOG NUMBERS (63-64-01)
- 1996-01-04: TECHNICAL ASSISTANCE PRE-CALL WORKSHEET (51-01-07)
- 1995-12-01: NEW PROCEDURE FOR ORDERING SERVICE REPL. EE PROMS (34-02-02)
- 1995-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE (53-65-07)
- 1995-10-10: WARRANTY INFORMATION ALL MODELS - ALL YEARS (58-05-03)
- 1995-10-09: INFO. ON DAYTIME RUNNING LAMPS (DRL) (53-82-09)
- 1995-09-01: WARRANTY INFORMATION - LABOR TIME SUBMISSION FORMAT (58-05-01A)
- 1995-09-01: REPLACEMENT OF ISOLATION DIODES (93-8-20)
- 1995-08-10: REVISED TECH 1 MASS STORAGE CARTRIDGE (MSC) OXYGEN SENSOR (51-65-47)
- 1995-06-12: INFO. ON REFORMULATED GASOLINE (RFG) (57-01-02)
- 1995-06-01: CAMPAIGN: SERVICE PART FUEL TANK SENDER RING WELDS (91-C-51)
- 1995-05-23: WARRANTY ADMINISTRATION WARRANTY INFORMATION (57-05-02)
- 1995-05-15: INFORMATION ON CONTAMINATED R12 REFRIGERANT TESTING (53-12-05)
- 1995-04-27: INFORMATION ON GM CAMPAIGN IDENTIFICATION LABEL (51-01-03)
- 1995-04-01: INFORMATION ON SIERRA-BRAND ENGINE COOLANT (43-62-01B)
- 1995-03-28: WARRANTY ADMINISTRATION DEALER/RETAILER ADMINISTRATION (57-05-01)
- 1995-03-01: SMU - SECTION 0 - GENERAL INFORMATION (57-02-01)
- 1995-02-21: SMU - SECTION 6A - REVISED BALANCE SHAFT (57-61-07)
- 1995-02-03: SMU - INFO. ON INSPECTION/ MAINTENANCE (I/M) EMISSIONS (51-65-02)
- 1995-01-11: ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-10)
- 1994-12-01: WEBESTO SUNROOF REPAIRS (81-15-26)
- 1994-11-29: INFO. ON ENHANCED EMISSION INSPECTION MAINTENANCE PROGRAM (43-65-07)
- 1994-11-23: FRONT BRAKE PULSATION - 'NEW' DIAGNOSIS (43-50-09)
- 1994-10-25: REV. TO ADHESIVE CAULKING KIT, NEW PRIMERS & PART NUMBERS (43-10-48)
- 1994-09-15: DLR. PRODUCT CAMPAIGN BULLETIN NUMBERING SYSTEM (41-01-03)
- 1994-09-12: INFO. ON NEW PROM/MEMCAL IDENTIFICATION MARKINGS (44-65-01)
- 1994-09-08: CONTAMINATED A/C REFRIGERANT (INFORMATIONAL) (43-12-23)
- 1994-09-01: INFORMATION ANNOUNCING THE NEW CORPORATE BULLETIN (33-01-05A)
- 1994-08-16: OBTAINING TECHNICAL ASSISTANCE (I/M 240 REPAIRS) (43-65-06)
- 1994-08-03: WARRANTY ADMINISTRATION-NEW WARRANTY CLAIM PROCESSING SYS. (41-05-02)
- 1994-07-18: INFORMATION ON RELEASE OF SERVICE PKG. FOR NICKEL TAPE (14-93-01)
- 1994-06-30: INFORMATION ON J39400 A/C LEAK DETECTOR MAINTENANCE KIT (43-12-18A)
- 1994-06-20: INFORMATION ON SPEED RATED TIRES (43-35-02)
- 1994-06-08: WARRANTY ADMINISTRATION - NEW LABOR OPERATION NUMBER (42-05-06)
- 1994-05-13: WARRANTY ADMINISTRATION - EMISSION WARR. PARTS COVERAGE (47-05-01)
- 1994-05-01: INFO. ON VEHICLES EQUIPPED WITH A WEBASTO SUNROOF (43-10-18A)
- 1994-04-08: REDUCED PWR STEERING ASSIST AT LOW AMBIENT TEMPERATURES (03-32-06)
- 1994-03-29: ENHANCED INSPECTION MAINTENANCE PROGRAMS (43-65-05)
- 1994-02-15: INFORMATION ON TRANSAXLE OIL FILTER DIFFERENCES (47-71-03)
- 1994-02-01: INFORMATION ON AFTER MARKET ANTI-LOCK BRAKE SYS. PRODUCTS (43-50-01)
- 1993-12-22: RETROFITTING R-12 VEHICLES TO R-134A (INFORMATIONAL) (33-12-26)
- 1993-10-22: CLEARCOAT DEGRADATION-CHALKING & WHITENING (REPAIR PROCEDURE) (33-17-08)
- 1993-08-30: BCM EPROM CALIBRATIONS SUMMARY OF SERVICE EPROMS (93-8C-130)
- 1993-08-26: INTERMIT. PULL W/O HARD BRAKE APPLY DURING NON-ABS STOP (31-50-04)
- 1993-08-01: TIRES SLIPPING ON WHEELS USE PROPER TIRE MOUNTING PROC (93-3-6)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-3-10)
- 1993-08-01: TIRES SLIPPING ON WHEELS USE PROPER TIRE MOUNTING PROC (93-3E-103)
- 1993-08-01: INFO. ON COSMETIC DAMAGE TO ALUMINUM WHEELS DURING BALANC. (93-3E-104)
- 1993-07-08: SERVICE MANUAL UPDATE-SEC 3F5A (SIR) TILT COLUMN UNIT REPAIR (93-3-15)
- 1993-07-08: SERVICE MANUAL UPDATE-SEC 3F5A (SIR) TILT COLUMN UNIT REPAIR (93-3B-602)
- 1993-07-01: LEAKING CAST ALUMINUM WHEELS (REPAIR WITH ADHESIVE SEALANT) (93-3-14)
- 1993-06-15: AIR CONDITIONING COMPRESSOR REPLACEMENT (NEW PROCEDURE) (93-1B-124)
- 1993-05-25: RECYCLING OF USED OIL FILTERS (INFORMATIONAL) (93-0-6)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7-1)
- 1993-05-19: INFO. ON SERVICING VEHICLE WITH CONTAMINATED TRANS. FLUID (93-7A-142)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1-9)
- 1993-05-06: A/C R-134A REFRIGERANT (INFORMATION) (93-1B-126)
- 1993-05-01: RETURN OF UNDEPLOYED (SIR) INFLATOR MODULES (92-9-3)
- 1993-04-30: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (93-10-194)
- 1993-04-05: CRANK (OR NO CRANK) AND NO START AND/OR NO START (31-81-13)
- 1993-03-16: ILLUSTRATED STEERING SYSTEM BLEED PROCEDURE (38-30-01A)
- 1993-02-15: INTERMITTENT CODES E047,B333 B334,B335,B336 AND/OR B337 (93-8A-110)
- 1993-01-30: SERVICE PROCEDURE - CODE E39 VISCOUS CONVERTER CLUTCH DIAG. (93-7A-117)
- 1993-01-27: INFO. ON FACTORS THAT AFFECT FUEL ECONOMY (30-65-02)
- 1992-12-15: INOPERATIVE POWER MODULE REPLACEMENT (CHECK PROCEDURE) (93-1B-105)
- 1992-12-01: ENG. MISS, HESITATION & ROUGH PIERCED SECONDARY IGNITION (93-6D-102)
- 1992-11-30: IMPROPER AIR DELIVERY FROM ECC (SERVICE INFORMATION/PROC.) (93-1A-101)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (92-6E-23)
- 1992-11-30: SERVICE GUILD: INFO. ON THE EFFECT OF FUEL VOLATILITY (93-6C-100)
- 1992-11-30: ALTERNATE REFRIGERANTS INFORMATION (93-1B-102)
- 1992-11-14: DECEL STALL/CRANK ON START UP (NEW IAC MOTOR) (93-6E-102)
- 1992-11-14: TRANS. CONTROL LEVER SHIFTERS EFFORT (REPLACE LEVER) (93-7A-107)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-7)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (92-2-128)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-179)
- 1992-11-01: INDUSTRIAL FALLOUT-PAINT DAM. FINESSE TYPE REPAIRS (93-10-148)
- 1992-10-31: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1D-100)
- 1992-10-01: DECEL STALL/CRANK ON START UP - NEW IAC MOTOR (93-6E-3)
- 1992-08-03: ALTERNATE REFRIGERANTS INFORMATION (92-1-16)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-17)
- 1992-06-16: SERVICE GUILD: INFO ON AVOID DAMAGE TO TIRE WHEELS (92-3-123)
- 1992-05-31: BRAKE PULSATION SERVICE INFORMATION (88-5-121)
- 1992-05-27: A/C LEAK (DIAGNOSIS BULLETIN) ALL MODELS 1992 AND PRIOR (92-1-13)
- 1992-04-30: PWR. STEERING PUMP NOISE OR INCREASED STEERING EFFORT (90-3-142)
- 1992-04-01: PROM I.D. NOT RECOGNIZED BY THE T-100 (GM CAMS) TERMINAL (23-65-08)
- 1992-03-25: TECH-1 GM 88-92 BRAKE CARTRIDGE EXCHANGE PROGRAM (92-1-12)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-12)
- 1992-03-24: INFO ON COATED WHEEL WEIGHTS USED FOR ALUMINUM WHEELS (92-3-121)
- 1992-03-02: ENG. OIL LEAK - REAR MAIN SEAL (NEW REAR MAIN SEAL RELEASED) (92-6-8)
- 1992-03-02: ENG. OIL LEAK - REAR MAIN SEAL (NEW REAR MAIN SEAL RELEASED) (92-638-104)
- 1992-02-21: HUB ASSY. SEAL SQUEAK/SQUAWK NOISE (LUBE SEAL & HUB ASSY.) (91-3-21)
- 1992-02-21: HUB ASSY. SEAL SQUEAK/SQUAWK NOISE (LUBE SEAL & HUB ASSY.) (91-3-138)
- 1992-02-05: CRUISE CONTROL DROPOUT (FAILS TO SET OR RESUME) (92-9-9)
- 1992-02-05: CRUISE CONTROL DROPOUT (FAILS TO SET OR RESUME) (92-8-140)
- 1992-01-31: A/C R-12 CHARGING CAPACITY (CHART) (92-1-109)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-74T60-5)
- 1992-01-23: SERVICE REPLACEMENT TRANSAXLE (SRTA MODEL UPDATE 4T60-4T60E) (92-74T60-104)
- 1992-01-09: SIR SENSOR REPLACE POLICY REV. ALL 1988-92 CARS WITH SIR (92-9-8)
- 1992-01-09: SIR SENSOR REPLACE POLICY REV. ALL 1988-92 CARS WITH SIR (92-8-127)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-74T60-4)
- 1991-12-18: NEW BOTTOM PAN/CONTROLLED COMP PAN GASKET AND SERVICE INFO. (92-74T60-103)
- 1991-11-30: ENGINE OIL ECONOMY (INFORMATIONAL BULLETIN) (93-6A-124)
- 1991-11-15: A/C R-12 CHARGING CAPACITY CADILLAC CHARGING TABLE (92-8-112)
- 1991-11-06: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (92-10-20)
- 1991-11-06: BINDING/STICKING LOCK CYLINDER RECOMMENDED LUBRICATIONS (92-2-141)
- 1991-10-15: A/C COMPRESSOR SHAFT NUT REMOVAL (IMPROVED QUALITY) (93-1-2)
- 1991-10-11: A/C COMPRESSOR SEALING WASHER USAGE (NEW DESIGN) (92-1-3)
- 1991-10-11: A/C COMPRESSOR SEALING WASHER USAGE (NEW DESIGN) (92-1-103)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7-2)
- 1991-10-02: DEXRON IIE A/T FLUID PREFERRED (GENERAL INFORMATION) (92-7-100)
- 1991-09-30: 3-4 CLUTCH/2-4 BAND SERVICE INFORMATION/SERVICE PROCEDURES (91-7-113)
- 1991-09-10: CAUTIONS REGARDING SIR SYSTEM REPAIRS AND PROCEDURES (92-10-7)
- 1991-09-10: CAUTIONS REGARDING SIR SYSTEM REPAIRS AND PROCEDURES (92-8-106)
- 1991-08-28: SERVICE GUILD: ENGINE OIL LEAK AT REAR MAIN SEAL (90-6-14)
- 1991-08-28: SERVICE GUILD: ENGINE OIL LEAK AT REAR MAIN SEAL (90-6-119)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-4T60-3)
- 1991-08-23: NEW END PLAY SPEC. 4T60/4T60-E (INPUT CARRIER PINION GEAR) (92-74T60-100)
- 1991-08-15: CODE F41 COOLING FAN FAULT CODE B441 COOLING LT. MESSAGE (89-8-244)
- 1991-08-15: ANTI-LOCK BRAKE PEDAL SQUEAK (INSTALL NEW SHIM) (90-5-132)
- 1991-08-15: FLASHING TELLTALES/IPC DISPLAY WITH IGNITION OFF (NEW PART) (91-8-232)
- 1991-08-13: PROPER PROC. FOR PROBING WIRES (NEW TEST PROBES AVAILABLE) (91-8-33)
- 1991-08-09: CELLULAR TELEPHONE PROGRAM (DELCO ELECT.) NEW INFORMATION (92-9-4)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-3)
- 1991-08-08: SERVICE GUILD: EVALUATING PEENED SPACER PLATE (91-7-115)
- 1991-08-06: OIL PRESSURE GAGE ERRATIC (REPLACE OIL PRESS. SENSOR) (90-6D-6)
- 1991-08-06: OIL PRESSURE GAGE ERRATIC (REPLACE OIL PRESS. SENSOR) (92-8-103)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (92-6E-3)
- 1991-07-24: DAMAGED ECM/PCM MIS-DIAGNOSIS INCORRECT 'TAP-TESTING' (91-6-121)
- 1991-07-15: UNWANTED BLOWER OPERATION OR IMPROPER AIR DELIVERY ECC (91-1-138)
- 1991-06-29: REVISED OIL PAN GASKET CONTAINS CIRCULAR SPACERS (90-645-119)
- 1991-06-20: DISPOSAL OF LIVE (UNDEPLOYED) SIR INFLATOR MODULES (92-9-2)
- 1991-06-13: RETAINING MEMORIES IN ELECT. DEVICES WITH BAT. DISCONNECTED (91-8-212)
- 1991-05-15: BINDING OR INOP REVERSE STUCK 3-4 SEQ. VALVE 2-3 SHIFT (91-74L60-104)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISSING ACCESS CAPS (91-1-4)
- 1991-04-30: A/C REFRIGERANT LOSS DUE TO LOOSE/MISS. ACCESS FITTING CAP (91-1-123)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6E-18)
- 1991-04-19: DAMAGE TO ECM/PCM CIRCUIT BOARD WHEN INSTALLING MEM-CAL (91-6-117)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-0-5)
- 1991-04-15: LOW OIL LEVEL MESSAGE OPERATION-NEW SENSOR RELEASED (91-8-183)
- 1991-04-15: CLEANING OF UPPER I/P SURFACES CLEANING PROCEDURES (91-2-197)
- 1991-02-28: SER. REPLACEMENT VALVE SPRING AND CAP ASSY. RELEASED (91-633-101)
- 1991-02-28: TIRE DAMAGE CAUSED IN GM ASSY. PLANTS-REPLACEMENT PROCEDURES (91-3-115)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-6D-5)
- 1991-02-15: INFO ON MULTEC FUEL INJECTORS DO NOT CLEAN MULTEC INJECTORS (91-6-111)
- 1991-02-15: NO START/VEHICLE BATTERY DEAD PARASITIC CURRENT DRAIN TEST (91-8-172)
- 1991-02-01: INFO ON ABS NOISE - SELF TEST NORMAL AFTER IGNITION CYCLE (91-5-5)
- 1991-02-01: INFO ON ABS NOISE - SELF TEST NORMAL AFTER IGNITION CYCLE (91-5-117)
- 1991-01-15: WATER LEAK/WIND NOISE AT TOP OF STATIONARY VENT GLASS (90-10-39)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6 NEW ROD BEARING CLEARANCE (91-633-103)
- 1991-01-15: SERVICE MAN. UPDATE SEC. 6 NEW ROD BEARING CLEARANCE (91-638-104)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-73T40-101)
- 1991-01-15: GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE (91-74T60105)
- 1991-01-02: NEW TWILIGHT SENTINEL MODULE SERVICE PART AND INFO (89-8-33)
- 1991-01-02: SERVICE MANUAL UPDATE SEC.8D1 ECM TROUBLE CODE DIAGNOSIS (90-8-22)
- 1991-01-02: SERVICE MANUAL UPDATE SEC.8D1 ECM TROUBLE CODE DIAGNOSIS (90-638-111)
- 1991-01-02: NEW TWILIGHT SENTINEL MODULE SERVICE PART AND INFO (91-8-146)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-0-4)
- 1990-12-31: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (90-74T60123)
- 1990-12-31: CHATTERING WIPER BLADES OR WIPEABILITY (91-2-123)
- 1990-12-31: BRAKE EFFECTIVENESS AFTER ROTOR REFINISHING (91-5-109)
- 1990-12-15: NEW PLATES-4TH CLUTCH REACTION FORWARD CLUTCH/LOW & REV. (90-74T60-122)
- 1990-12-15: GRINDING OR GROWLING NOISE IN PARK ON INCLINE (90-74T60121)
- 1990-12-15: BCM EPROM CALIBRATIONS(SUMMARYOF SERVICE EPROM'S) (90-8-241)
- 1990-12-10: CLUTCH PLATE IDENTIFIERS FOR 3RD CLUTCH PLATE (91-74T60-7)
- 1990-12-10: CLUTCH PLATE IDENTIFIERS FOR 3RD CLUTCH PLATE (91-74T60-116)
- 1990-11-30: NO REVERSE/SLIPPING IN REVERSE REPEAT REVERSE BAND DISTRESS (90-74T60-120)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-74T60-8)
- 1990-11-27: NEW THERMO ELEMENT & PIN HEIGHT SETTING PROCEDURE (91-74T60-114)
- 1990-11-21: LOW OIL LEVEL MESSAGE OPERATION/DIAG. & NEW PART (90-8-13)
- 1990-11-15: LOW OIL LEVEL MESSAGE NORMAL OPERATION (91-6D-2)
- 1990-11-15: LOW OIL LEVEL MESSAGE NORMAL OPERATION (91-8-134)
- 1990-11-14: SERVICE MANUAL UPDATE SEC. 6 NEW BEARING CLEARANCE (91-6-4)
- 1990-11-14: SERVICE MANUAL UPDATE SEC. 6 NEW BEARING CLEARANCE (91-630-101)
- 1990-10-15: CODE B446, B447 & B448 DIAG. REPLACE WITH REVISED PROM (90-1-133)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-74T60-15)
- 1990-10-09: DRIVE LINK NOISE-IN PARK/ NEUTRAL (91-74T60-108)
- 1990-10-08: INFO/RECOMMENDED FUELS FOR NON-TURBO PFI ENGINES (91-6E-3)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-7440-5)
- 1990-10-08: INFO/RECOMMENDED FUELS FOR NON-TURBO PFI ENGINES (91-6-103)
- 1990-10-08: NO 3RD GEAR AND/OR NO DRIVE OR REVERSE (91-74T60-109)
- 1990-09-21: AIR AND/OR WATER LEAK AT TOP OF DOOR GLASS TO VENT GLASS (91-10-7)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-7-1)
- 1990-09-21: AIR AND/OR WATER LEAK AT TOP OF DOOR GLASS TO VENT GLASS (91-2-112)
- 1990-09-21: NEW FORWARD CLUTCH LO & REV. WAVED PLATES (91-74T60-106)
- 1990-09-11: NO REVERSE/SLIPPING IN REVERSE REPEAT REVERSE BAND DISTRESS (91-7440-3)
- 1990-09-11: NO REVERSE/SLIPPING IN REVERSE REPEAT REVERSE BAND DISTRESS (91-74T60-104)
- 1990-08-31: BELT CHIRP OR SQUEAL SERVICE PROCEDURE (90-638-106)
- 1990-08-15: STATE EMISSIONS TESTING INFORMATION / PROCEDURE (91-6E-2)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-74T60-13)
- 1990-08-14: NEW 1-2 & REVERSE BANDS 440-T4 F7/NO SELECTIVE BAND APPLY PIN (91-74T60-101)
- 1990-08-02: NEW WARRANTY CLAIM FAILURE CODES (90-0-10)
- 1990-07-26: REAR COMPARTMENT ACCESS DOOR RATTLE/NEW LATCH PIN (89-10-36)
- 1990-07-26: RELEASE OF ANTENNA BEZEL NUT-1991 ESSENTIAL TOOL (91-9-3)
- 1990-07-26: REAR COMPARTMENT ACCESS DOOR RATTLE/NEW LATCH PIN (89-2-221)
- 1990-07-24: BRAKE EFFECTIVENESS CHANGE AFTER ROTOR & BRAKE PAD WORK (90-5-12)
- 1990-07-13: WATER LEAK AND/OR WIND NOISE TOP OF STATIONARY VENT GLASS (90-2-208)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (91-3-1)
- 1990-06-29: COATED WHEEL WEIGHTS FOR ALUMINUM WHEELS (90-3-127)
- 1990-06-28: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (90-6-7)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-10)
- 1990-06-22: BRAKE ROTOR REFINISH PARTS ORDERING INFORMATION (90-5-118)
- 1990-06-15: FLOOR PAN OIL CANNING INSTALL BETA BRACE MATERIAL (90-10-30)
- 1990-06-15: FLOOR PAN OIL CANNING INSTALL BETA BRACE MATERIAL (90-2-203)
- 1990-06-08: RATTLE TYPE NOISE FROM REAR OF ENGINE - NEW DAMPENER P/N (90-6-6)
- 1990-06-08: RATTLE TYPE NOISE FROM REAR OF ENGINE - NEW DAMPENER P/N (90-638-105)
- 1990-05-02: SERVICE REPLACEMENT TRANS. (SRTA) ASSEMBLY MODEL UPDATE (90-7440-117)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-7440-12)
- 1990-04-30: HARSH ENGAGE, DOUBLE BUMP OR SHUDDER-PARK/NEUTRAL-REVERSE (90-7440-119)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-7440-11)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (91-9-1)
- 1990-04-11: DISTRESSED SECOND CLUTCH 440-T4/4T60 DIAGNOSIS (90-7440-114)
- 1990-04-11: INSTALLATION GUIDELINES FOR AFTERMARKET ACCESSORIES (90-8-184)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (91-6B-1)
- 1990-04-06: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE TESTING (90-6-107)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-6D-2)
- 1990-03-21: PARASITIC DRAIN ON BATTERY AMMETER CONNECTING PROCEDURE (90-8-170)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-7440-8)
- 1990-03-16: NEW 1-2 BAND ASSY. DOES NOT REQUIRE 1-2 BAND STOP (90-7440-112)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6E-15)
- 1990-03-15: MANUAL UPDATE-SEC. 6E1/6E2/6E3 CODE 33,34,63,64 (NON-TURBOS) (90-6-105)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-7440-9)
- 1990-02-15: INTERMITTENT DELAYED UPSHIFTS HOT OR COLD/PARTS AVAILABLE (90-7440-111)
- 1990-02-14: ENG. WON'T STAY RUNNING MAY HAVE FUEL PRESS. LOSS (89-6E-25)
- 1990-02-14: ENG. WON'T STAY RUNNING MAY HAVE FUEL PRESS. LOSS (89-638-107)
- 1990-02-13: A/C R-12 SERVICE PROCEDURES CHARGING CAPACITY CHART (90-1-119)
- 1990-01-09: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (90-7440-7A)
- 1990-01-09: HARSH SHIFT CONDITIONS AND ON CAR SERVICE INFORMATION (90-7440-109)
- 1989-11-09: BATTERY INTERMITTENTLY GOES DEAD/REPAIR PROCEDURE (88-6D-7)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-10-9)
- 1989-11-09: BATTERY INTERMITTENTLY GOES DEAD/REPAIR PROCEDURE (89-8-226)
- 1989-11-09: LOOSE CARPET ON SIDE WALL TRIM PADS (REPAIR PROCEDURE) (90-2-114)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7-3A)
- 1989-11-01: REVISED DRIVE LINK WEAR SPECIFICATION 125C - 440T4 (90-7440-104)
- 1989-10-19: SLOW AIR LEAKS AT TIRE WHEEL WEIGHTS (PROCEDURE/NEW PART) (90-3-4)
- 1989-10-19: SLOW AIR LEAKS AT TIRE WHEEL WEIGHTS (PROCEDURE/NEW PART) (90-3-106)
- 1989-10-10: THEFT PREVENTION STANDARDS ANTI-THEFT LABELING (90-0-2)
- 1989-10-10: THEFT PREVENTION STANDARDS ANTI-THEFT LABELING (90-0-103)
- 1989-10-09: RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES (90-8-114)
- 1989-10-06: TIRE COMPANY WARRANTY ASSISTANCE PROGRAMS (90-3-3)
- 1989-09-27: SERVICE GUILD: USE OF FUEL WITH 15% MTBE IN ALL GM VEH. (89-0-7)
- 1989-09-11: IMPROPER TEMPERATURE CONTROL IN DRIVER SELECTED MODES (88-1-161)
- 1989-09-07: INTERMITTENT MESSAGE ON DIC OR ERRATIC A/C OPERATION (89-8-27)
- 1989-09-07: INTERMITTENT MESSAGE ON DIC OR ERRATIC A/C OPERATION (89-8-219)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-6B-1)
- 1989-08-18: SERVICE GUILD: RECONSTITUTED ANTI-FREEZE INFORMATION (90-0-101)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-15)
- 1989-08-10: CFC REDUCTION AND REFRIGERANT RECOVERY (RECYCLING PROGRAM) (89-1-126)
- 1989-07-26: A/T TRANSAXLE FLUID COLOR LEVEL CHECK INFORMATION (89-7-6)
- 1989-07-26: A/T TRANSAXLE FLUID COLOR LEVEL CHECK INFORMATION (89-7-119)
- 1989-07-13: INTERMITTENT DASH BRAKE TELLTALE LIGHT OPERATION (89-5-12)
- 1989-07-13: INTERMITTENT DASH BRAKE TELLTALE LIGHT OPERATION (89-8-195)
- 1989-06-15: INCORRECT CRUISE CONTROL RESUME OPERATION (89-8-19)
- 1989-06-15: INCORRECT CRUISE CONTROL RESUME OPERATION (89-8-178)
- 1989-06-14: SERVICE MANUAL DIAGNOSTIC PROCEDURE (88-8-26A)
- 1989-06-14: SERVICE MANUAL DIAGNOSTIC PROCEDURE (88-8-199)
- 1989-06-12: ASHTRAY COVER DISTORTING INSTALL NEW COVER (88-2-272)
- 1989-06-12: VIB. DIAG. USING A REED TACH. AND ROTATIONAL ORDER CHARTS (89-0-114)
- 1989-06-06: LOW OIL LEVEL MESSAGE OPERATION/DIAGNOSIS & NEW PART (90-8-160)
- 1989-06-01: SPECIFICATIONS FOR HEAD BOLT TORQUE (88-6-123)
- 1989-06-01: LOW OIL LEVEL MESSAGE OPERATION/DIAG. & NEW PARTS (89-8-174)
- 1989-05-30: SERVICE MANUAL UPDATE (SECTION 8) ELECTRICAL (88-8-27)
- 1989-05-30: SERVICE MANUAL UPDATE (SECTION 8) ELECTRICAL (88-8-212)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (88-POL-4A)
- 1989-05-29: SPECIAL POLICY: TEMPORARY REDUCTION/POWER STRG.-COLD (9S02)
- 1989-05-25: SPECIAL POLICY: TEMPORARY REDUCTION OF POWER STRG.-COLD (88-POL-4)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-7-5)
- 1989-05-24: NEW PROCEDURE FOR REPLACEMENT OF FINAL DRIVE PINION (89-7-109)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-7440-8)
- 1989-05-23: CRT / CRTC CONNECTOR KIT COAXIAL CABLE KIT P/N (89-8-11)
- 1989-05-23: TRANSAXLE FINAL DRIVE RATIO -440-T4/4T60 (89-7440-108)
- 1989-05-23: INTERMITTENT LOSS OF DRIVE CHECK 1-2 BAND STOP (89-7440-110)
- 1989-05-23: CRT / CRTC CONNECTOR KIT COAXIAL CABLE KIT P/N (89-8-159)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-10-22)
- 1989-05-18: CHIPPED PAINT DIAGNOSIS AND REPAIR (89-2-161)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (90-6-5)
- 1989-05-12: OIL FILTER LEAKAGE PROPER INSTALLATION PROCEDURE (89-6-115)
- 1989-04-19: POWER RACK & PINION GEAR SERVICE INFORMATION (89-3-17)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-8-14)
- 1989-04-19: SERVICE GUILD: CORRECT CABLE INSULATION FOR CABLE (WIRING) (89-8-162)
- 1989-04-14: GOODWRENCH VEHICLE SECURITY SYSTEM LABOR OPERATIONS (89-9-7)
- 1989-04-07: ACID RAIN PAINT LABOR OPERATIONS (89-LTG-1)
- 1989-04-03: SERVICE GUILD: POWER STEERING FLUID (PROPER FLUID USAGE) (89-3-15)
- 1989-04-03: SERVICE GUILD: POWER STEERING FLUID (PROPER FLUID USAGE) (89-3-116)
- 1989-03-03: SERVICE GUILD: USE OF CRANKSHAFT SENSOR ADJ. TOOL (89-6E-8)
- 1989-03-03: SERVICE GUILD: USE OF CRANKSHAFT SENSOR ADJ. TOOL (89-630-100)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-7440-6)
- 1989-03-02: INSTRUMENT PANEL & CCDIC- DISPLAYS FLICKER OR TURN OFF (89-8-15)
- 1989-03-02: NO 3RD GEAR (NEW THRUST BEARING) (89-7440-106)
- 1989-03-02: INSTRUMENT PANEL & CCDIC- DISPLAYS FLICKER OR TURN OFF (89-8-142)
- 1989-02-23: MANUAL UPDATE-SECTION 6E3-C7-4 (EGR FLOW CHECK) (88-6E-26)
- 1989-02-23: MANUAL UPDATE-SECTION 6E3-C7-4 (EGR FLOW CHECK) (88-638-118)
- 1989-02-21: PAINT FLAKES IN TRANS. FLUID CORRODED FILL TUBES (88-7-6A)
- 1989-02-21: PAINT FLAKES IN TRANS. FLUID CORRODED FILL TUBES (88-7440-113)
- 1989-02-20: SPOOL VALVE SPLIT RINGS RACK AND PINION POWER STEERING (88-3-25)
- 1989-02-20: DRIVEABILITY SYMTOMS MAYBE OPERATING IAC (88-638-117)
- 1989-02-09: REATTA EMERGENCY PARTS ORDERING PROGRAM (89-0-3)
- 1989-02-09: A/C REFRIGERANT LOSS DUE TO LOOSE/ MISSING ACCESS FIT. CAP (89-1-112)
- 1989-02-03: THM 400/475 PRODUCT UPDATE BOOK (89-7400-104)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-9-6)
- 1989-01-31: POOR AM OR FM RADIO RECEPTION ANT. COAX. FEMALE TERM. REPAIR (89-8-137)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-7-2)
- 1989-01-30: AXLE SEAL PROTECTOR TO PREVENT SEAL DAMAGE DURING INSTALL (89-7-105)
- 1989-01-24: REATTA PASSENGERS SEAT BACK MOVEMENT WHEN STOPPING (88-10-58)
- 1989-01-24: USE HIGH CHARGER SETTING TO RECHARGE BATTERIES/PROCEDURE (89-6D-2)
- 1989-01-24: DRIVEABILITY SYMPTOMS MAYBE INCORRECTLY OPERATING IAC (89-6E-10)
- 1989-01-24: REATTA PASSENGERS SEAT BACK MOVEMENT WHEN STOPPING (88-2-262)
- 1989-01-24: DRIVEABILITY SYMPTOMS MAYBE INCORRECTLY OPERATING IAC (89-638-101)
- 1989-01-24: USE HIGH CHARGER SETTING TO RECHARGE BATTERIES/PROCEDURE (89-8-131)
- 1989-01-23: WINDSHIELD WASHER STREAKING OR POOR PERFORMANCE (89-8-8)
- 1989-01-23: WINDSHIELD WASHER STREAKING OR POOR PERFORMANCE (88-2-260)
- 1989-01-23: WINDSHIELD WASHER STREAKING OR POOR PERFORMANCE (89-2-130)
- 1989-01-14: ANTI-LOCK BRAKE PEDAL SQUEAK INSTALL SHIM (89-5-7)
- 1989-01-14: ANTI-LOCK BRAKE PEDAL SQUEAK INSTALL SHIM (89-5-106)
- 1989-01-10: CAST ALUMINUM WHEEL POROSITY (REPAIR PROC. & SEALER) (89-3-105)
- 1989-01-05: MANUAL UPDATE-SEC 6F. EXHAUST INTERMEDIATE PIPE REPLACEMENT (88-6F-4)
- 1989-01-05: MANUAL UPDATE-SEC 6F. EXHAUST INTERMEDIATE PIPE REPLACEMENT (88-6-124)
- 1989-01-05: HARSH SHIFT CONDITIONS AND CAR SERVICE INFORMATION (89-7440-105)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (89-6C-8)
- 1988-12-26: SERVICE GUILD: FUEL PUMP STRAINER IN-TANK FILTER/SOCK (88-6-125)
- 1988-12-21: BRAKE PULSATION AND ON CAR BRAKE ROTOR TURNING (89-5-6)
- 1988-12-21: BRAKE PULSATION AND ON CAR BRAKE ROTOR TURNING (89-5-105)
- 1988-12-12: SERVICE GUILD: NEW MEM-CAL FOR INCORRECT MPG DISPLAY ON CRT (88-6E-23)
- 1988-12-12: SERVICE GUILD: NEW MEM-CAL FOR INCORRECT MPG DISPLAY ON CRT (88-8-206)
- 1988-12-05: WINDSHIELD REMOVAL & INSTALL. SERVICE MANUAL REVISION (89-2-103)
- 1988-11-15: DOOR JAMB SWITCH CORROSION NEW SWITCH SERVICE PROCEDURE (89-8-4)
- 1988-11-15: SERVICE MANUAL DIAGNOSTIC PROCEDURE (88-6E-20)
- 1988-11-15: DOOR JAMB SWITCH CORROSION NEW SWITCH SERVICE PROCEDURE (89-8-101)
- 1988-11-07: SERVICE MANUAL SUPPLEMENT TAIL LAMP REMOVAL/INSTALLATION (88-10-54)
- 1988-11-07: SERVICE MANUAL SUPPLEMENT TAIL LAMP REMOVAL/INSTALLATION (88-2-263)
- 1988-11-02: SERVICE MANUAL UPDATE DIAGNOSTIC CODES (88-6E-29)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-6C-2)
- 1988-11-02: SERVICE MANUAL UPDATE DIAGNOSTIC CODES (88-638-115)
- 1988-11-02: FUEL FEED AND/OR RETURN PIPE REPAIR PROCEDURES (89-6-101)
- 1988-11-01: A/C ODOR CLEANING PROCEDURE (89-1-3)
- 1988-10-31: FREEZING DOOR LOCK CYLINDERS REPAIR PROCEDURE OUTLINED (88-2-234)
- 1988-10-25: 89 TEVES ABS HYDRAULIC UNIT SERVICE PROCEDURE (88-5-18)
- 1988-10-25: POOR DRIVEABILITY PCV AND/OR GROMMET LOOSE (88-6E-21)
- 1988-10-25: 89 TEVES ABS HYDRAULIC UNIT SERVICE PROCEDURE (88-5-136)
- 1988-10-25: POOR DRIVEABILITY PCV AND/OR GROMMET LOOSE (88-638-114)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-1-5)
- 1988-10-19: V5 AIR CONDITIONING AND REFRIGERANT SYSTEM DIAGNOSTICS (89-1-110)
- 1988-10-10: SERVICE MANUAL UPDATE DRIVE AXLE REMOVAL PROCEDURE (89-3-5)
- 1988-10-10: SERVICE MANUAL UPDATE DRIVE AXLE REMOVAL PROCEDURE (89-4-101)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-5-2)
- 1988-10-07: MANUAL REVISION-WINDSHIELD REMOVAL & INSTALLATION (89-10-15A)
- 1988-10-07: MANUAL REVISION-WINDSHIELD REMOVAL & INSTALLATION (89-2-179)
- 1988-10-07: BRAKE LEAD DIAGNOSIS INFORMATION (89-5-101)
- 1988-10-05: FRONT AND REAR RUB STRIPS GAP TO FACIA REPAIR (88-10-48)
- 1988-10-05: FRONT AND REAR RUB STRIPS GAP TO FACIA REPAIR (88-2-247)
- 1988-10-01: INSUFFICIENT COOLING AT IDLE PARTS AND PROCEDURES (88-1-9A)
- 1988-10-01: INSUFFICIENT COOLING AT IDLE PARTS AND PROCEDURES (88-1-104)
- 1988-09-26: SERVICE MANUAL UPDATE RIVIERA LANDAU CAP ASSEMBLY (88-10-47)
- 1988-09-26: FRONT DOOR WINDOW CLICKING OR CREAKING (88-10-52)
- 1988-09-26: FRONT DOOR WINDOW CLICKING OR CREAKING (88-2-243)
- 1988-09-26: SERVICE MANUAL UPDATE RIVIERA LANDAU CAP ASSEMBLY (88-2-244)
- 1988-08-30: SERVICE MANUAL UPDATE RELOCATION OF TURN/HAZARD (88-8-20)
- 1988-08-30: SERVICE MANUAL UPDATE RELOCATION OF TURN/HAZARD (88-8-188)
- 1988-08-17: HARSH 3-2 DETENT DOWNSHIFT AT HIGH ALTITUDES- W/440-T4 (88-7440-10)
- 1988-08-17: HARSH 3-2 DETENT DOWNSHIFT AT HIGH ALTITUDES- W/440-T4 (88-7440-111)
- 1988-08-15: HIGH EFFORT TO OPEN REAR COMPARTMENT LID (88-10-34)
- 1988-08-15: PROCEDURE FOR RELEASING PRODUCT SERVICE BULLETINS (88-0-111)
- 1988-08-15: HIGH EFFORT TO OPEN REAR COMPARTMENT LID (88-2-221)
- 1988-08-10: TRI-COAT PAINT REPAIR PROCEDURES (89-10-2)
- 1988-08-10: TRI-COAT PAINT REPAIR PROCEDURES (89-2-101)
- 1988-08-08: ELECTROSTATIC DISCHARGE DAMAGE TO ECM (INFO. TO PREVENT) (88-8-168)
- 1988-08-01: REV. STEERING PUMP NOISE OR INCREASED STEERING EFFORT (88-3-8B)
- 1988-08-01: REV. STEERING PUMP NOISE OR INCREASED STEERING EFFORT (88-3-117)
- 1988-07-28: DOOR CHUCKING NOISE (REPLACE LOCK ASSEMBLY P/N) (88-10-40)
- 1988-07-28: ANTI-LOCK BRAKE SERVICE MANUAL DIAGNOSTIC CHARTS (88-5-14)
- 1988-07-28: DOOR CHUCKING NOISE (REPLACE LOCK ASSEMBLY P/N) (88-2-253)
- 1988-07-28: ANTI-LOCK BRAKE SERVICE MANUAL DIAGNOSTIC CHARTS (88-5-124)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-5)
- 1988-07-18: INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP (88-8-25)
- 1988-07-18: SERVICE REPLACEMENT TRANSMISSION ASSEMBLY UPDATE (88-7-108)
- 1988-07-18: INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP (88-8-170)
- 1988-07-04: BOSE RADIO RATTLE RETURN RADIO TO REPAIR CENTER (88-2-192)
- 1988-07-04: DRIVE LINE VIBRATION AT 70-95 KM/H WITH LIGHT LOAD (88-4-105)
- 1988-06-24: NEW FINAL DRIVE ASSEMBLY FINAL DRIVE SUN GEAR SHAFT (88-7440-9)
- 1988-06-24: NEW FINAL DRIVE ASSEMBLY FINAL DRIVE SUN GEAR SHAFT (88-7440-110)
- 1988-06-23: SERVICE GUILD: BROKEN VALVE SPRING CAPS REP. ALL WITH P/N (88-6-20)
- 1988-06-23: SERVICE GUILD: BROKEN VALVE SPRING CAPS REP. ALL WITH P/N (88-638-112)
- 1988-06-14: SERVICE GUILD: SUSPENSION AND STEERING INFO. & DESCRIPTION (88-3-133)
- 1988-06-09: SERVICE MANUAL UPDATE REVISED POWER STEERING HOSE (88-3-20)
- 1988-06-09: SERVICE MANUAL UPDATE REVISED POWER STEERING HOSE (88-3-131)
- 1988-06-06: CONSOLE ARMREST COVER HIGH LATCHING EFFORT/ADJUST HINGE (88-10-28)
- 1988-06-06: CONSOLE ARMREST COVER HIGH LATCHING EFFORT/ADJUST HINGE (88-2-217)
- 1988-06-06: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (88-638-110)
- 1988-06-01: SPOOL VALVE SPLIT RINGS IN POWER STRG RACK & PINION GEARS (88-3-18)
- 1988-05-31: INTERMITTENT ECM CONNECTION MAY BE WEAK TERMINAL GRIP (88-6E-15)
- 1988-05-31: INTERMITTENT ECM CONNECTION MAY BE WEAK TERMINAL GRIP (88-6-116)
- 1988-05-27: DRIVE LINE VIBRATION AT 45-60 MPH WITH LIGHT LOAD (88-4-1)
- 1988-05-27: DRIVE LINE VIBRATION AT 45-60 MPH WITH LIGHT LOAD (88-4-104)
- 1988-05-26: NO OIL PRESSURE READING AT COLD START (REPLACE P/N) (88-6-19)
- 1988-05-26: NO OIL PRESSURE READING AT COLD START (REPLACE P/N) (88-8-156)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-10-27)
- 1988-05-19: SERVICE GUILD: INSTALLATION OF AFTER MARKET STYLED WHEELS (88-3-16)
- 1988-05-19: CLEANING OF UPPER INSTRUMENT PANEL SURFACES (88-2-183)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-3-19)
- 1988-05-17: VALVE BODY CLAMPING PLATE ELIMINATED W/ 440T4 TRANS. (88-7440-8)
- 1988-05-17: IDENTIFYING RACK AND PINION STEERING SYSTEM NOISES (88-3-128)
- 1988-05-17: VALVE BODY CLAMPING PLATE ELIMINATED W/ 440T4 TRANS. (88-7440-109)
- 1988-05-05: SERVICE MANUAL UPDATE REAR BRAKE CALIPER OVERHAUL (88-5-12)
- 1988-05-05: SERVICE MANUAL UPDATE REAR BRAKE CALIPER OVERHAUL (88-5-128)
- 1988-04-27: BELT CHIRP OR SQUEAL DIAGNOSIS PROCEDURE (88-630-101)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-7-3)
- 1988-04-25: SPORADIC ENGAGEMENT OF THE TORQUE CONVERTER CLUTCH (88-7-105)
- 1988-04-22: POWER ANTENNA WILL NOT RETRACT WITH RADIO OFF (88-9-6)
- 1988-04-22: POWER ANTENNA WILL NOT RETRACT WITH RADIO OFF (88-8-149)
- 1988-04-14: DIM GEAR INDICATOR LIGHT OR REPEAT FAILURE (INCORRECT P/N) (88-8-16)
- 1988-04-14: DIM GEAR INDICATOR LIGHT OR REPEAT FAILURE (INCORRECT P/N) (88-8-144)
- 1988-03-29: REAR BRAKE NOISE OR VIBRATION (MAYBE ROTOR DISTORTION) (88-5-9)
- 1988-03-29: REAR BRAKE NOISE OR VIBRATION (MAYBE ROTOR DISTORTION) (88-5-113)
- 1988-03-21: GAS-TECH. INFO FROM THE CANADIAN GEN. STANDARDS BOARD (88-6-109)
- 1988-03-17: NEW PRODUCT INFORMATION PRODUCTION CHANGES 440-T4 (88-7440-7)
- 1988-03-17: NEW PRODUCT INFORMATION PRODUCTION CHANGES 440-T4 (88-7440-107)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-7440-6)
- 1988-03-15: TCC ENGAGES IN 2ND CHECK TCC SCREEN SEAL P/N (88-7440-108)
- 1988-03-01: NEW BOTTOM PAN AND COATING CELLULOSE GASKET (88-7440-5)
- 1988-03-01: NEW BOTTOM PAN AND COATING CELLULOSE GASKET (88-7440-106)
- 1988-03-01: BCM VEHICLE OPTION PARAMETERS DESCRIPTION AND SYMPTOMS (88-8-138)
- 1988-02-29: ENG. MISS,HESITATION & ROUGH PIERCED SEC. IGN. COMPONENTS (88-6-106)
- 1988-02-12: SERVICE ENGINE SOON LIGHT WITH A CODE 44 OR 48 STORED (88-6E-8)
- 1988-02-12: NEW THERMOSTAT GASKET MAY REPAIR HEATER COMPLAINTS (89-6-3)
- 1988-02-12: SERVICE ENGINE SOON LIGHT WITH A CODE 44 OR 48 STORED (88-638-107)
- 1988-02-12: NEW THERMOSTAT GASKET MAY REPAIR HEATER COMPLAINTS (88-638-109)
- 1988-02-11: BRAKE/ANTI-LOCK WARNING LAMPS NO POWER ASSIST OR PUMP OPER. (88-5-6)
- 1988-02-11: BRAKE/ANTI-LOCK WARNING LAMPS NO POWER ASSIST OR PUMP OPER. (88-5-108)
- 1988-02-04: ODOR FROM A/C AT START-UP PROCEDURE TO REPAIR DESCRIBED (90-1-1)
- 1988-01-26: SCAN TOOL WORKSHEET AID TO DIAGNOSIS (88-6-105)
- 1988-01-22: POSSIBLE FALSE CRT DIAGNOSTIC CODE C339 (88-8-9)
- 1988-01-22: POSSIBLE FALSE CRT DIAGNOSTIC CODE C339 (88-8-127)
- 1988-01-19: CELLULAR MOBILE TELEPHONES (OPERATION DESCRIBED) (88-9-4)
- 1988-01-11: WINDSHIELD REMOVAL AND INSTALLATION (INSTRUCTIONS) (88-10-4)
- 1988-01-11: PART WARRANTY CLAIM SUBMISSION REVISED FOR NON DIV. VEHICLES (88-POL-2)
- 1988-01-11: WINDSHIELD REMOVAL AND INSTALLATION (INSTRUCTIONS) (88-2-128)
- 1988-01-11: REMOVAL OF CHEMICAL SPOTTING AND MINOR PAINT IMPERFECTIONS (88-10-11)
- 1988-01-07: 'FAST START' CRANK SENSOR ADJUSTMENT (88-6-6)
- 1988-01-07: ERASE REMINDER PRIOR TO DELIVERY (PROCEDURE DESCRIBED) (88-8-8)
- 1988-01-07: 'FAST START' CRANK SENSOR ADJUSTMENT (88-638-106)
- 1988-01-07: ERASE REMINDER PRIOR TO DELIVERY (PROCEDURE DESCRIBED) (88-8-124)
- 1988-01-07: CLIMATE CONTROL TEMP. BUTTON INOPERATIVE (88-1-111)
- 1988-01-04: ASSEMBLY PLANT PAINT SUPPLIER INFORMATION (88-10-6)
- 1988-01-04: ASSEMBLY PLANT PAINT SUPPLIER INFORMATION (88-2-124)
- 1988-01-04: FALSE HIGH OIL PRESSURE GAUGE READING (88-638-105)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-7440-3)
- 1987-12-11: NEW DESIGN INPUT CLUTCH AND THIRD CLUTCH SEAL INSTALLERS (88-7440-102)
- 1987-12-10: FRONT SUSPENSION UPPER STRUT MOUNT NUT CHANGE / CORRECTION (88-3-7)
- 1987-12-10: REVISED LABOR OPERATIONS FOR DRIVEABILITY DIAGNOSIS (88-6E-4)
- 1987-12-10: FRONT SUSPENSION UPPER STRUT MOUNT NUT CHANGE / CORRECTION (88-3-107)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-7440-1)
- 1987-12-08: NEW DESIGN SECOND CLUTCH PISTON INNER SEAL (88-7440-101)
- 1987-12-07: BALANCE SHAFT BEARING FAILURE ALL MODELS W/3800 (80-95-08)
- 1987-12-07: OBSCENE MESSAGE IN ECC PROCEDURE TO REMOVE (80-95-09)
- 1987-12-07: WIND NOISE AT FRT. DOOR WINDOW MAY BE MISSING CAULK SEALER (88-10-5)
- 1987-12-07: WIND NOISE AT FRT. DOOR WINDOW MAY BE MISSING CAULK SEALER (88-2-119)
- 1987-12-03: HARSH ENGAGEMENT CONDITIONS SYMPTOMS/DIAGNOSIS/REPAIRS (88-7440-2)
- 1987-12-03: AC DELCO RADIO REPAIR NEW CAR LIMITED WARRANTY (88-9-1)
- 1987-12-03: HARSH ENGAGEMENT CONDITIONS SYMPTOMS/DIAGNOSIS/REPAIRS (88-7440-100)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-8-6)
- 1987-12-01: DAMAGE TO WIRING TERMINALS ON ENGINE SENSORS-METRI-PACK 150 (88-8-117)
- 1987-11-30: FALSE HIGH OIL PRESSURE GAUGE READINGS (88-6-3)
- 1987-11-30: FALSE HIGH OIL PRESSURE GAUGE READINGS (88-630-100)
- 1987-11-23: ENGINE CLUNK DURING ACCELERATION OR SHIFT (88-6-4A)
- 1987-11-23: ENGINE CLUNK DURING ACCELERATION OR SHIFT (88-638-103)
- 1987-11-16: DELCO BATTERY STORAGE TESTING DIAGNOSIS AND CHARGING (87-8-5)
- 1987-11-16: AIR CONDITION COMPRESSOR REPLACEMENT PROCEDURE (88-1-3)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-5)
- 1987-11-16: A/C COMPRESSOR REPLACEMENT SYSTEM FILLER DESCRIBED (88-1-107)
- 1987-11-16: AIR CONDITION COMPRESSOR REPLACEMENT PROCEDURE (88-1-112)
- 1987-11-16: TIRE WARRANTIES IRREGULAR/PREMATURE WEAR (88-3-104)
- 1987-11-16: DELCO BATTERY STORAGE TESTING DIAGNOSIS AND CHARGING (89-8-109)
- 1987-11-11: DIGITAL AND QUARTZ INSTRUMENT CLUSTER AND GCC MONITOR (88-8-3)
- 1987-11-10: WINDSHIELD WIPER OPERATION NOISE/ARM MAY STRIKE MOLDING (88-8-5)
- 1987-11-10: WINDSHIELD WIPER OPERATION NOISE/ARM MAY STRIKE MOLDING (88-2-116)
- 1987-11-09: SERVICE MANUAL REVISION CHART A-3 AND C4 SECTION 6E (87-638-111)
- 1987-10-19: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (88-8-106)
- 1987-10-12: BUICK NEW VEHICLE ANNOUNCEMENT MANUAL AND LABEL ORDERING (88-0-1A)
- 1987-09-24: ECM AND BCM MODULE EXCHANGE PROGRAM (87-6E-2)
- 1987-09-24: ECM AND BCM MODULE EXCHANGE PROGRAM (87-8-100)
- 1987-09-24: INSTRUMENT CLUSTER EXCHANGE REPAIR PROGRAM (89-8-112)
- 1987-09-22: ACRYLIC COATING TOUCH UP PAINT NEW PRODUCT ORDER INFORMATION (88-10-2)
- 1987-09-15: DELCO REMY DIRECT IGN. REPLACEMENT PARTS (87-6D-13)
- 1987-09-15: DELCO REMY DIRECT IGN. REPLACEMENT PARTS (88-6-101)
- 1987-09-07: FRENCH LABEL INSTALLATION INSTRUCTIONS (PASS. CARS) (88-0-100)
- 1987-09-01: INSTRUMENT CLUSTER EXCHANGE REPAIR PROGRAM (88-8-107)
- 1987-08-20: STEERING LEAD OR PULL DIAGNOSIS AND POSSIBLE REPAIR (87-3-132)
- 1987-07-31: WARRANTY CLAIMS PROCESSING INFORMATION (88-POL-1)
- 1987-07-22: CHECKING PROPER FLUID LEVEL PROCEDURE (88-7-1)
- 1987-07-22: CHECKING PROPER FLUID LEVEL PROCEDURE (88-7-100)
- 1987-06-03: TIRE COMPANY ASSISTANCE PROGRAM (87-3-11)
- 1987-04-07: METHOD OF VERIFYING ' GOOD ELECTRICAL SYSTEM GROUND ' (87-8-139)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (89-3-7)
- 1987-03-16: CAST ALUMINUM WHEEL POROSITY REPAIR AND SEALER REVISED (87-3-115)
- 1986-12-15: INSTRUMENT CLUSTER EXCHANGE PROGRAM INFORMATION (87-8-113)
- 1986-10-20: USE OF UNLEADED GASOLINE IN VEHICLES USING LEADED GAS (87-6-100)
- 1986-09-23: USE OF UNLEADED GASOLINE VEHICLES USING LEADED GAS (87-0-104)
- 1986-09-22: DELCO FREEDOM BATTERY STORAGE AND TESTING (87-8-3)
- 1986-09-22: DELCO FREEDOM BATTERY STORAGE AND TESTING (87-8-108)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (86-8-15)
- 1986-08-28: SERVICE GUILD: ELECTROSTATIC DISCHARGE DAMAGE (87-8-102)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (86-1-1)
- 1985-10-23: DA6 A/C COMPRESSOR REPAIR REPAIR ASSEMBLY P/N (86-1-100)
- 1985-10-07: CRACKED PAINT USING RM HIGH SOLIDS RAPID FILTER (86-2-103)