For 1990-2009 cars

# D.I.C. LENS SCRATCHED LENS CAN BE REPLACED

#### VEHICLES AFFECTED: 1986-87 TORONADO MODELS

In the event a 1986 or 1987 Toronado digital instrument cluster lens is scratched, the lens can be replaced without sending the cluster to the repair stations.

The lens, part no. 1642867, can be ordered from GM Parts.

The procedure for replacing the lens is as follows:

REMOVAL

1. Remove cluster as instructed in the 1986 Toronado Chassis Service Manual. 2. Remove the two (2) lower lens attaching screws. 3. Slide the lens downward to disengage the tabs from the cluster.

INSTALLATION

1. Reverse the removal procedure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.