For 1990-2009 cars

Application | N·m | Lb Ft | Lb In.
--- | --- | --- | ---
Battery Cable to Battery Post | 15 | 11 | --
Battery Cable Nut at the Solenoid | 8 | -- | 71
Battery Cable to Generator Output Stud | 20 | 15 | --
Battery Cable to Generator Output Stud (L47) | 15 | 11 | --
Battery Cable to Starter | 10 | -- | 88
Battery Hold Down Retainer Bolt | 18 | 13 | --
Engine Ground Cable | 30 | 22 | --
Flywheel Inspection Cover Bolts | 15 | 11 | --
Generator Front Studs | 38 | 28 | --
Generator Mounting Bolt ( L67) | 50 | 37 | --
Generator Mounting Bolt (L47) | 47 | 36 | --
Generator Output Wire ( L47 L67) | 20 | 15 | --
Negative Battery Cable Bolt at the Battery | 15 | 11 | --
Positive Battery Cable Bolt at the Battery | 15 | 11 | --
Positive Booster Cable Bolt at Multifuse Relay Center | 20 | 15 | --
Solenoid Battery Terminal Nut | 16 | 12 | --
Solenoid Screw | 6.5 | -- | 60
Solenoid S Terminal Nut | 3 | -- | 26
Spark Plug | 15 | 11 | --
Starter Motor Mounting Bolt | 30 | 22 | --