For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: Perform only if both seat belts do not retract.
1 | Was the entire Seat Belts System Check performed? | -- | Go to Step 2 | Go to Seat Belt System Check
2 | Backprobe the LH seat belt retractor solenoid with a test lamp from cavity A (ORN) to ground. Does the test lamp light? | -- | Go to Step 3 | Go to Step 5
3 | Check that G201 is clean and tight. Refer to Intermittents and Poor Connections Diagnosis in Wiring Systems. Is G201 OK? | -- | Go to Step 4 | Go to Step 9
4 | Repair the open in CKT 151 (BLK) between G201 and S212. Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Seat Belt System Check | --
5 | Check the RH rear fuse block PWR DR LK Fuse by visual inspection. Is the PWR DR LK Fuse OK? | -- | Go to Step 6 | Go to Step 7
6 | Repair the open in CKT 1540 (ORN) between the RH rear fuse block and S309. Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Seat Belt System Check | --
7 | Repair the short to ground in CKT 1540 (ORN). Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Step 8 | --
8 | Replace the RH rear fuse block PWR DR LK Fuse. Is the fuse replacement complete? | -- | Go to Seat Belt System Check | --
9 | Repair the ground G201. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Seat Belt System Check | --