For 1990-2009 cars

1. Remove the key from the ignition switch.
2. Connect the inflatable restraint IP module yellow 2-way connector located above the passenger sound insulator.
3. Install the Connector Position Assurance (CPA) (2) to the inflatable restraint IP module yellow 2-way connector(1) located above the passenger sound insulator.
4. Install the passenger sound insulator.
5. Attach the inflatable restraint IP module yellow 2-way connector to the HVAC programmer bracket.
6. Connect the inflatable restraint steering wheel yellow 2-way connector (2) located near the base of the steering column.
7. Install the Connector Position Assurance (CPA) (4) to the inflatable restraint steering wheel yellow 2-way connector (2) located near the base of the steering column.
8. Install the sound left insulator.
9. Install the AIR BAG Fuse to the IP Fuse Block.
10. Staying well away from both air bags, turn the ignition switch to the RUN position.

10.1. | The AIR BAG warning lamp will flash seven times.

10.2. | The AIR BAG warning lamp will then turn OFF.

11. Perform the SIR Diagnostic System Check if the AIR BAG warning lamp does not operate as described. Refer to SIR Diagnostic System Check .