For 1990-2009 cars

### Installation Procedure

#### Tools Required

J 36660-A

1. Turn the crankshaft so that the number one piston is at top dead center.
2. Turn the camshaft so that the timing mark (2) is straight down (with the sprocket temporarily installed).
3. Assemble the timing chain on the sprockets. Ensure that the timing marks are in the closest together position.
4. Install the timing chain (1) and the crankshaft sprocket (3).
5. Install the camshaft sprocket.

Notice: This bolt is designed to permanently stretch when tightened, and therefore MUST be replaced anytime it is removed. The correct part number fastener must be used to replace this type of fastener. Do not use a bolt that is stronger in this application. If the correct bolt is not used, the parts will not be tightened correctly. The system or the components may be damaged.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

6. Install the camshaft sprocket bolt.

Tighten
Tighten the camshaft sprocket bolt to 100 N·m (74 lb ft). Use the J 36660-A in order to tighten the bolt an additional 90 degrees.

7. Install the timing chain damper.
8. Install the timing chain damper bolt.

Tighten
Tighten the timing chain damper bolt to 22 N·m (16 lb ft).

9. Install the engine front engine cover. Refer to Engine Front Cover Replacement

### Removal Procedure

1. Remove the engine front cover. Refer to Engine Front Cover Replacement .
2. Align the timing marks (2) on the sprockets. Position the sprockets as close together as possible.
3. Remove the timing chain damper.
4. Remove the camshaft sprocket bolt.
5. Remove the camshaft sprocket (2).
6. Remove the timing chain (1).
7. Inspect the following components:

• | Timing chain

• | Sprockets

• | All components for wear and/or damage