For 1990-2009 cars

### Removal Procedure

### Tools Required

J 34730 Fuel Pressure Gauge

1. Relieve the fuel system fuel pressure. Refer to the Fuel Pressure Relief .
2. Remove the rear compartment floor trim (1). Refer to Rear Compartment Trim Panel Replacement in Body and Accessories.
3. Remove the bolts from the fuel sender access panel (2).
4. Remove the fuel tank pressure sensor (1) electrical sensor connector.
5. Remove the fuel tank pressure sensor from the sender.

### Installation Procedure

1. Install the new fuel tank vapor pressure sensor into the modular fuel sender.
2. Install the fuel tank pressure sensor (1) electrical sensor connector.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the fuel sender access panel bolts.

Tighten
Tighten the bolts to 2 N·m (18 lb in).

4. Install the rear compartment floor trim (1). Refer to Rear Compartment Trim Panel Replacement in Body and Accessories.
5. Install the fuel tank filler pipe cap.
6. Install the negative battery cable. Refer to Battery Cable in Engine Electrical.
7. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Body and Accessories.