For 1990-2009 cars

# REAR COMPARTMENT LID HINGE BINDING HINGE ARM TO HINGE BOX

1983 " E " C A R A BINDING CONDITION ON REAR COMPARTMENT LID HINGES MAY BE ENCOUNTERED ON LATE BUILD (1983) "E" CARS EQUIPPED WITH TORQUE RODS. THE BIND CAN OFTEN BE FOUND BETWEEN THE HINGE ARM AND THE HINGE BOX ON RIGHT ON/OR LEFT SIDES AS INDICATED IN FIGURE 1... THIS CONDITION MAY BE CONFUSED WITH LOW OUTPUT FROM TORQUE RODS. CORRECTION OF THIS CONDITION CAN BE ACCOMPLISHED BY PRYING THE HINGE ARM AWAY FROM THE HINGE BOX AS ILLUSTRATED IN FIGURE 1... APPLY A HEAVY LUBE TO SURFACES.(REFERENCE MF 83-026)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.