For 1990-2009 cars

### Removal Procedure

1. Remove the caliper. Refer to Brake Caliper Replacement .
2. Remove the brake pads from the caliper anchor bracket.
3. Remove the caliper anchor bracket bolts.
4. Remove the anchor bracket.

### Installation Procedure

Important: Apply a few drops of GM Loctite™ (or equivalent) to the threads of the caliper anchor bracket bolts before installing or replace the bolts with new pre-coated bolts.

1. Install the caliper anchor bracket to the steering knuckle.
2. Install the caliper anchor bracket bolt.

Tighten
Tighten the caliper anchor bracket bolts to 185 N·m (137 lb ft).

3. Install the caliper. Refer to Brake Caliper Replacement .