For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the push-in retainers and screws (4) from the air baffle (3).
3. Release the snap tabs (2) that retain the air baffle (3).
4. Lower the air baffle (3).

### Installation Procedure

1. Install the lower air baffle (3).
2. Engage the snap tabs (2) in order to retain the air baffle (3).
3. Install the push-in retainers (4).
4. Lower the vehicle.