For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Exterior Lights System Check? | -- | Go to Step 2 | Go to Exterior Lights System Check
2 |

1. Disconnect the hazard flasher connector.
2. Measure the voltage to ground at the hazard flasher connector terminal B (ORN).

Is the voltage within the specified range?

10-15 V

Go to Step 3

Go to Step 5

3 |

1. Set the turn/hazard switch to HAZARD.
2. Connect a fused jumper between the hazard flasher connector terminal B (ORN) and terminal A (BRN).

Do all of the turn lamps light?

--

Go to Step 4

Go to Step 6

4 | Replace the hazard flasher. Is the repair complete? | -- | Go to Exterior Lights System Check | --
5 | Repair the open or the short to ground in CKT 140 (ORN). Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --
6 | Test CKT 27 (BRN) for an open or a short to ground. Refer to Testing for Continuity or Testing for Short to Ground in Wiring Systems. Is CKT 27 OK? | -- | Go to Step 7 | Go to Step 8
7 | Replace the turn/hazard switch assembly. Is the repair complete? | -- | Go to Exterior Lights System Check | --
8 | Repair the suspect wiring. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Exterior Lights System Check | --