For 1990-2009 cars

### Removal Procedure

1. Rotate the assist handle downward.
2. Remove the 2 fasteners from the assist handle.
3. Partially pull the assist handle downward.
4. Disconnect the electrical connectors.
5. Remove the handle assembly.

### Installation Procedure

1. Connect the electrical connectors.
2. Ensure the wires are pushed into the roof cavity.
3. Position the assist handle in the headliner.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the 2 fasteners in order to secure the assist handle.

Tighten
Tighten the two fasteners to 2 N·m (18 lb in).